$Id$
Legend:
SPEC!!  - Not specified
SPEC    - Spec not finalized
N       - nick claims
R       - arma claims
P       - phobos claims
S       - Steven claims
M       - Matt claims
J       - Jeff claims
        - Not done
        * Top priority
        . Partially done
        o Done
        d Deferrable
        D Deferred
        X Abandoned

For Tor 0.2.0.13-alpha:
  - Put a consensus in place of the empty fallback-consensus file in
    src/config and see what breaks.
  - let bridges set relaybandwidthrate as low as 5kb

Things we'd like to do in 0.2.0.x:
  - See also Flyspray tasks.
  - See also all items marked XXXX020 and DOCDOC in the code
  - https://www.torproject.org/eff/legal-faq.html#License doesn't mention
    licenses for other components of the bundles.

  - Before the feature freeze: (Nick)
    D 118 if feasible and obvious
    D Maintain a skew estimate and use ftime consistently.
    - 105+TLS, if possible.
      . TLS backend work
        - New list of ciphers for clients
        o Servers detect new ciphers, and only send ID cert when they
          get an older cipher list, and only request client cert when
          they get an older cipher list.
        - Clients only send certificates when asked for them.
        o Servers disable callback once negotiation is finished, so
          that renegotiation happens according to the old rules.
        o Clients initiate renegotiation immediately on completing
          a v2 connection.
        o Servers detect renegotiation, and if there is now a client
          cert, they adust the client ID.
          o Detect.
          o Adjust.
      o Add a separate handshake structure that handles version negotiation,
        and stores netinfo data until authentication is done.
      o Revise versions and netinfo to use separate structure; make
        act-on-netinfo logic separate so it can get called _after_
        negotiation.
      o Variable-length cells
        o Add structure
        o Add parse logic
        o Make CERT variable.
        o Make VERSIONS variable.
      o CERT cells
        o functions to parse x509 certs
        o functions to validate a single x509 cert against a TLS connection
        o functions to validate a chain of x509 certs, and extract a PK.
        o function to encode x509 certs
        o Parse CERT cells
        o Generate CERT cells
        o Keep copies of X509 certs around, not necessarily associated with
          connection.
      o LINK_AUTH cells
        o Code to generate
          o Remember certificate digests from TLS
        o Code to parse and check
      X Revised handshake: post-TLS.
        o If in 'handshaking' state (since v2+ conn is in use), accept
          VERSIONS and NETINFO and CERT and LINK_AUTH.
        o After we send NETINFO, send CERT and LINK_AUTH if needed.
        o Once we get a good LINK_AUTH, the connection is OPEN.
        - Ban most cell types on a non-OPEN connection.
        o Close connections on handshake failure.
      - New revised handshake: post-TLS:
        - start by sending VERSIONS cells
        - once we have a version, send a netinfo and become open
        - Ban most cell types on a non-OPEN connection.
      o Make code work right wrt TLS context rotation.
      - NETINFO fallout
        - Don't extend a circuit over a noncanonical connection with
          mismatched address.
        - Learn our outgoing IP address from netinfo cells?
      o Protocol revision.
        o Earliest stages of 110 (infinite-length) in v2 protocol:
          add support for RELAY_EARLY.
  o Before the feature freeze: (Roger)
    o Make tunnelled dir conns use begin_dir if enabled
    o make bridge users fall back from bridge authority to direct attempt

  - get more v3 authorities before 0.2.0.x comes out.
    - brainstorm about who those should be

  - Bugs.
     - Bug reports Roger has heard along the way that don't have enough
        details/attention to solve them yet.
        o tup said that when he set FetchUselessDescriptors, after
          24 or 48 hours he wasn't fetching any descriptors at all
          anymore. This was in 0.2.0 but worked fine in 0.1.2.
        - arma noticed that when his network went away and he tried
          a new guard node and the connect() syscall failed to it,
          the guard wasn't being marked as down. 0.2.0.x.
        - after being without network for 12 hours, arma's tor decided
          it couldn't fetch any network statuses, and never tried again
          even when the network came back and arma clicked on things.
          also 0.2.0.
        - phobos says relaybandwidth* sometimes don't do what we expect.
          http://interloper.org/tmp/2007-06-bw-usage.png
          I believe this is the result of confusion about whether to use
          relaybandwidth or bandwidthrate to control bandwidth usage for 
          servers.  Chances are, this isn't a bug per se. [phobos]
        o this notion of authorities notifying servers that they're
          unreachable is bunk -- it's leftover from the time when all
          servers ran 24/7. now it triggers every time a server goes
          away and then returns before the old descriptor has expired.
      - we need a config option to turn off proposal 109 behavior, else
        running a private tor network on your own computer is very hard.
      . man page entry for HidServDirectoryV2 and
        MinUptimeHidServDirectoryV2.
      o add a --quiet commandline option that suppresses logs. useful
        for --hashed-password and maybe others.
      d Tor logs the libevent version on startup, for debugging purposes.
        This is great. But it does this before configuring the logs, so
        it only goes to stdout and is then lost.
      d we should do another bandwidth test every 12 hours or something
        if we're showing less than 50KB and our bandwidthrate says we can
        do more than that. I think some servers are forgetting the results
        of their first test, and then never seeing use.

  - Proposals:
    o 101: Voting on the Tor Directory System (plus 103)
      D Use if-modified-since on consensus download
      - Controller support
        - GETINFO to get consensus
        - Event when new consensus arrives
    - 105: Version negotiation for the Tor protocol
    . 111: Prioritize local traffic over relayed.
      - Merge into tor-spec.txt.

  - Refactoring:
    . Make cells get buffered on circuit, not on the or_conn.
      . Switch to pool-allocation for cells?
        - Benchmark pool-allocation vs straightforward malloc.
        - Adjust memory allocation logic in pools to favor a little less
          slack memory.
    . Remove socketpair-based bridges conns, and the word "bridge".  (Use
      shared (or connected) buffers for communication, rather than sockets.)
      . Implement
        - Handle rate-limiting on directory writes to linked directory
          connections in a more sensible manner.
        - Find more ways to test this.
    D Do TLS connection rotation more often than "once a week" in the
      extra-stable case.
    D Streamline how we pick entry nodes: Make choose_random_entry() have
      less magic and less control logic.
    - Refactor networkstatus generation:
      - Include "v" line in getinfo values.

  - Bridges:
    . Bridges users (rudimentary version)
      o Ability to specify bridges manually
      o Config option 'UseBridges' that bridge users can turn on.
        o uses bridges as first hop rather than entry guards.
      o if you don't have any routerinfos for your bridges, or you don't
        like the ones you have, ask a new bridge for its server/authority.
      . Ask all directory questions to bridge via BEGIN_DIR.
        - use the bridges for dir fetches even when our dirport is open.
R     - drop 'authority' queries if they're to our own identity key; accept
        them otherwise.
      X Design/implement the "local-status" or something like it, from the
        "Descriptor purposes: how to tell them apart" section of
        http://archives.seul.org/or/dev/May-2007/msg00008.html
      o timeout and retry schedules for fetching bridge descriptors
      - give extend_info_t a router_purpose again
      o react faster to download networkstatuses after the first bridge
        descriptor arrives
      o be more robust to bridges being marked as down and leaving us
        stranded without any known "running" bridges.
    - Bridges operators (rudimentary version)
      * Ability to act as dir cache without a dir port.
      o Bridges publish to bridge authorities
      o Fix BEGIN_DIR so that you connect to bridge of which you only
        know IP (and optionally fingerprint), and then use BEGIN_DIR to learn
        more about it.
      - look at server_mode() and decide if it always applies to bridges too.
    - Bridges authorities (rudimentary version)
      o Rudimentary "do not publish networkstatus" option for bridge
        authorities.
      d Clients can ask bridge authorities for more bridges.
    - Bridges
      o Clients can ask bridge authorities for updates on known bridges.
    - Misc
      * Make BEGIN_DIR mandatory for asking questions of bridge authorities?

  - Features (other than bridges):
    - Audit how much RAM we're using for buffers and cell pools; try to
      trim down a lot.
    - Base relative control socket paths on datadir.
    - Make TrackHostExits expire TrackHostExitsExpire seconds after their
       *last* use, not their *first* use.
    - Limit to 2 dir, 2 OR, N SOCKS connections per IP.
      - Or maybe close connections from same IP when we get a lot from one.
      - Or maybe block IPs that connect too many times at once.
    D add an AuthDirBadexit torrc option if we decide we want one.

  - Testing
N   - Hack up a client that gives out weird/no certificates, so we can
      test to make sure that this doesn't cause servers to crash.

  - Deprecations:
    - can we deprecate 'getinfo network-status'?
    - can we deprecate the FastFirstHopPK config option?

  - Documentation
    - HOWTO for DNSPort.
    - Quietly document NT Service options
    - More prominently, we should have a recommended apps list.
      - recommend pidgin (gaim is renamed)
      - unrecommend IE because of ftp:// bug.
    - we should add a preamble to tor-design saying it's out of date.
    . Document transport and natdport in a good HOWTO.
    - Publicize torel.  (What else?
    . Finish path-spec.txt

P - Packaging:
P - Plan a switch to polipo.  Perhaps we'll offer two http proxies in
    the future.
P - Make documentation realize that location of system configuration file
    will depend on location of system defaults, and isn't always /etc/torrc.
P - Figure out why dll's compiled in mingw don't work right in WinXP.
  - Create packages for Nokia 800, requested by Chris Soghoian
P - Consider creating special Tor-Polipo-Vidalia test packages,
    requested by Dmitri Vitalev
  o Get Vidalia supporting protocolinfo and using auth by default.
P - create a "make win32-bundle" for vidalia-privoxy-tor-torbutton bundle
P - Flyspray 487, create a universal binary privoxy for inclusion in
    packages.

Nice-to-have items for 0.2.0.x, time permitting:
  - Low-priority bugs:
    - we try to build 4 test circuits to break them over different
      servers. but sometimes our entry node is the same for multiple
      test circuits. this defeats the point.

Planned for 0.2.1.x, December:
  - mirror tor downloads on (via) tor dir caches
R   - spec
    - deploy
  - geoip caching and publishing for bridges
R   - spec
    - deploy
    d let Vidalia use the geoip data too rather than doing its own
      anonymized queries
  - bridge address disbursal strategies
    o get the cached-descriptors* to bridges@moria
    - parse out bridge addresses from cached-descriptors*
      (or parse them out before Tonga sends them)
      (or get Tonga's Tor to write them out better in the first place)
    * answer by IP/timestamp
      - run a little web server on moria?
    d answer by answering email to bridges@torproject
      - keep track of which addresses have been answered already
    d some sort of reachability testing on bridges
  - families of bridges
  - interface for letting soat modify flags that authorities assign
R   - spec
    - deploy
S * tor usb windows image (vidalia, polipo, tor, firefox)
S/M - vidalia can launch firefox
    - build a community version of firefox
    - pick our favorite extensions

Planned for 0.2.1.x:
  - enforce a lower limit on MaxCircuitDirtiness and CircuitBuildTimeout.
  - configurable timestamp granularity. defaults to 'seconds'.
  - consider making 'safelogging' extend to info-level logs too.
  - we should consider a single config option TorPrivateNetwork that
    turns on all the config options for running a private test tor
    network. having to keep updating all the tools, and the docs,
    just isn't working.
  - consider whether a single Guard flag lets us distinguish between
    "was good enough to be a guard when we picked it" and "is still
    adequate to be used as a guard even after we've picked it". We should
    write a real proposal for this.
  - switch out privoxy in the bundles and replace it with polipo.
  - make the new tls handshake blocking-resistant.
  - figure out some way to collect feedback about what countries are using
    bridges, in a way that doesn't screw anonymity too much.
  - let tor dir mirrors proxy connections to the tor download site, so
    if you know a bridge you can fetch the tor software.
  - more strategies for distributing bridge addresses in a way that
    doesn't rely on knowing somebody who runs a bridge for you.
  - A way to adjust router status flags from the controller.  (How do we
    prevent the authority from clobbering them soon afterward?)
  - Bridge authorities should do reachability testing but only on the
    purpose==bridge descriptors they have.
  - Clients should estimate their skew as median of skew from servers
    over last N seconds.
  - Investigate RAM use in Tor servers.
  - Start on the WSAENOBUFS solution.
  - Start on Windows auto-update for Tor

Deferred from 0.2.0.x:
  - Proposals
    - 113: Simplifying directory authority administration
    - 110: prevent infinite-length circuits (phase one)
    - 118: Listen on and advertise multiple ports:
      - Tor should be able to have a pool of outgoing IP addresses that it is
        able to rotate through. (maybe.  Possible overlap with proposal 118.)
      - config option to publish what ports you listen on, beyond
        ORPort/DirPort.  It should support ranges and bit prefixes (?) too.
        (This is very similar to proposal 118.)
    - 117: IPv6 Exits
      - Internal code support for ipv6:
        o Clone ipv6 functions (inet_ntop, inet_pton) where they don't exist.
        - Most address variables need to become tor_addr_t
        - Teach resolving code how to handle ipv6.
        - Teach exit policies about ipv6 (consider ipv4/ipv6 interaction!)
  - Features
    - Let controller set router flags for authority to transmit, and for
      client to use.
    - add an 'exit-address' line in the descriptor for servers that exit
      from something that isn't their published address.
    - More work on AvoidDiskWrites?
  - Features
    - Make a TCP DNSPort
  - Protocol work
    - MAYBE kill stalled circuits rather than stalled connections.  This is
      possible thanks to cell queues, but we need to consider the anonymity
      implications.
    - Implement TLS shutdown properly when possible.
  - Bugs
    - If the client's clock is too far in the past, it will drop (or just not
      try to get) descriptors, so it'll never build circuits.
  - Refactoring
    - Make resolves no longer use edge_connection_t unless they are actually
      _on_ a socks connection: have edge_connection_t and (say)
      dns_request_t both extend an edge_stream_t, and have p_streams and
      n_streams both be linked lists of edge_stream_t.
    - Generate torrc.{complete|sample}.in, tor.1.in, the HTML manual, and the
      online config documentation from a single source.
    - Move all status info out of routerinfo into local_routerstatus.  Make
      "who can change what" in local_routerstatus explicit.  Make
      local_routerstatus (or equivalent) subsume all places to go for "what
      router is this?"
  - Blocking/scanning-resistance
    - It would be potentially helpful to https requests on the OR port by
      acting like an HTTPS server.
    - Do we want to maintain our own set of entryguards that we use as
      next hop after the bridge? Open research question; let's say no
      for 0.2.0 unless we learn otherwise.
    - Some mechanism for specifying that we want to stop using a cached
      bridge.
  - Build:
    - Detect correct version of libraries from autoconf script.


Future versions:
  - See also Flyspray tasks.
  - See also all OPEN/ACCEPTED proposals.
  - See also all items marked XXXX and FFFF in the code.

  - Protocol:
    - Our current approach to block attempts to use Tor as a single-hop proxy
      is pretty lame; we should get a better one.
    - Allow small cells and large cells on the same network?
    - Cell buffering and resending. This will allow us to handle broken
      circuits as long as the endpoints don't break, plus will allow
      connection (tls session key) rotation.
    - Implement Morphmix, so we can compare its behavior, complexity,
      etc.  But see paper breaking morphmix.
    - Other transport. HTTP, udp, rdp, airhook, etc. May have to do our own
      link crypto, unless we can bully DTLS into it.
    - Need a relay teardown cell, separate from one-way ends.
      (Pending a user who needs this)
    - Handle half-open connections: right now we don't support all TCP
      streams, at least according to the protocol. But we handle all that
      we've seen in the wild.
      (Pending a user who needs this)

  - Directory system
    - BEGIN_DIR items
      X turn the received socks addr:port into a digest for setting .exit
      - handle connect-dir streams that don't have a chosen_exit_name set.
    - Have a "Faster" status flag that means it. Fast2, Fast4, Fast8?
    - Add an option (related to AvoidDiskWrites) to disable directory
      caching.  (Is this actually a good idea??)
    - Add d64 and fp64 along-side d and fp so people can paste status
      entries into a url. since + is a valid base64 char, only allow one
      at a time. Consider adding to controller as well.
    - Some back-out mechanism for auto-approval on authorities
      - a way of rolling back approvals to before a timestamp
        - Consider minion-like fingerprint file/log combination.
    - Have new people be in limbo and need to demonstrate usefulness
      before we approve them.

  - Hidden services:
    - Standby/hotswap/redundant hidden services.
    . Update the hidden service stuff for the new dir approach.  (Much
      of this will be superseded by 114.)
      - switch to an ascii format, maybe sexpr?
      - authdirservers publish blobs of them.
      - other authdirservers fetch these blobs.
      - hidserv people have the option of not uploading their blobs.
      - you can insert a blob via the controller.
      - and there's some amount of backwards compatibility.
      - teach clients, intro points, and hidservs about auth mechanisms.
      - come up with a few more auth mechanisms.
    - auth mechanisms to let hidden service midpoint and responder filter
      connection requests.
    - Let each hidden service (or other thing) specify its own
      OutboundBindAddress?
    - Hidserv offerers shouldn't need to define a SocksPort

  - Server operation
    X When we notice a 'Rejected: There is already a named server with
      this nickname' message... or maybe instead when we see in the
      networkstatuses that somebody else is Named with the name we
      want: warn the user, send a STATUS_SERVER message, and fall back
      to unnamed.
    - If the server is spewing complaints about raising your ulimit -n,
      we should add a note about this to the server descriptor so other
      people can notice too.
    - When we hit a funny error from a dir request (eg 403 forbidden),
      but tor is working and happy otherwise, and we haven't seen many
      such errors recently, then don't warn about it.

  - Controller
    - Implement missing status events and accompanying getinfos
      - DIR_REACHABLE
      - BAD_DIR_RESPONSE (Unexpected directory response; maybe we're behind
        a firewall.)
      - BAD_PROXY (Bad http or https proxy)
      - UNRECOGNIZED_ROUTER (a nickname we asked for is unavailable)
      - Status events related to hibernation
      - something about failing to parse our address?
        from resolve_my_address() in config.c
      - sketchy OS, sketchy threading
      - too many onions queued: threading problems or slow CPU?
    - Implement missing status event fields:
      - TIMEOUT on CHECKING_REACHABILITY
    - GETINFO status/client, status/server, status/general: There should be
      some way to learn which status events are currently "in effect."
      We should specify which these are, what format they appear in, and so
      on.
    - More information in events:
      - Include bandwidth breakdown by conn->type in BW events.
      - Change circuit status events to give more details, like purpose,
        whether they're internal, when they become dirty, when they become
        too dirty for further circuits, etc.
      - Change stream status events analogously.
    - Expose more information via getinfo:
      - import and export rendezvous descriptors
      - Review all static fields for additional candidates
    - Allow EXTENDCIRCUIT to unknown server.
      - We need some way to adjust server status, and to tell tor not to
        download directories/network-status, and a way to force a download.
      - Make everything work with hidden services

  - Performance/resources
    - per-conn write buckets
    - separate config options for read vs write limiting
      (It's hard to support read > write, since we need better
       congestion control to avoid overfull buffers there.  So,
       defer the whole thing.)
    - Look into pulling serverdescs off buffers as they arrive.
    - Rate limit exit connections to a given destination -- this helps
      us play nice with websites when Tor users want to crawl them; it
      also introduces DoS opportunities.
    - Consider truncating rather than destroying failed circuits,
      in order to save the effort of restarting.  There are security
      issues here that need thinking, though.
    - Handle full buffers without totally borking
    - Rate-limit OR and directory connections overall and per-IP and
      maybe per subnet.

  - Misc
    - Hold-open-until-flushed now works by accident; it should work by
      design.
    - Display the reasons in 'destroy' and 'truncated' cells under
      some circumstances?
    - Make router_is_general_exit() a bit smarter once we're sure what
      it's for.
    - Automatically determine what ports are reachable and start using
      those, if circuits aren't working and it's a pattern we
      recognize ("port 443 worked once and port 9001 keeps not
      working").

  - Security
    - some better fix for bug #516?
    - don't do dns hijacking tests if we're reject *:* exit policy?
      (deferred until 0.1.1.x is less common)
    - Directory guards
    - Mini-SoaT:
      - Servers might check certs for known-good ssl websites, and if
        they come back self-signed, declare themselves to be
        non-exits.  Similar to how we test for broken/evil dns now.
      - Authorities should try using exits for http to connect to some
        URLS (specified in a configuration file, so as not to make the
        List Of Things Not To Censor completely obvious) and ask them
        for results.  Exits that don't give good answers should have
        the BadExit flag set.
      - Alternatively, authorities should be able to import opinions
        from Snakes on a Tor.
    - More consistent error checking in router_parse_entry_from_string().
      I can say "banana" as my bandwidthcapacity, and it won't even squeak.
    - Bind to random port when making outgoing connections to Tor servers,
      to reduce remote sniping attacks.
    - Audit everything to make sure rend and intro points are just as
      likely to be us as not.
    - Do something to prevent spurious EXTEND cells from making
      middleman nodes connect all over.  Rate-limit failed
      connections, perhaps?
    - DoS protection: TLS puzzles, public key ops, bandwidth exhaustion.

  - Needs thinking
    - Now that we're avoiding exits when picking non-exit positions,
      we need to consider how to pick nodes for internal circuits. If
      we avoid exits for all positions, we skew the load balancing. If
      we accept exits for all positions, we leak whether it's an
      internal circuit at every step. If we accept exits only at the
      last hop, we reintroduce Lasse's attacks from the Oakland paper.

  - Windows server usability
    - Solve the ENOBUFS problem.
      - make tor's use of openssl operate on buffers rather than sockets,
        so we can make use of libevent's buffer paradigm once it has one.
      - make tor's use of libevent tolerate either the socket or the
        buffer paradigm; includes unifying the functions in connect.c.
    - We need a getrlimit equivalent on Windows so we can reserve some
      file descriptors for saving files, etc. Otherwise we'll trigger
      asserts when we're out of file descriptors and crash.
    - Merge code from Urz into libevent
    - Make Tor use evbuffers.

  - Documentation
    - a way to generate the website diagrams from source, so we can
      translate them as utf-8 text rather than with gimp. (svg? or
      imagemagick?)
    . Flesh out options_description array in src/or/config.c
    . multiple sample torrc files
    . figure out how to make nt service stuff work?
      . Document it.
    - Refactor tor man page to divide generally useful options from
      less useful ones?
    - Add a doxygen style checker to make check-spaces so nick doesn't drift
       too far from arma's undocumented styleguide.  Also, document that
       styleguide in HACKING.  (See r9634 for example.)
       - exactly one space at beginning and at end of comments, except i
         guess when there's line-length pressure.
       - if we refer to a function name, put a () after it.
       - only write <b>foo</b> when foo is an argument to this function.
       - doxygen comments must always end in some form of punctuation.
       - capitalize the first sentence in the doxygen comment, except
         when you shouldn't.
       - avoid spelling errors and incorrect comments. ;)

  - Packaging
    - The Debian package now uses --verify-config when (re)starting,
      to distinguish configuration errors from other errors. Perhaps
      the RPM and other startup scripts should too?
    - add a "default.action" file to the tor/vidalia bundle so we can
      fix the https thing in the default configuration:
      http://wiki.noreply.org/noreply/TheOnionRouter/TorFAQ#PrivoxyWeirdSSLPort

  - Related tools
    - Patch privoxy and socks protocol to pass strings to the browser.


Documentation, non-version-specific.
  - Specs
    - Mark up spec; note unclear points about servers
NR  - write a spec appendix for 'being nice with tor'
    - Specify the keys and key rotation schedules and stuff
  - Mention controller libs someplace.
  - Remove need for HACKING file.
  - document http://wiki.noreply.org/noreply/TheOnionRouter/TransparentProxy on freebsd and osx
P - figure out why x86_64 won't build rpms from tor.spec
P - figure out spec files for bundles of vidalia-tor-polipo
P - figure out polipo install scripts for bundles of vidalia-tor-polipo on osx, win32
  - figure out selinux policy for tor
P - change packaging system to more automated and specific for each
     platform, suggested by Paul Wouter
P - Setup repos for redhat and suse rpms & start signing the rpms the
    way package management apps prefer

Website:
J  - tor-in-the-media page
P  - Figure out licenses for website material.
    (Phobos reccomends the Open Publication License at
    http://opencontent.org/openpub/)
P  - put the logo on the website, in source form, so people can put it on
    stickers directly, etc.
P  - put the source image for the stickers on the website, so people can
    print their own
P - figure out a license for the logos and docs we publish (trademark
figures into this)
    (Phobos reccomends the Open Publication License at
    http://opencontent.org/openpub/)
R - make a page with the hidden service diagrams.
P  - ask Jan/Jens to be the translation coordinator? add to volunteer page.
  - add a page for localizing all tor's components.
  - It would be neat if we had a single place that described _all_ the
    tor-related tools you can use, and what they give you, and how well they
    work.  Right now, we don't give a lot of guidance wrt
    torbutton/foxproxy/privoxy/polipo in any consistent place.
P - create a 'blog badge' for tor fans to link to and feature on their
    blogs. A sample can be found at http://interloper.org/tmp/tor/tor-button.png

  - Tor mirrors
    - make a mailing list with the mirror operators
    - make an automated tool to check /project/trace/ at mirrors to
      learn which ones are lagging behind.
    - auto (or manually) cull the mirrors that are broken; and
      contact their operator?
    - a set of instructions for mirror operators to make their apaches
      serve our charsets correctly, and bonus points for language
      negotiation.
    - figure out how to load-balance the downloads across mirrors?
    - ponder how to get users to learn that they should google for
      "tor mirrors" if the main site is blocked.
    - find a mirror volunteer to coordinate all of this

