```
Filename: 224-rend-spec-ng.txt
Title: Next-Generation Hidden Services in Tor
Author: David Goulet, George Kadianakis, Nick Mathewson
Created: 2013-11-29
Status: Closed
Implemented-In: 0.3.2.1-alpha

Table of contents:

    0. Hidden services: overview and preliminaries.
        0.1. Improvements over previous versions.
        0.2. Notation and vocabulary
        0.3. Cryptographic building blocks
        0.4. Protocol building blocks [BUILDING-BLOCKS]
        0.5. Assigned relay cell types
        0.6. Acknowledgments
    1. Protocol overview
        1.1. View from 10,000 feet
        1.2. In more detail: naming hidden services [NAMING]
        1.3. In more detail: Access control [IMD:AC]
        1.4. In more detail: Distributing hidden service descriptors. [IMD:DIST]
        1.5. In more detail: Scaling to multiple hosts
        1.6. In more detail: Backward compatibility with older hidden service
        1.7. In more detail: Keeping crypto keys offline
        1.8. In more detail: Encryption Keys And Replay Resistance
        1.9. In more detail: A menagerie of keys
            1.9.1. In even more detail: Client authorization [CLIENT-AUTH]
    2. Generating and publishing hidden service descriptors [HSDIR]
        2.1. Deriving blinded keys and subcredentials [SUBCRED]
        2.2. Locating, uploading, and downloading hidden service descriptors
            2.2.1. Dividing time into periods [TIME-PERIODS]
            2.2.2. When to publish a hidden service descriptor [WHEN-HSDESC]
            2.2.3. Where to publish a hidden service descriptor [WHERE-HSDESC]
            2.2.4. Using time periods and SRVs to fetch/upload HS descriptors
            2.2.5. Expiring hidden service descriptors [EXPIRE-DESC]
            2.2.6. URLs for anonymous uploading and downloading
        2.3. Publishing shared random values [PUB-SHAREDRANDOM]
            2.3.1. Client behavior in the absense of shared random values
            2.3.2. Hidden services and changing shared random values
        2.4. Hidden service descriptors: outer wrapper [DESC-OUTER]
        2.5. Hidden service descriptors: encryption format [HS-DESC-ENC]
            2.5.1. First layer of encryption [HS-DESC-FIRST-LAYER]
                2.5.1.1. First layer encryption logic
                2.5.1.2. First layer plaintext format
                2.5.1.3. Client behavior
                2.5.1.4. Obfuscating the number of authorized clients
            2.5.2. Second layer of encryption [HS-DESC-SECOND-LAYER]
                2.5.2.1. Second layer encryption keys
                2.5.2.2. Second layer plaintext format
            2.5.3. Deriving hidden service descriptor encryption keys [HS-DESC-ENCRYPTION-KEYS]
    3. The introduction protocol [INTRO-PROTOCOL]
        3.1. Registering an introduction point [REG_INTRO_POINT]
            3.1.1. Extensible ESTABLISH_INTRO protocol. [EST_INTRO]
            3.1.2. Registering an introduction point on a legacy Tor node [LEGACY_EST_INTRO]
            3.1.3. Acknowledging establishment of introduction point [INTRO_ESTABLISHED]
        3.2. Sending an INTRODUCE1 cell to the introduction point. [SEND_INTRO1]
            3.2.1. INTRODUCE1 cell format [FMT_INTRO1]
            3.2.2. INTRODUCE_ACK cell format. [INTRO_ACK]
        3.3. Processing an INTRODUCE2 cell at the hidden service. [PROCESS_INTRO2]
            3.3.1. Introduction handshake encryption requirements [INTRO-HANDSHAKE-REQS]
            3.3.2. Example encryption handshake: ntor with extra data [NTOR-WITH-EXTRA-DATA]
        3.4. Authentication during the introduction phase. [INTRO-AUTH]
            3.4.1. Ed25519-based authentication.
    4. The rendezvous protocol
        4.1. Establishing a rendezvous point [EST_REND_POINT]
        4.2. Joining to a rendezvous point [JOIN_REND]
            4.2.1. Key expansion
        4.3. Using legacy hosts as rendezvous points
    5. Encrypting data between client and host
    6. Encoding onion addresses [ONIONADDRESS]
    7. Open Questions:

-1. Draft notes

   This document describes a proposed design and specification for
   hidden services in Tor version 0.2.5.x or later. It's a replacement
   for the current rend-spec.txt, rewritten for clarity and for improved
   design.

   Look for the string "TODO" below: it describes gaps or uncertainties
   in the design.

   Change history:

       2013-11-29: Proposal first numbered. Some TODO and XXX items remain.

       2014-01-04: Clarify some unclear sections.

       2014-01-21: Fix a typo.

       2014-02-20: Move more things to the revised certificate format in the
           new updated proposal 220.

       2015-05-26: Fix two typos.


0. Hidden services: overview and preliminaries.

   Hidden services aim to provide responder anonymity for bidirectional
   stream-based communication on the Tor network. Unlike regular Tor
   connections, where the connection initiator receives anonymity but
   the responder does not, hidden services attempt to provide
   bidirectional anonymity.

   Participants:

      Operator -- A person running a hidden service

      Host, "Server" -- The Tor software run by the operator to provide
         a hidden service.

      User -- A person contacting a hidden service.

      Client -- The Tor software running on the User's computer

      Hidden Service Directory (HSDir) -- A Tor node that hosts signed
        statements from hidden service hosts so that users can make
        contact with them.

      Introduction Point -- A Tor node that accepts connection requests
        for hidden services and anonymously relays those requests to the
        hidden service.

      Rendezvous Point -- A Tor node to which clients and servers
        connect and which relays traffic between them.

0.1. Improvements over previous versions.

   Here is a list of improvements of this proposal over the legacy hidden
   services:

   a) Better crypto (replaced SHA1/DH/RSA1024 with SHA3/ed25519/curve25519)
   b) Improved directory protocol leaking less to directory servers.
   c) Improved directory protocol with smaller surface for targeted attacks.
   d) Better onion address security against impersonation.
   e) More extensible introduction/rendezvous protocol.
   f) Offline keys for onion services
   g) Advanced client authorization

0.2. Notation and vocabulary

   Unless specified otherwise, all multi-octet integers are big-endian.

   We write sequences of bytes in two ways:

     1. A sequence of two-digit hexadecimal values in square brackets,
        as in [AB AD 1D EA].

     2. A string of characters enclosed in quotes, as in "Hello". The
        characters in these strings are encoded in their ascii
        representations; strings are NOT nul-terminated unless
        explicitly described as NUL terminated.

   We use the words "byte" and "octet" interchangeably.

   We use the vertical bar | to denote concatenation.

   We use INT_N(val) to denote the network (big-endian) encoding of the
   unsigned integer "val" in N bytes. For example, INT_4(1337) is [00 00
   05 39]. Values are truncated like so: val % (2 ^ (N * 8)). For example,
   INT_4(42) is 42 % 4294967296 (32 bit).

0.3. Cryptographic building blocks

   This specification uses the following cryptographic building blocks:

      * A pseudorandom number generator backed by a strong entropy source.
        The output of the PRNG should always be hashed before being posted on
        the network to avoid leaking raw PRNG bytes to the network
        (see [PRNG-REFS]).

      * A stream cipher STREAM(iv, k) where iv is a nonce of length
        S_IV_LEN bytes and k is a key of length S_KEY_LEN bytes.

      * A public key signature system SIGN_KEYGEN()->seckey, pubkey;
        SIGN_SIGN(seckey,msg)->sig; and SIGN_CHECK(pubkey, sig, msg) ->
        { "OK", "BAD" }; where secret keys are of length SIGN_SECKEY_LEN
        bytes, public keys are of length SIGN_PUBKEY_LEN bytes, and
        signatures are of length SIGN_SIG_LEN bytes.

        This signature system must also support key blinding operations
        as discussed in appendix [KEYBLIND] and in section [SUBCRED]:
        SIGN_BLIND_SECKEY(seckey, blind)->seckey2 and
        SIGN_BLIND_PUBKEY(pubkey, blind)->pubkey2 .

      * A public key agreement system "PK", providing
        PK_KEYGEN()->seckey, pubkey; PK_VALID(pubkey) -> {"OK", "BAD"};
        and PK_HANDSHAKE(seckey, pubkey)->output; where secret keys are
        of length PK_SECKEY_LEN bytes, public keys are of length
        PK_PUBKEY_LEN bytes, and the handshake produces outputs of
        length PK_OUTPUT_LEN bytes.

      * A cryptographic hash function H(d), which should be preimage and
        collision resistant. It produces hashes of length HASH_LEN
        bytes.

      * A cryptographic message authentication code MAC(key,msg) that
        produces outputs of length MAC_LEN bytes.

      * A key derivation function KDF(message, n) that outputs n bytes.

   As a first pass, I suggest:

      * Instantiate STREAM with AES256-CTR.

      * Instantiate SIGN with Ed25519 and the blinding protocol in
        [KEYBLIND].

      * Instantiate PK with Curve25519.

      * Instantiate H with SHA3-256.

      * Instantiate KDF with SHAKE-256.

      * Instantiate MAC(key=k, message=m) with H(k_len | k | m),
        where k_len is htonll(len(k)).

   For legacy purposes, we specify compatibility with older versions of
   the Tor introduction point and rendezvous point protocols. These used
   RSA1024, DH1024, AES128, and SHA1, as discussed in
   rend-spec.txt.

   As in [proposal 220], all signatures are generated not over strings
   themselves, but over those strings prefixed with a distinguishing
   value.

0.4. Protocol building blocks [BUILDING-BLOCKS]

   In sections below, we need to transmit the locations and identities
   of Tor nodes. We do so in the link identification format used by
   EXTEND2 cells in the Tor protocol.

         NSPEC      (Number of link specifiers)   [1 byte]
         NSPEC times:
           LSTYPE (Link specifier type)           [1 byte]
           LSLEN  (Link specifier length)         [1 byte]
           LSPEC  (Link specifier)                [LSLEN bytes]

   Link specifier types are as described in tor-spec.txt. Every set of
   link specifiers MUST include at minimum specifiers of type [00]
   (TLS-over-TCP, IPv4), [02] (legacy node identity) and [03] (ed25519
   identity key).

   We also incorporate Tor's circuit extension handshakes, as used in
   the CREATE2 and CREATED2 cells described in tor-spec.txt. In these
   handshakes, a client who knows a public key for a server sends a
   message and receives a message from that server. Once the exchange is
   done, the two parties have a shared set of forward-secure key
   material, and the client knows that nobody else shares that key
   material unless they control the secret key corresponding to the
   server's public key.

0.5. Assigned relay cell types

   These relay cell types are reserved for use in the hidden service
   protocol.

      32 -- RELAY_COMMAND_ESTABLISH_INTRO

            Sent from hidden service host to introduction point;
            establishes introduction point. Discussed in
            [REG_INTRO_POINT].

      33 -- RELAY_COMMAND_ESTABLISH_RENDEZVOUS

            Sent from client to rendezvous point; creates rendezvous
            point. Discussed in [EST_REND_POINT].

      34 -- RELAY_COMMAND_INTRODUCE1

            Sent from client to introduction point; requests
            introduction. Discussed in [SEND_INTRO1]

      35 -- RELAY_COMMAND_INTRODUCE2

            Sent from introduction point to hidden service host; requests
            introduction. Same format as INTRODUCE1. Discussed in
            [FMT_INTRO1] and [PROCESS_INTRO2]

      36 -- RELAY_COMMAND_RENDEZVOUS1

            Sent from hidden service host to rendezvous point;
            attempts to join host's circuit to
            client's circuit. Discussed in [JOIN_REND]

      37 -- RELAY_COMMAND_RENDEZVOUS2

            Sent from rendezvous point to client;
            reports join of host's circuit to
            client's circuit. Discussed in [JOIN_REND]

      38 -- RELAY_COMMAND_INTRO_ESTABLISHED

            Sent from introduction point to hidden service host;
            reports status of attempt to establish introduction
            point. Discussed in [INTRO_ESTABLISHED]

      39 -- RELAY_COMMAND_RENDEZVOUS_ESTABLISHED

            Sent from rendezvous point to client; acknowledges
            receipt of ESTABLISH_RENDEZVOUS cell. Discussed in
            [EST_REND_POINT]

      40 -- RELAY_COMMAND_INTRODUCE_ACK

            Sent from introduction point to client; acknowledges
            receipt of INTRODUCE1 cell and reports success/failure.
            Discussed in [INTRO_ACK]

0.6. Acknowledgments

   This design includes ideas from many people, including
     Christopher Baines,
     Daniel J. Bernstein,
     Matthew Finkel,
     Ian Goldberg,
     George Kadianakis,
     Aniket Kate,
     Tanja Lange,
     Robert Ransom,
     Roger Dingledine,
     Aaron Johnson,
     Tim Wilson-Brown ("teor"),
     special (John Brooks),
     s7r

   It's based on Tor's original hidden service design by Roger
   Dingledine, Nick Mathewson, and Paul Syverson, and on improvements to
   that design over the years by people including
     Tobias Kamm,
     Thomas Lauterbach,
     Karsten Loesing,
     Alessandro Preite Martinez,
     Robert Ransom,
     Ferdinand Rieger,
     Christoph Weingarten,
     Christian Wilms,

   We wouldn't be able to do any of this work without good attack
   designs from researchers including
     Alex Biryukov,
     Lasse Øverlier,
     Ivan Pustogarov,
     Paul Syverson
     Ralf-Philipp Weinmann,
   See [ATTACK-REFS] for their papers.

   Several of these ideas have come from conversations with
      Christian Grothoff,
      Brian Warner,
      Zooko Wilcox-O'Hearn,

   And if this document makes any sense at all, it's thanks to
   editing help from
      Matthew Finkel
      George Kadianakis,
      Peter Palfrader,
      Tim Wilson-Brown ("teor"),


   [XXX  Acknowledge the huge bunch of people working on 8106.]
   [XXX  Acknowledge the huge bunch of people working on 8244.]


   Please forgive me if I've missed you; please forgive me if I've
   misunderstood your best ideas here too.


1. Protocol overview

   In this section, we outline the hidden service protocol. This section
   omits some details in the name of simplicity; those are given more
   fully below, when we specify the protocol in more detail.

1.1. View from 10,000 feet

   A hidden service host prepares to offer a hidden service by choosing
   several Tor nodes to serve as its introduction points. It builds
   circuits to those nodes, and tells them to forward introduction
   requests to it using those circuits.

   Once introduction points have been picked, the host builds a set of
   documents called "hidden service descriptors" (or just "descriptors"
   for short) and uploads them to a set of HSDir nodes. These documents
   list the hidden service's current introduction points and describe
   how to make contact with the hidden service.

   When a client wants to connect to a hidden service, it first chooses
   a Tor node at random to be its "rendezvous point" and builds a
   circuit to that rendezvous point. If the client does not have an
   up-to-date descriptor for the service, it contacts an appropriate
   HSDir and requests such a descriptor.

   The client then builds an anonymous circuit to one of the hidden
   service's introduction points listed in its descriptor, and gives the
   introduction point an introduction request to pass to the hidden
   service. This introduction request includes the target rendezvous
   point and the first part of a cryptographic handshake.

   Upon receiving the introduction request, the hidden service host
   makes an anonymous circuit to the rendezvous point and completes the
   cryptographic handshake. The rendezvous point connects the two
   circuits, and the cryptographic handshake gives the two parties a
   shared key and proves to the client that it is indeed talking to the
   hidden service.

   Once the two circuits are joined, the client can send Tor RELAY cells
   to the server. RELAY_BEGIN cells open streams to an external process
   or processes configured by the server; RELAY_DATA cells are used to
   communicate data on those streams, and so forth.

1.2. In more detail: naming hidden services [NAMING]

   A hidden service's name is its long term master identity key.  This is
   encoded as a hostname by encoding the entire key in Base 32, including a
   version byte and a checksum, and then appending the string ".onion" at the
   end. The result is a 56-character domain name.

   (This is a change from older versions of the hidden service protocol,
   where we used an 80-bit truncated SHA1 hash of a 1024 bit RSA key.)

   The names in this format are distinct from earlier names because of
   their length. An older name might look like:

        unlikelynamefora.onion
        yyhws9optuwiwsns.onion

   And a new name following this specification might look like:

        l5satjgud6gucryazcyvyvhuxhr74u6ygigiuyixe3a6ysis67ororad.onion

   Please see section [ONIONADDRESS] for the encoding specification.

1.3. In more detail: Access control [IMD:AC]

   Access control for a hidden service is imposed at multiple points through
   the process above. Furthermore, there is also the option to impose
   additional client authorization access control using pre-shared secrets
   exchanged out-of-band between the hidden service and its clients.

   The first stage of access control happens when downloading HS descriptors.
   Specifically, in order to download a descriptor, clients must know which
   blinded signing key was used to sign it. (See the next section for more info
   on key blinding.)

   To learn the introduction points, clients must decrypt the body of the
   hidden service descriptor. To do so, clients must know the _unblinded_
   public key of the service, which makes the descriptor unuseable by entities
   without that knowledge (e.g. HSDirs that don't know the onion address).

   Also, if optional client authorization is enabled, hidden service
   descriptors are superencrypted using each authorized user's identity x25519
   key, to further ensure that unauthorized entities cannot decrypt it.

   In order to make the introduction point send a rendezvous request to the
   service, the client needs to use the per-introduction-point authentication
   key found in the hidden service descriptor.

   The final level of access control happens at the server itself, which may
   decide to respond or not respond to the client's request depending on the
   contents of the request. The protocol is extensible at this point: at a
   minimum, the server requires that the client demonstrate knowledge of the
   contents of the encrypted portion of the hidden service descriptor. If
   optional client authorization is enabled, the service may additionally
   require the client to prove knowledge of a pre-shared private key.

1.4. In more detail: Distributing hidden service descriptors. [IMD:DIST]

   Periodically, hidden service descriptors become stored at different
   locations to prevent a single directory or small set of directories
   from becoming a good DoS target for removing a hidden service.

   For each period, the Tor directory authorities agree upon a
   collaboratively generated random value. (See section 2.3 for a
   description of how to incorporate this value into the voting
   practice; generating the value is described in other proposals,
   including [SHAREDRANDOM-REFS].) That value, combined with hidden service
   directories' public identity keys, determines each HSDir's position
   in the hash ring for descriptors made in that period.

   Each hidden service's descriptors are placed into the ring in
   positions based on the key that was used to sign them. Note that
   hidden service descriptors are not signed with the services' public
   keys directly. Instead, we use a key-blinding system [KEYBLIND] to
   create a new key-of-the-day for each hidden service. Any client that
   knows the hidden service's credential can derive these blinded
   signing keys for a given period. It should be impossible to derive
   the blinded signing key lacking that credential.

   The body of each descriptor is also encrypted with a key derived from
   the credential.

   To avoid a "thundering herd" problem where every service generates
   and uploads a new descriptor at the start of each period, each
   descriptor comes online at a time during the period that depends on
   its blinded signing key. The keys for the last period remain valid
   until the new keys come online.

1.5. In more detail: Scaling to multiple hosts

   This design is compatible with our current approaches for scaling hidden
   services. Specifically, hidden service operators can use onionbalance to
   achieve high availability between multiple nodes on the HSDir
   layer. Furthermore, operators can use proposal 255 to load balance their
   hidden services on the introduction layer. See [SCALING-REFS] for further
   discussions on this topic and alternative designs.

1.6. In more detail: Backward compatibility with older hidden service
      protocols

   This design is incompatible with the clients, server, and hsdir node
   protocols from older versions of the hidden service protocol as
   described in rend-spec.txt. On the other hand, it is designed to
   enable the use of older Tor nodes as rendezvous points and
   introduction points.

1.7. In more detail: Keeping crypto keys offline

   In this design, a hidden service's secret identity key may be
   stored offline.  It's used only to generate blinded signing keys,
   which are used to sign descriptor signing keys.

   In order to operate a hidden service, the operator can generate in
   advance a number of blinded signing keys and descriptor signing
   keys (and their credentials; see [DESC-OUTER] and [HS-DESC-ENC]
   below), and their corresponding descriptor encryption keys, and
   export those to the hidden service hosts.

   As a result, in the scenario where the Hidden Service gets
   compromised, the adversary can only impersonate it for a limited
   period of time (depending on how many signing keys were generated
   in advance).

   It's important to not send the private part of the blinded signing
   key to the Hidden Service since an attacker can derive from it the
   secret master identity key. The secret blinded signing key should
   only be used to create credentials for the descriptor signing keys.

1.8. In more detail: Encryption Keys And Replay Resistance

   To avoid replays of an introduction request by an introduction point,
   a hidden service host must never accept the same request
   twice. Earlier versions of the hidden service design used an
   authenticated timestamp here, but including a view of the current
   time can create a problematic fingerprint. (See proposal 222 for more
   discussion.)

1.9. In more detail: A menagerie of keys

   [In the text below, an "encryption keypair" is roughly "a keypair you
   can do Diffie-Hellman with" and a "signing keypair" is roughly "a
   keypair you can do ECDSA with."]

   Public/private keypairs defined in this document:

      Master (hidden service) identity key -- A master signing keypair
        used as the identity for a hidden service.  This key is long
        term and not used on its own to sign anything; it is only used
        to generate blinded signing keys as described in [KEYBLIND]
        and [SUBCRED]. The public key is encoded in the ".onion"
        address according to [NAMING].

      Blinded signing key -- A keypair derived from the identity key,
        used to sign descriptor signing keys. It changes periodically for
        each service. Clients who know a 'credential' consisting of the
        service's public identity key and an optional secret can derive
        the public blinded identity key for a service.  This key is used
        as an index in the DHT-like structure of the directory system
        (see [SUBCRED]).

      Descriptor signing key -- A key used to sign hidden service
        descriptors.  This is signed by blinded signing keys. Unlike
        blinded signing keys and master identity keys, the secret part
        of this key must be stored online by hidden service hosts. The
        public part of this key is included in the unencrypted section
        of HS descriptors (see [DESC-OUTER]).

      Introduction point authentication key -- A short-term signing
        keypair used to identify a hidden service to a given
        introduction point. A fresh keypair is made for each
        introduction point; these are used to sign the request that a
        hidden service host makes when establishing an introduction
        point, so that clients who know the public component of this key
        can get their introduction requests sent to the right
        service. No keypair is ever used with more than one introduction
        point. (previously called a "service key" in rend-spec.txt)

      Introduction point encryption key -- A short-term encryption
        keypair used when establishing connections via an introduction
        point. Plays a role analogous to Tor nodes' onion keys. A fresh
        keypair is made for each introduction point.

   Symmetric keys defined in this document:

      Descriptor encryption keys -- A symmetric encryption key used to
        encrypt the body of hidden service descriptors. Derived from the
        current period and the hidden service credential.

   Public/private keypairs defined elsewhere:

      Onion key -- Short-term encryption keypair

      (Node) identity key

   Symmetric key-like things defined elsewhere:

      KH from circuit handshake -- An unpredictable value derived as
      part of the Tor circuit extension handshake, used to tie a request
      to a particular circuit.

1.9.1. In even more detail: Client authorization keys [CLIENT-AUTH]

   When client authorization is enabled, each authorized client of a hidden
   service has two more assymetric keypairs which are shared with the hidden
   service. An entity without those keys is not able to use the hidden
   service. Throughout this document, we assume that these pre-shared keys are
   exchanged between the hidden service and its clients in a secure out-of-band
   fashion.

   Specifically, each authorized client possesses:

   - An x25519 keypair used to compute decryption keys that allow the client to
     decrypt the hidden service descriptor. See [HS-DESC-ENC].

   - An ed25519 keypair which allows the client to compute signatures which
     prove to the hidden service that the client is authorized. These
     signatures are inserted into the INTRODUCE1 cell, and without them the
     introduction to the hidden service cannot be completed. See [INTRO-AUTH].

   The right way to exchange these keys is to have the client generate keys and
   send the corresponding public keys to the hidden service out-of-band. An
   easier but less secure way of doing this exchange would be to have the
   hidden service generate the keypairs and pass the corresponding private keys
   to its clients. See section [CLIENT-AUTH-MGMT] for more details on how these
   keys should be managed.

   [TODO: Also specify stealth client authorization.]

2. Generating and publishing hidden service descriptors [HSDIR]

   Hidden service descriptors follow the same metaformat as other Tor
   directory objects. They are published anonymously to Tor servers with the
   HSDir flag, HSDir=2 protocol version and tor version >= 0.3.0.8 (because a
   bug was fixed in this version).

2.1. Deriving blinded keys and subcredentials [SUBCRED]

   In each time period (see [TIME-PERIODS] for a definition of time
   periods), a hidden service host uses a different blinded private key
   to sign its directory information, and clients use a different
   blinded public key as the index for fetching that information.

   For a candidate for a key derivation method, see Appendix [KEYBLIND].

   Additionally, clients and hosts derive a subcredential for each
   period. Knowledge of the subcredential is needed to decrypt hidden
   service descriptors for each period and to authenticate with the
   hidden service host in the introduction process. Unlike the
   credential, it changes each period. Knowing the subcredential, even
   in combination with the blinded private key, does not enable the
   hidden service host to derive the main credential--therefore, it is
   safe to put the subcredential on the hidden service host while
   leaving the hidden service's private key offline.

   The subcredential for a period is derived as:

       subcredential = H("subcredential" | credential | blinded-public-key).

   In the above formula, credential corresponds to:

       credential = H("credential" | public-identity-key)

   where public-identity-key is the public identity master key of the hidden
   service.

2.2. Locating, uploading, and downloading hidden service descriptors
       [HASHRING]

   To avoid attacks where a hidden service's descriptor is easily
   targeted for censorship, we store them at different directories over
   time, and use shared random values to prevent those directories from
   being predictable far in advance.

   Which Tor servers hosts a hidden service depends on:

         * the current time period,
         * the daily subcredential,
         * the hidden service directories' public keys,
         * a shared random value that changes in each time period,
         * a set of network-wide networkstatus consensus parameters.
           (Consensus parameters are integer values voted on by authorities
           and published in the consensus documents, described in
           dir-spec.txt, section 3.3.)

   Below we explain in more detail.

2.2.1. Dividing time into periods [TIME-PERIODS]

   To prevent a single set of hidden service directory from becoming a
   target by adversaries looking to permanently censor a hidden service,
   hidden service descriptors are uploaded to different locations that
   change over time.

   The length of a "time period" is controlled by the consensus
   parameter 'hsdir-interval', and is a number of minutes between 30 and
   14400 (10 days). The default time period length is 1440 (one day).

   Time periods start at the Unix epoch (Jan 1, 1970), and are computed by
   taking the number of minutes since the epoch and dividing by the time
   period. However, we want our time periods to start at 12:00UTC every day, so
   we subtract a "rotation time offset" of 12*60 minutes from the number of
   minutes since the epoch, before dividing by the time period (effectively
   making "our" epoch start at Jan 1, 1970 12:00UTC).

   Example: If the current time is 2016-04-13 11:15:01 UTC, making the seconds
   since the epoch 1460546101, and the number of minutes since the epoch
   24342435.  We then subtract the "rotation time offset" of 12*60 minutes from
   the minutes since the epoch, to get 24341715. If the current time period
   length is 1440 minutes, by doing the division we see that we are currently
   in time period number 16903.

   Specifically, time period #16903 began 16903*1440*60 + (12*60*60) seconds
   after the epoch, at 2016-04-12 12:00 UTC, and ended at 16904*1440*60 +
   (12*60*60) seconds after the epoch, at 2016-04-13 12:00 UTC.

2.2.2. When to publish a hidden service descriptor [WHEN-HSDESC]

   Hidden services periodically publish their descriptor to the responsible
   HSDirs. The set of responsible HSDirs is determined as specified in
   [WHERE-HSDESC].

   Specifically, everytime a hidden service publishes its descriptor, it also
   sets up a timer for a random time between 60 minutes and 120 minutes in the
   future. When the timer triggers, the hidden service needs to publish its
   descriptor again to the responsible HSDirs for that time period.
   [TODO: Control republish period using a consensus parameter?]

2.2.2.1. Overlapping descriptors

   Hidden services need to upload multiple descriptors so that they can be
   reachable to clients with older or newer consensuses than them. Services
   need to upload their descriptors to the HSDirs _before_ the beginning of
   each upcoming time period, so that they are readily available for clients to
   fetch them. Furthermore, services should keep uploading their old descriptor
   even after the end of a time period, so that they can be reachable by
   clients that still have consensuses from the previous time period.

   Hence, services maintain two active descriptors at every point. Clients on
   the other hand, don't have a notion of overlapping descriptors, and instead
   always download the descriptor for the current time period and shared random
   value. It's the job of the service to ensure that descriptors will be
   available for all clients. See section [FETCHUPLOADDESC] for how this is
   achieved.

   [TODO: What to do when we run multiple hidden services in a single host?]

2.2.3. Where to publish a hidden service descriptor [WHERE-HSDESC]

   This section specifies how the HSDir hash ring is formed at any given
   time. Whenever a time value is needed (e.g. to get the current time period
   number), we assume that clients and services use the valid-after time from
   their latest live consensus.

   The following consensus parameters control where a hidden service
   descriptor is stored;

        hsdir_n_replicas = an integer in range [1,16] with default value 2.
        hsdir_spread_fetch = an integer in range [1,128] with default value 3.
        hsdir_spread_store = an integer in range [1,128] with default value 3.

   To determine where a given hidden service descriptor will be stored
   in a given period, after the blinded public key for that period is
   derived, the uploading or downloading party calculates:

        for replicanum in 1...hsdir_n_replicas:
            hs_index(replicanum) = H("store-at-idx" |
                                     blinded_public_key |
                                     INT_8(replicanum) |
                                     INT_8(period_length) |
                                     INT_8(period_num) )

   where blinded_public_key is specified in section [KEYBLIND], period_length
   is the length of the time period in minutes, and period_num is calculated
   using the current consensus "valid-after" as specified in section
   [TIME-PERIODS].

   Then, for each node listed in the current consensus with the HSDirV3 flag,
   we compute a directory index for that node as:

           hsdir_index(node) = H("node-idx" | node_identity |
                                 shared_random_value |
                                 INT_8(period_num) |
                                 INT_8(period_length) )

   where shared_random_value is the shared value generated by the authorities
   in section [PUB-SHAREDRANDOM], and node_identity is the ed25519 identity
   key of the node.

   Finally, for replicanum in 1...hsdir_n_replicas, the hidden service
   host uploads descriptors to the first hsdir_spread_store nodes whose
   indices immediately follow hs_index(replicanum). If any of those
   nodes have already been selected for a lower-numbered replica of the
   service, any nodes already chosen are disregarded (i.e. skipped over)
   when choosing a replica's hsdir_spread_store nodes.

   When choosing an HSDir to download from, clients choose randomly from
   among the first hsdir_spread_fetch nodes after the indices.  (Note
   that, in order to make the system better tolerate disappearing
   HSDirs, hsdir_spread_fetch may be less than hsdir_spread_store.)
   Again, nodes from lower-numbered replicas are disregarded when
   choosing the spread for a replica.

2.2.4. Using time periods and SRVs to fetch/upload HS descriptors [FETCHUPLOADDESC]

   Hidden services and clients need to make correct use of time periods (TP)
   and shared random values (SRVs) to successfuly fetch and upload
   descriptors. Furthermore, to avoid problems with skewed clocks, both clients
   and services use the 'valid-after' time of a live consensus as a way to take
   decisions with regards to uploading and fetching descriptors. By using the
   consensus times as the ground truth here, we minimize the desynchronization
   of clients and services due to system clock. Whenever time-based decisions
   are taken in this section, assume that they are consensus times and not
   system times.

   As [PUB-SHAREDRANDOM] specifies, consensuses contain two shared random
   values (the current one and the previous one). Hidden services and clients
   are asked to match these shared random values with descriptor time periods
   and use the right SRV when fetching/uploading descriptors. This section
   attempts to precisely specify how this works.

   Let's start with an illustration of the system:

      +------------------------------------------------------------------+
      |                                                                  |
      | 00:00      12:00       00:00       12:00       00:00       12:00 |
      | SRV#1      TP#1        SRV#2       TP#2        SRV#3       TP#3  |
      |                                                                  |
      |  $==========|-----------$===========|-----------$===========|    |
      |                                                                  |
      |                                                                  |
      +------------------------------------------------------------------+

                                      Legend: [TP#1 = Time Period #1]
                                              [SRV#1 = Shared Random Value #1]
                                              ["$" = descriptor rotation moment]

2.2.4.1. Client behavior for fetching descriptors [CLIENTFETCH]

   And here is how clients use TPs and SRVs to fetch descriptors:

   Clients always aim to synchronize their TP with SRV, so they always want to
   use TP#N with SRV#N: To achieve this wrt time periods, clients always use
   the current time period when fetching descriptors. Now wrt SRVs, if a client
   is in the time segment between a new time period and a new SRV (i.e. the
   segments drawn with "-") it uses the current SRV, else if the client is in a
   time segment between a new SRV and a new time period (i.e. the segments
   drawn with "="), it uses the previous SRV.

   Example:

   +------------------------------------------------------------------+
   |                                                                  |
   | 00:00      12:00       00:00       12:00       00:00       12:00 |
   | SRV#1      TP#1        SRV#2       TP#2        SRV#3       TP#3  |
   |                                                                  |
   |  $==========|-----------$===========|-----------$===========|    |
   |              ^           ^                                       |
   |              C1          C2                                      |
   +------------------------------------------------------------------+

   If a client (C1) is at 13:00 right after TP#1, then it will use TP#1 and
   SRV#1 for fetching descriptors. Also, if a client (C2) is at 01:00 right
   after SRV#2, it will still use TP#1 and SRV#1.

2.2.4.2. Service behavior for uploading descriptors [SERVICEUPLOAD]

   As discussed above, services maintain two active descriptors at any time. We
   call these the "first" and "second" service descriptors. Services rotate
   their descriptor everytime they receive a consensus with a valid_after time
   past the next SRV calculation time. They rotate their descriptors by
   discarding their first descriptor, pushing the second descriptor to the
   first, and rebuilding their second descriptor with the latest data.

   Services like clients also employ a different logic for picking SRV and TP
   values based on their position in the graph above. Here is the logic:

2.2.4.2.1. First descriptor upload logic [FIRSTDESCUPLOAD]

   Here is the service logic for uploading its first descriptor:

   When a service is in the time segment between a new time period a new SRV
   (i.e. the segments drawn with "-"), it uses the previous time period and
   previous SRV for uploading its first descriptor: that's meant to cover
   for clients that have a consensus that is still in the previous time period.

   Example: Consider in the above illustration that the service is at 13:00
   right after TP#1. It will upload its first descriptor using TP#0 and SRV#0.
   So if a client still has a 11:00 consensus it will be able to access it
   based on the client logic above.

   Now if a service is in the time segment between a new SRV and a new time
   period (i.e. the segments drawn with "=") it uses the current time period
   and the previous SRV for its first descriptor: that's meant to cover clients
   with an up-to-date consensus in the same time period as the service.

   Example:

   +------------------------------------------------------------------+
   |                                                                  |
   | 00:00      12:00       00:00       12:00       00:00       12:00 |
   | SRV#1      TP#1        SRV#2       TP#2        SRV#3       TP#3  |
   |                                                                  |
   |  $==========|-----------$===========|-----------$===========|    |
   |                          ^                                       |
   |                          S                                       |
   +------------------------------------------------------------------+

   Consider that the service is at 01:00 right after SRV#2: it will upload its
   first descriptor using TP#1 and SRV#1.

2.2.4.2.2. Second descriptor upload logic [SECONDDESCUPLOAD]

   Here is the service logic for uploading its second descriptor:

   When a service is in the time segment between a new time period a new SRV
   (i.e. the segments drawn with "-"), it uses the current time period and
   current SRV for uploading its second descriptor: that's meant to cover for
   clients that have an up-to-date consensus on the same TP as the service.

   Example: Consider in the above illustration that the service is at 13:00
   right after TP#1: it will upload its second descriptor using TP#1 and SRV#1.

   Now if a service is in the time segment between a new SRV and a new time
   period (i.e. the segments drawn with "=") it uses the next time period and
   the current SRV for its second descriptor: that's meant to cover clients
   with a newer consensus than the service (in the next time period).

   Example:

   +------------------------------------------------------------------+
   |                                                                  |
   | 00:00      12:00       00:00       12:00       00:00       12:00 |
   | SRV#1      TP#1        SRV#2       TP#2        SRV#3       TP#3  |
   |                                                                  |
   |  $==========|-----------$===========|-----------$===========|    |
   |                          ^                                       |
   |                          S                                       |
   +------------------------------------------------------------------+

   Consider that the service is at 01:00 right after SRV#2: it will upload its
   second descriptor using TP#2 and SRV#2.

2.2.5. Expiring hidden service descriptors [EXPIRE-DESC]

   Hidden services set their descriptor's "descriptor-lifetime" field to 180
   minutes (3 hours). Hidden services ensure that their descriptor will remain
   valid in the HSDir caches, by republishing their descriptors periodically as
   specified in [WHEN-HSDESC].

   Hidden services MUST also keep their introduction circuits alive for as long
   as descriptors including those intro points are valid (even if that's after
   the time period has changed).

2.2.6. URLs for anonymous uploading and downloading

   Hidden service descriptors conforming to this specification are uploaded
   with an HTTP POST request to the URL /tor/hs/<version>/publish relative to
   the hidden service directory's root, and downloaded with an HTTP GET
   request for the URL /tor/hs/<version>/<z> where <z> is a base64 encoding of
   the hidden service's blinded public key and <version> is the protocol
   version which is "3" in this case.

   These requests must be made anonymously, on circuits not used for
   anything else.

2.2.7. Client-side validation of onion addresses

   When a Tor client receives a prop224 onion address from the user, it
   MUST first validate the onion address before attempting to connect or
   fetch its descriptor. If the validation fails, the client MUST
   refuse to connect.

   As part of the address validation, Tor clients should check that the
   underlying ed25519 key does not have a torsion component. If Tor accepted
   ed25519 keys with torsion components, attackers could create multiple
   equivalent onion addresses for a single ed25519 key, which would map to the
   same service. We want to avoid that because it could lead to phishing
   attacks and surprising behaviors (e.g. imagine a browser plugin that blocks
   onion addresses, but could be bypassed using an equivalent onion address
   with a torsion component).

   The right way for clients to detect such fraudulent addresses (which should
   only occur malevolently and never natutally) is to extract the ed25519
   public key from the onion address and multiply it by the ed25519 group order
   and ensure that the result is the ed25519 identity element. For more
   details, please see [TORSION-REFS].

2.3. Publishing shared random values [PUB-SHAREDRANDOM]

   Our design for limiting the predictability of HSDir upload locations
   relies on a shared random value (SRV) that isn't predictable in advance or
   too influenceable by an attacker. The authorities must run a protocol
   to generate such a value at least once per hsdir period. Here we
   describe how they publish these values; the procedure they use to
   generate them can change independently of the rest of this
   specification. For more information see [SHAREDRANDOM-REFS].

   According to proposal 250, we add two new lines in consensuses:

     "shared-rand-previous-value" SP NUM_REVEALS SP VALUE NL
     "shared-rand-current-value" SP NUM_REVEALS SP VALUE NL

2.3.1. Client behavior in the absense of shared random values

   If the previous or current shared random value cannot be found in a
   consensus, then Tor clients and services need to generate their own random
   value for use when choosing HSDirs.

   To do so, Tor clients and services use:

     SRV = H("shared-random-disaster" | INT_8(period_length) | INT_8(period_num))

   where period_length is the length of a time period in minutes, period_num is
   calculated as specified in [TIME-PERIODS] for the wanted shared random value
   that could not be found originally.

2.3.2. Hidden services and changing shared random values

   It's theoretically possible that the consensus shared random values will
   change or disappear in the middle of a time period because of directory
   authorities dropping offline or misbehaving.

   To avoid client reachability issues in this rare event, hidden services
   should use the new shared random values to find the new responsible HSDirs
   and upload their descriptors there.

   XXX How long should they upload descriptors there for?

2.4. Hidden service descriptors: outer wrapper [DESC-OUTER]

   The format for a hidden service descriptor is as follows, using the
   meta-format from dir-spec.txt.

     "hs-descriptor" SP version-number NL

       [At start, exactly once.]

       The version-number is a 32 bit unsigned integer indicating the version
       of the descriptor. Current version is "3".

     "descriptor-lifetime" SP LifetimeMinutes NL

       [Exactly once]

       The lifetime of a descriptor in minutes. An HSDir SHOULD expire the
       hidden service descriptor at least LifetimeMinutes after it was
       uploaded.

       The LifetimeMinutes field can take values between 30 and 3000 (50 hours).

    "descriptor-signing-key-cert" NL certificate NL

       [Exactly once.]

       The 'certificate' field contains a certificate in the format from
       proposal 220, wrapped with "-----BEGIN ED25519 CERT-----".  The
       certificate cross-certifies the short-term descriptor signing key with
       the blinded public key.  The certificate type must be [08], and the
       blinded public key must be present as the signing-key extension.

     "revision-counter" SP Integer NL

       [Exactly once.]

       The revision number of the descriptor. If an HSDir receives a
       second descriptor for a key that it already has a descriptor for,
       it should retain and serve the descriptor with the higher
       revision-counter.

       (Checking for monotonically increasing revision-counter values
       prevents an attacker from replacing a newer descriptor signed by
       a given key with a copy of an older version.)

     "superencrypted" NL encrypted-string

       [Exactly once.]

       An encrypted blob, whose format is discussed in [HS-DESC-ENC] below. The
       blob is base64 encoded and enclosed in -----BEGIN MESSAGE---- and
       ----END MESSAGE---- wrappers.

     "signature" SP signature NL

       [exactly once, at end.]

       A signature of all previous fields, using the signing key in the
       descriptor-signing-key-cert line, prefixed by the string "Tor onion
       service descriptor sig v3". We use a separate key for signing, so that
       the hidden service host does not need to have its private blinded key
       online.

   HSDirs accept hidden service descriptors of up to 50k bytes (a consensus
   parameter should also be introduced to control this value).

2.5. Hidden service descriptors: encryption format [HS-DESC-ENC]

   Hidden service descriptors are protected by two layers of encryption.
   Clients need to decrypt both layers to connect to the hidden service.

   The first layer of encryption provides confidentiality against entities who
   don't know the public key of the hidden service (e.g. HSDirs), while the
   second layer of encryption is only useful when client authorization is enabled
   and protects against entities that do not possess valid client credentials.

2.5.1. First layer of encryption [HS-DESC-FIRST-LAYER]

   The first layer of HS descriptor encryption is designed to protect
   descriptor confidentiality against entities who don't know the blinded
   public key of the hidden service.

2.5.1.1. First layer encryption logic

   The encryption keys and format for the first layer of encryption are
   generated as specified in [HS-DESC-ENCRYPTION-KEYS] with customization
   parameters:

     SECRET_DATA = blinded-public-key
     STRING_CONSTANT = "hsdir-superencrypted-data"

   The ciphertext is placed on the "superencrypted" field of the descriptor.

   Before encryption the plaintext is padded with NUL bytes to the nearest
   multiple of 10k bytes.

2.5.1.2. First layer plaintext format

   After clients decrypt the first layer of encryption, they need to parse the
   plaintext to get to the second layer ciphertext which is contained in the
   "encrypted" field.

   If client auth is enabled, the hidden service generates a fresh
   descriptor_cookie key (32 random bytes) and encrypts it using each
   authorized client's identity x25519 key. Authorized clients can use the
   descriptor cookie to decrypt the second layer of encryption. Our encryption
   scheme requires the hidden service to also generate an ephemeral x25519
   keypair for each new descriptor.

   If client auth is disabled, fake data is placed in each of the fields below
   to obfuscate whether client authorization is enabled.

   Here are all the supported fields:

     "desc-auth-type" SP type NL

      [Exactly once]

      This field contains the type of authorization used to protect the
      descriptor. The only recognized type is "x25519" and specifies the
      encryption scheme described in this section.

      If client authorization is disabled, the value here should be "x25519".

     "desc-auth-ephemeral-key" SP key NL

      [Exactly once]

      This field contains an ephemeral x25519 public key generated by the
      hidden service and encoded in base64. The key is used by the encryption
      scheme below.

      If client authorization is disabled, the value here should be a fresh
      x25519 pubkey that will remain unused.

     "auth-client" SP client-id SP iv SP encrypted-cookie

      [Any number]

      When client authorization is enabled, the hidden service inserts an
      "auth-client" line for each of its authorized clients. If client
      authorization is disabled, the fields here can be populated with random
      data of the right size (that's 8 bytes for 'client-id', 16 bytes for 'iv'
      and 16 bytes for 'encrypted-cookie' all encoded with base64).

      When client authorization is enabled, each "auth-client" line contains
      the descriptor cookie encrypted to each individual client. We assume that
      each authorized client possesses a pre-shared x25519 keypair which is
      used to decrypt the descriptor cookie.

      We now describe the descriptor cookie encryption scheme. Here are the
      relevant keys:

          client_x = private x25519 key of authorized client
          client_X = public x25519 key of authorized client
          hs_y = private key of ephemeral x25519 keypair of hidden service
          hs_Y = public key of ephemeral x25519 keypair of hidden service
          descriptor_cookie = descriptor cookie used to encrypt the descriptor

      And here is what the hidden service computes:

          SECRET_SEED = x25519(hs_y, client_X)
          KEYS = KDF(SECRET_SEED, 40)
          CLIENT-ID = fist 8 bytes of KEYS
          COOKIE-KEY = last 32 bytes of KEYS

      Here is a description of the fields in the "auth-client" line:

      - The "client-id" field is CLIENT-ID from above encoded in base64.

      - The "iv" field is 16 random bytes encoded in base64.

      - The "encrypted-cookie" field contains the descriptor cookie ciphertext
        as follows and is encoded in base64:
           encrypted-cookie = STREAM(iv, COOKIE-KEY) XOR descriptor_cookie

      See section [FIRST-LAYER-CLIENT-BEHAVIOR] for the client-side logic of
      how to decrypt the descriptor cookie.

    "encrypted" NL encrypted-string

     [Exactly once]

      An encrypted blob containing the second layer ciphertext, whose format is
      discussed in [HS-DESC-SECOND-LAYER] below. The blob is base64 encoded
      and enclosed in -----BEGIN MESSAGE---- and ----END MESSAGE---- wrappers.

2.5.1.3. Client behavior [FIRST-LAYER-CLIENT-BEHAVIOR]

    The goal of clients at this stage is to decrypt the "encrypted" field as
    described in [HS-DESC-SECOND-LAYER].

    If client authorization is enabled, authorized clients need to extract the
    descriptor cookie to proceed with decryption of the second layer as
    follows:

    An authorized client parsing the first layer of an encrypted descriptor,
    extracts the ephemeral key from "desc-auth-ephemeral-key" and calculates
    CLIENT-ID and COOKIE-KEY as described in the section above using their
    x25519 private key. The client then uses CLIENT-ID to find the right
    "auth-client" field which contains the ciphertext of the descriptor
    cookie. The client then uses COOKIE-KEY and the iv to decrypt the
    descriptor_cookie, which is used to decrypt the second layer of descriptor
    encryption as described in [HS-DESC-SECOND-LAYER].

2.5.1.4. Hiding client authorization data

    Hidden services should avoid leaking whether client authorization is
    enabled or how many authorized clients there are.

    Hence even when client authorization is disabled, the hidden service adds
    fake "desc-auth-type", "desc-auth-ephemeral-key" and "auth-client" lines to
    the descriptor, as described in [HS-DESC-FIRST-LAYER].

    The hidden service also avoids leaking the number of authorized clients by
    adding fake "auth-client" entries to its descriptor. Specifically,
    descriptors always contain a number of authorized clients that is a
    multiple of 16 by adding fake "auth-client" entries if needed.
    [XXX consider randomization of the value 16]

    Clients MUST accept descriptors with any number of "auth-client" lines as
    long as the total descriptor size is within the max limit of 50k (also
    controlled with a consensus parameter).

2.5.2. Second layer of encryption [HS-DESC-SECOND-LAYER]

   The second layer of descriptor encryption is designed to protect descriptor
   confidentiality against unauthorized clients. If client authorization is
   enabled, it's encrypted using the descriptor_cookie, and contains needed
   information for connecting to the hidden service, like the list of its
   introduction points.

   If client authorization is disabled, then the second layer of HS encryption
   does not offer any additional security, but is still used.

2.5.2.1. Second layer encryption keys

   The encryption keys and format for the second layer of encryption are
   generated as specified in [HS-DESC-ENCRYPTION-KEYS] with customization
   parameters as follows:

     SECRET_DATA = blinded-public-key | descriptor_cookie
     STRING_CONSTANT = "hsdir-encrypted-data"

   If client authorization is disabled the 'descriptor_cookie' field is left blank.

   The ciphertext is placed on the "encrypted" field of the descriptor.

2.5.2.2. Second layer plaintext format

   After decrypting the second layer ciphertext, clients can finally learn the
   list of intro points etc. The plaintext has the following format:

     "create2-formats" SP formats NL

      [Exactly once]

      A space-separated list of integers denoting CREATE2 cell format numbers
      that the server recognizes. Must include at least ntor as described in
      tor-spec.txt. See tor-spec section 5.1 for a list of recognized
      handshake types.

     "intro-auth-required" SP types NL

      [At most once]

      A space-separated list of introduction-layer authentication types; see
      section [INTRO-AUTH] for more info. A client that does not support at
      least one of these authentication types will not be able to contact the
      host. Recognized types are: 'password' and 'ed25519'.

     "single-onion-service"

      [None or at most once]

      If present, this line indicates that the service is a Single Onion
      Service (see prop260 for more details about that type of service). This
      field has been introduced in 0.3.0 meaning 0.2.9 service don't include
      this.

     Followed by zero or more introduction points as follows (see section
     [NUM_INTRO_POINT] below for accepted values):

        "introduction-point" SP link-specifiers NL

          [Exactly once per introduction point at start of introduction
            point section]

          The link-specifiers is a base64 encoding of a link specifier
          block in the format described in BUILDING-BLOCKS.

        "onion-key" SP "ntor" SP key NL

          [Exactly once per introduction point]

          The key is a base64 encoded curve25519 public key which is the onion
          key of the introduction point Tor node used for the ntor handshake
          when a client extends to it.

        "auth-key" NL certificate NL

          [Exactly once per introduction point]

          The certificate is a proposal 220 certificate wrapped in
          "-----BEGIN ED25519 CERT-----", cross-certifying the descriptor
          signing key with the introduction point authentication key, which
          is included in the mandatory signing-key extension.  The certificate
          type must be [09].

        "enc-key" SP "ntor" SP key NL

          [Exactly once per introduction point]

          The key is a base64 encoded curve25519 public key used to encrypt
          the introduction request to service.

        "enc-key-cert" NL certificate NL

          [Exactly once per introduction point]

          Cross-certification of the descriptor signing key by the encryption
          key.

          For "ntor" keys, certificate is a proposal 220 certificate wrapped
          in "-----BEGIN ED25519 CERT-----" armor, cross-certifying the
          descriptor signing key with the ed25519 equivalent of a curve25519
          public encryption key derived using the process in proposal 228
          appendix A. The certificate type must be [0B], and the signing-key
          extension is mandatory.

        "legacy-key" NL key NL

          [None or at most once per introduction point]

          The key is an ASN.1 encoded RSA public key in PEM format used for a
          legacy introduction point as described in [LEGACY_EST_INTRO].

          This field is only present if the introduction point only supports
          legacy protocol (v2) that is <= 0.2.9 or the protocol version value
          "HSIntro 3".

        "legacy-key-cert NL certificate NL

          [None or at most once per introduction point]

          MUST be present if "legacy-key" is present.

          The certificate is a proposal 220 RSA->Ed cross-certificate wrapped
          in "-----BEGIN CROSSCERT-----" armor, cross-certifying the
          descriptor signing key with the RSA public key found in
          "legacy-key".

   To remain compatible with future revisions to the descriptor format,
   clients should ignore unrecognized lines in the descriptor.
   Other encryption and authentication key formats are allowed; clients
   should ignore ones they do not recognize.

   Clients who manage to extract the introduction points of the hidden service
   can prroceed with the introduction protocol as specified in [INTRO-PROTOCOL].

2.5.3. Deriving hidden service descriptor encryption keys [HS-DESC-ENCRYPTION-KEYS]

   In this section we present the generic encryption format for hidden service
   descriptors. We use the same encryption format in both encryption layers,
   hence we introduce two customization parameters SECRET_DATA and
   STRING_CONSTANT which vary between the layers.

   The SECRET_DATA parameter specifies the secret data that are used during
   encryption key generation, while STRING_CONSTANT is merely a string constant
   that is used as part of the KDF.

   Here is the key generation logic:

       SALT = 16 bytes from H(random), changes each time we rebuld the
              descriptor even if the content of the descriptor hasn't changed.
              (So that we don't leak whether the intro point list etc. changed)

       secret_input = SECRET_DATA | subcredential | INT_8(revision_counter)

       keys = KDF(secret_input | salt | STRING_CONSTANT, S_KEY_LEN + S_IV_LEN + MAC_KEY_LEN)

       SECRET_KEY = first S_KEY_LEN bytes of keys
       SECRET_IV  = next S_IV_LEN bytes of keys
       MAC_KEY    = last MAC_KEY_LEN bytes of keys

   The encrypted data has the format:

       SALT       hashed random bytes from above  [16 bytes]
       ENCRYPTED  The ciphertext                  [variable]
       MAC        MAC of both above fields        [32 bytes]

   The final encryption format is ENCRYPTED = STREAM(SECRET_IV,SECRET_KEY) XOR Plaintext

2.5.4. Number of introduction points [NUM_INTRO_POINT]

   This section defines how many introduction points an hidden service
   descriptor can have at minimum, by default and the maximum:

      Minimum: 0 - Default: 3 - Maximum: 20

   A value of 0 would means that the service is still alive but doesn't want
   to be reached by any client at the moment. Note that the descriptor size
   increases considerably as more introduction points are added.

   The reason for a maximum value of 20 is to give enough scalability to tools
   like OnionBalance to be able to load balance up to 120 servers (20 x 6
   HSDirs) but also in order for the descriptor size to not overwhelmed hidden
   service directories with user defined values that could be gigantic.

3. The introduction protocol [INTRO-PROTOCOL]

   The introduction protocol proceeds in three steps.

   First, a hidden service host builds an anonymous circuit to a Tor
   node and registers that circuit as an introduction point.

        [After 'First' and before 'Second', the hidden service publishes its
        introduction points and associated keys, and the client fetches
        them as described in section [HSDIR] above.]

   Second, a client builds an anonymous circuit to the introduction
   point, and sends an introduction request.

   Third, the introduction point relays the introduction request along
   the introduction circuit to the hidden service host, and acknowledges
   the introduction request to the client.

3.1. Registering an introduction point [REG_INTRO_POINT]

3.1.1. Extensible ESTABLISH_INTRO protocol. [EST_INTRO]

   When a hidden service is establishing a new introduction point, it
   sends an ESTABLISH_INTRO cell with the following contents:

     AUTH_KEY_TYPE    [1 byte]
     AUTH_KEY_LEN     [2 bytes]
     AUTH_KEY         [AUTH_KEY_LEN bytes]
     N_EXTENSIONS     [1 byte]
     N_EXTENSIONS times:
        EXT_FIELD_TYPE [1 byte]
        EXT_FIELD_LEN  [1 byte]
        EXT_FIELD      [EXT_FIELD_LEN bytes]
     HANDSHAKE_AUTH   [MAC_LEN bytes]
     SIG_LEN          [2 bytes]
     SIG              [SIG_LEN bytes]

   The AUTH_KEY_TYPE field indicates the type of the introduction point
   authentication key and the type of the MAC to use in
   HANDSHAKE_AUTH. Recognized types are:

       [00, 01] -- Reserved for legacy introduction cells; see
                   [LEGACY_EST_INTRO below]
       [02] -- Ed25519; SHA3-256.

   The AUTH_KEY_LEN field determines the length of the AUTH_KEY
   field. The AUTH_KEY field contains the public introduction point
   authentication key.

   The EXT_FIELD_TYPE, EXT_FIELD_LEN, EXT_FIELD entries are reserved for
   future extensions to the introduction protocol. Extensions with
   unrecognized EXT_FIELD_TYPE values must be ignored.

   The HANDSHAKE_AUTH field contains the MAC of all earlier fields in
   the cell using as its key the shared per-circuit material ("KH")
   generated during the circuit extension protocol; see tor-spec.txt
   section 5.2, "Setting circuit keys". It prevents replays of
   ESTABLISH_INTRO cells.

   SIG_LEN is the length of the signature.

   SIG is a signature, using AUTH_KEY, of all contents of the cell, up
   to but not including SIG. These contents are prefixed with the string
   "Tor establish-intro cell v1".

   Upon receiving an ESTABLISH_INTRO cell, a Tor node first decodes the
   key and the signature, and checks the signature. The node must reject
   the ESTABLISH_INTRO cell and destroy the circuit in these cases:

        * If the key type is unrecognized
        * If the key is ill-formatted
        * If the signature is incorrect
        * If the HANDSHAKE_AUTH value is incorrect

        * If the circuit is already a rendezvous circuit.
        * If the circuit is already an introduction circuit.
          [TODO: some scalability designs fail there.]
        * If the key is already in use by another circuit.

   Otherwise, the node must associate the key with the circuit, for use
   later in INTRODUCE1 cells.

3.1.2. Registering an introduction point on a legacy Tor node
       [LEGACY_EST_INTRO]

   Tor nodes should also support an older version of the ESTABLISH_INTRO
   cell, first documented in rend-spec.txt. New hidden service hosts
   must use this format when establishing introduction points at older
   Tor nodes that do not support the format above in [EST_INTRO].

   In this older protocol, an ESTABLISH_INTRO cell contains:

        KEY_LEN        [2 bytes]
        KEY            [KEY_LEN bytes]
        HANDSHAKE_AUTH [20 bytes]
        SIG            [variable, up to end of relay payload]

   The KEY_LEN variable determines the length of the KEY field.

   The KEY field is the ASN1-encoded legacy RSA public key that was also
   included in the hidden service descriptor.

   The HANDSHAKE_AUTH field contains the SHA1 digest of (KH | "INTRODUCE").

   The SIG field contains an RSA signature, using PKCS1 padding, of all
   earlier fields.

   Older versions of Tor always use a 1024-bit RSA key for these introduction
   authentication keys.

3.1.3. Acknowledging establishment of introduction point [INTRO_ESTABLISHED]

   After setting up an introduction circuit, the introduction point reports its
   status back to the hidden service host with an INTRO_ESTABLISHED cell.

   The INTRO_ESTABLISHED cell has the following contents:

     N_EXTENSIONS [1 byte]
     N_EXTENSIONS times:
       EXT_FIELD_TYPE [1 byte]
       EXT_FIELD_LEN  [1 byte]
       EXT_FIELD      [EXT_FIELD_LEN bytes]

   Older versions of Tor send back an empty INTRO_ESTABLISHED cell instead.
   Services must accept an empty INTRO_ESTABLISHED cell from a legacy relay.

3.2. Sending an INTRODUCE1 cell to the introduction point. [SEND_INTRO1]

   In order to participate in the introduction protocol, a client must
   know the following:

     * An introduction point for a service.
     * The introduction authentication key for that introduction point.
     * The introduction encryption key for that introduction point.

   The client sends an INTRODUCE1 cell to the introduction point,
   containing an identifier for the service, an identifier for the
   encryption key that the client intends to use, and an opaque blob to
   be relayed to the hidden service host.

   In reply, the introduction point sends an INTRODUCE_ACK cell back to
   the client, either informing it that its request has been delivered,
   or that its request will not succeed.

   [TODO: specify what tor should do when receiving a malformed cell. Drop it?
          Kill circuit? This goes for all possible cells.]

3.2.1. INTRODUCE1 cell format [FMT_INTRO1]

   When a client is connecting to an introduction point, INTRODUCE1 cells
   should be of the form:

     LEGACY_KEY_ID   [20 bytes]
     AUTH_KEY_TYPE   [1 byte]
     AUTH_KEY_LEN    [2 bytes]
     AUTH_KEY        [AUTH_KEY_LEN bytes]
     N_EXTENSIONS    [1 byte]
     N_EXTENSIONS times:
       EXT_FIELD_TYPE [1 byte]
       EXT_FIELD_LEN  [1 byte]
       EXT_FIELD      [EXT_FIELD_LEN bytes]
     ENCRYPTED        [Up to end of relay payload]

   AUTH_KEY_TYPE is defined as in [EST_INTRO]. Currently, the only value of
   AUTH_KEY_TYPE for this cell is an Ed25519 public key [02].

   The LEGACY_KEY_ID field is used to distinguish between legacy and new style
   INTRODUCE1 cells. In new style INTRODUCE1 cells, LEGACY_KEY_ID is 20 zero
   bytes. Upon receiving an INTRODUCE1 cell, the introduction point checks the
   LEGACY_KEY_ID field. If LEGACY_KEY_ID is non-zero, the INTRODUCE1 cell
   should be handled as a legacy INTRODUCE1 cell by the intro point.

   Upon receiving a INTRODUCE1 cell, the introduction point checks
   whether AUTH_KEY matches the introduction point authentication key for an
   active introduction circuit.  If so, the introduction point sends an
   INTRODUCE2 cell with exactly the same contents to the service, and sends an
   INTRODUCE_ACK response to the client.

3.2.2. INTRODUCE_ACK cell format. [INTRO_ACK]

   An INTRODUCE_ACK cell has the following fields:

     STATUS       [2 bytes]
     N_EXTENSIONS [1 bytes]
     N_EXTENSIONS times:
       EXT_FIELD_TYPE [1 byte]
       EXT_FIELD_LEN  [1 byte]
       EXT_FIELD      [EXT_FIELD_LEN bytes]

   Recognized status values are:
     [00 00] -- Success: cell relayed to hidden service host.
     [00 01] -- Failure: service ID not recognized
     [00 02] -- Bad message format
     [00 03] -- Can't relay cell to service

3.3. Processing an INTRODUCE2 cell at the hidden service. [PROCESS_INTRO2]

   Upon receiving an INTRODUCE2 cell, the hidden service host checks whether
   the AUTH_KEY or LEGACY_KEY_ID field matches the keys for this
   introduction circuit.

   The service host then checks whether it has received a cell with these
   contents or rendezvous cookie before. If it has, it silently drops it as a
   replay. (It must maintain a replay cache for as long as it accepts cells
   with the same encryption key. Note that the encryption format below should
   be non-malleable.)

   If the cell is not a replay, it decrypts the ENCRYPTED field,
   establishes a shared key with the client, and authenticates the whole
   contents of the cell as having been unmodified since they left the
   client. There may be multiple ways of decrypting the ENCRYPTED field,
   depending on the chosen type of the encryption key. Requirements for
   an introduction handshake protocol are described in
   [INTRO-HANDSHAKE-REQS]. We specify one below in section
   [NTOR-WITH-EXTRA-DATA].

   The decrypted plaintext must have the form:

      RENDEZVOUS_COOKIE                          [20 bytes]
      N_EXTENSIONS                               [1 byte]
      N_EXTENSIONS times:
          EXT_FIELD_TYPE                         [1 byte]
          EXT_FIELD_LEN                          [1 byte]
          EXT_FIELD                              [EXT_FIELD_LEN bytes]
      ONION_KEY_TYPE                             [1 bytes]
      ONION_KEY_LEN                              [2 bytes]
      ONION_KEY                                  [ONION_KEY_LEN bytes]
      NSPEC      (Number of link specifiers)     [1 byte]
      NSPEC times:
          LSTYPE (Link specifier type)           [1 byte]
          LSLEN  (Link specifier length)         [1 byte]
          LSPEC  (Link specifier)                [LSLEN bytes]
      PAD        (optional padding)              [up to end of plaintext]

   Upon processing this plaintext, the hidden service makes sure that
   any required authentication is present in the extension fields, and
   then extends a rendezvous circuit to the node described in the LSPEC
   fields, using the ONION_KEY to complete the extension. As mentioned
   in [BUILDING-BLOCKS], the "TLS-over-TCP, IPv4" and "Legacy node
   identity" specifiers must be present.

   The hidden service SHOULD NOT reject any LSTYPE fields which it
   doesn't recognize; instead, it should use them verbatim in its EXTEND
   request to the rendezvous point.

   The ONION_KEY_TYPE field is:

      [01] NTOR:          ONION_KEY is 32 bytes long.

   The ONION_KEY field describes the onion key that must be used when
   extending to the rendezvous point. It must be of a type listed as
   supported in the hidden service descriptor.

   When using a legacy introduction point, the INTRODUCE cells must be padded
   to a certain length using the PAD field in the encrypted portion.

   Upon receiving a well-formed INTRODUCE2 cell, the hidden service host
   will have:

     * The information needed to connect to the client's chosen
       rendezvous point.
     * The second half of a handshake to authenticate and establish a
       shared key with the hidden service client.
     * A set of shared keys to use for end-to-end encryption.

3.3.1. Introduction handshake encryption requirements [INTRO-HANDSHAKE-REQS]

   When decoding the encrypted information in an INTRODUCE2 cell, a
   hidden service host must be able to:

     * Decrypt additional information included in the INTRODUCE2 cell,
       to include the rendezvous token and the information needed to
       extend to the rendezvous point.

     * Establish a set of shared keys for use with the client.

     * Authenticate that the cell has not been modified since the client
       generated it.

   Note that the old TAP-derived protocol of the previous hidden service
   design achieved the first two requirements, but not the third.

3.3.2. Example encryption handshake: ntor with extra data
       [NTOR-WITH-EXTRA-DATA]

   [TODO: relocate this]

   This is a variant of the ntor handshake (see tor-spec.txt, section
   5.1.4; see proposal 216; and see "Anonymity and one-way
   authentication in key-exchange protocols" by Goldberg, Stebila, and
   Ustaoglu).

   It behaves the same as the ntor handshake, except that, in addition
   to negotiating forward secure keys, it also provides a means for
   encrypting non-forward-secure data to the server (in this case, to
   the hidden service host) as part of the handshake.

   Notation here is as in section 5.1.4 of tor-spec.txt, which defines
   the ntor handshake.

   The PROTOID for this variant is "tor-hs-ntor-curve25519-sha3-256-1".
   We also use the following tweak values:

      t_hsenc    = PROTOID | ":hs_key_extract"
      t_hsverify = PROTOID | ":hs_verify"
      t_hsmac    = PROTOID | ":hs_mac"
      m_hsexpand = PROTOID | ":hs_key_expand"

   To make an INTRODUCE1 cell, the client must know a public encryption
   key B for the hidden service on this introduction circuit. The client
   generates a single-use keypair:
             x,X = KEYGEN()
   and computes:
             intro_secret_hs_input = EXP(B,x) | AUTH_KEY | X | B | PROTOID
             info = m_hsexpand | subcredential
             hs_keys = KDF(intro_secret_hs_input | t_hsenc | info, S_KEY_LEN+MAC_LEN)
             ENC_KEY = hs_keys[0:S_KEY_LEN]
             MAC_KEY = hs_keys[S_KEY_LEN:S_KEY_LEN+MAC_KEY_LEN]

   and sends, as the ENCRYPTED part of the INTRODUCE1 cell:

          CLIENT_PK                [PK_PUBKEY_LEN bytes]
          ENCRYPTED_DATA           [Padded to length of plaintext]
          MAC                      [MAC_LEN bytes]


   Substituting those fields into the INTRODUCE1 cell body format
   described in [FMT_INTRO1] above, we have

            LEGACY_KEY_ID               [20 bytes]
            AUTH_KEY_TYPE               [1 byte]
            AUTH_KEY_LEN                [2 bytes]
            AUTH_KEY                    [AUTH_KEY_LEN bytes]
            N_EXTENSIONS                [1 bytes]
            N_EXTENSIONS times:
               EXT_FIELD_TYPE           [1 byte]
               EXT_FIELD_LEN            [1 byte]
               EXT_FIELD                [EXT_FIELD_LEN bytes]
            ENCRYPTED:
               CLIENT_PK                [PK_PUBKEY_LEN bytes]
               ENCRYPTED_DATA           [Padded to length of plaintext]
               MAC                      [MAC_LEN bytes]


   (This format is as documented in [FMT_INTRO1] above, except that here
   we describe how to build the ENCRYPTED portion.)

   Here, the encryption key plays the role of B in the regular ntor
   handshake, and the AUTH_KEY field plays the role of the node ID.
   The CLIENT_PK field is the public key X. The ENCRYPTED_DATA field is
   the message plaintext, encrypted with the symmetric key ENC_KEY. The
   MAC field is a MAC of all of the cell from the AUTH_KEY through the
   end of ENCRYPTED_DATA, using the MAC_KEY value as its key.

   To process this format, the hidden service checks PK_VALID(CLIENT_PK)
   as necessary, and then computes ENC_KEY and MAC_KEY as the client did
   above, except using EXP(CLIENT_PK,b) in the calculation of
   intro_secret_hs_input. The service host then checks whether the MAC is
   correct. If it is invalid, it drops the cell. Otherwise, it computes
   the plaintext by decrypting ENCRYPTED_DATA.

   The hidden service host now completes the service side of the
   extended ntor handshake, as described in tor-spec.txt section 5.1.4,
   with the modified PROTOID as given above. To be explicit, the hidden
   service host generates a keypair of y,Y = KEYGEN(), and uses its
   introduction point encryption key 'b' to computes:

      intro_secret_hs_input = EXP(X,b) | AUTH_KEY | X | B | PROTOID
      info = m_hsexpand | subcredential
      hs_keys = KDF(intro_secret_hs_input | t_hsenc | info, S_KEY_LEN+MAC_LEN)
      HS_DEC_KEY = hs_keys[0:S_KEY_LEN]
      HS_MAC_KEY = hs_keys[S_KEY_LEN:S_KEY_LEN+MAC_KEY_LEN]

      (The above are used to check the MAC and then decrypt the
      encrypted data.)

      rend_secret_hs_input = EXP(X,y) | EXP(X,b) | AUTH_KEY | B | X | Y | PROTOID
      NTOR_KEY_SEED = MAC(rend_secret_hs_input, t_hsenc)
      verify = MAC(rend_secret_hs_input, t_hsverify)
      auth_input = verify | AUTH_KEY | B | Y | X | PROTOID | "Server"
      AUTH_INPUT_MAC = MAC(auth_input, t_hsmac)

      (The above are used to finish the ntor handshake.)

   The server's handshake reply is:
       SERVER_PK   Y                         [PK_PUBKEY_LEN bytes]
       AUTH        AUTH_INPUT_MAC            [MAC_LEN bytes]

   These fields will be sent to the client in a RENDEZVOUS1 cell using the
   HANDSHAKE_INFO element (see [JOIN_REND]).

   The hidden service host now also knows the keys generated by the
   handshake, which it will use to encrypt and authenticate data
   end-to-end between the client and the server. These keys are as
   computed in tor-spec.txt section 5.1.4.

3.4. Authentication during the introduction phase. [INTRO-AUTH]

   Hidden services may restrict access only to authorized users.
   One mechanism to do so is the credential mechanism, where only users who
   know the credential for a hidden service may connect at all.

3.4.1. Ed25519-based authentication.

   To authenticate with an Ed25519 private key, the user must include an
   extension field in the encrypted part of the INTRODUCE1 cell with an
   EXT_FIELD_TYPE type of [02] and the contents:

        Nonce     [16 bytes]
        Pubkey    [32 bytes]
        Signature [64 bytes]

   Nonce is a random value. Pubkey is the public key that will be used
   to authenticate. [TODO: should this be an identifier for the public
   key instead?]  Signature is the signature, using Ed25519, of:

        "hidserv-userauth-ed25519"
        Nonce       (same as above)
        Pubkey      (same as above)
        AUTH_KEY    (As in the INTRODUCE1 cell)

   The hidden service host checks this by seeing whether it recognizes
   and would accept a signature from the provided public key. If it
   would, then it checks whether the signature is correct. If it is,
   then the correct user has authenticated.

   Replay prevention on the whole cell is sufficient to prevent replays
   on the authentication.

   Users SHOULD NOT use the same public key with multiple hidden
   services.

4. The rendezvous protocol

   Before connecting to a hidden service, the client first builds a
   circuit to an arbitrarily chosen Tor node (known as the rendezvous
   point), and sends an ESTABLISH_RENDEZVOUS cell. The hidden service
   later connects to the same node and sends a RENDEZVOUS cell. Once
   this has occurred, the relay forwards the contents of the RENDEZVOUS
   cell to the client, and joins the two circuits together.

4.1. Establishing a rendezvous point [EST_REND_POINT]

   The client sends the rendezvous point a RELAY_COMMAND_ESTABLISH_RENDEZVOUS
   cell containing a 20-byte value.

            RENDEZVOUS_COOKIE         [20 bytes]

   Rendezvous points MUST ignore any extra bytes in an
   ESTABLISH_RENDEZVOUS cell. (Older versions of Tor did not.)

   The rendezvous cookie is an arbitrary 20-byte value, chosen randomly
   by the client. The client SHOULD choose a new rendezvous cookie for
   each new connection attempt. If the rendezvous cookie is already in
   use on an existing circuit, the rendezvous point should reject it and
   destroy the circuit.

   Upon receiving an ESTABLISH_RENDEZVOUS cell, the rendezvous point associates
   the cookie with the circuit on which it was sent. It replies to the client
   with an empty RENDEZVOUS_ESTABLISHED cell to indicate success. Clients MUST
   ignore any extra bytes in a RENDEZVOUS_ESTABLISHED cell.

   The client MUST NOT use the circuit which sent the cell for any
   purpose other than rendezvous with the given location-hidden service.

   The client should establish a rendezvous point BEFORE trying to
   connect to a hidden service.

4.2. Joining to a rendezvous point [JOIN_REND]

   To complete a rendezvous, the hidden service host builds a circuit to
   the rendezvous point and sends a RENDEZVOUS1 cell containing:

       RENDEZVOUS_COOKIE          [20 bytes]
       HANDSHAKE_INFO             [variable; depends on handshake type
                                   used.]

   where RENDEZVOUS_COOKIE is the cookie suggested by the client during the
   introduction (see [PROCESS_INTRO2]) and HANDSHAKE_INFO is defined in
   [NTOR-WITH-EXTRA-DATA].

   If the cookie matches the rendezvous cookie set on any
   not-yet-connected circuit on the rendezvous point, the rendezvous
   point connects the two circuits, and sends a RENDEZVOUS2 cell to the
   client containing the HANDSHAKE_INFO field of the RENDEZVOUS1 cell.

   Upon receiving the RENDEZVOUS2 cell, the client verifies that HANDSHAKE_INFO
   correctly completes a handshake. To do so, the client parses SERVER_PK from
   HANDSHAKE_INFO and reverses the final operations of section
   [NTOR-WITH-EXTRA-DATA] as shown here:

      rend_secret_hs_input = EXP(Y,x) | EXP(B,x) | AUTH_KEY | B | X | Y | PROTOID
      NTOR_KEY_SEED = MAC(ntor_secret_input, t_hsenc)
      verify = MAC(ntor_secret_input, t_hsverify)
      auth_input = verify | AUTH_KEY | B | Y | X | PROTOID | "Server"
      AUTH_INPUT_MAC = MAC(auth_input, t_hsmac)

   Finally the client verifies that the received AUTH field of HANDSHAKE_INFO
   is equal to the computed AUTH_INPUT_MAC.

   Now both parties use the handshake output to derive shared keys for use on
   the circuit as specified in the section below:

4.2.1. Key expansion

   The hidden service and its client need to derive crypto keys from the
   NTOR_KEY_SEED part of the handshake output. To do so, they use the KDF
   construction as follows:

       K = KDF(NTOR_KEY_SEED | m_hsexpand,    HASH_LEN * 2 + S_KEY_LEN * 2)

   The first HASH_LEN bytes of K form the forward digest Df; the next HASH_LEN
   bytes form the backward digest Db; the next S_KEY_LEN bytes form Kf, and the
   final S_KEY_LEN bytes form Kb.  Excess bytes from K are discarded.

   Subsequently, the rendezvous point passes relay cells, unchanged, from each
   of the two circuits to the other.  When Alice's OP sends RELAY cells along
   the circuit, it authenticates with Df, and encrypts them with the Kf, then
   with all of the keys for the ORs in Alice's side of the circuit; and when
   Alice's OP receives RELAY cells from the circuit, it decrypts them with the
   keys for the ORs in Alice's side of the circuit, then decrypts them with Kb,
   and checks integrity with Db.  Bob's OP does the same, with Kf and Kb
   interchanged.

   [TODO: Should we encrypt HANDSHAKE_INFO as we did INTRODUCE2
   contents? It's not necessary, but it could be wise. Similarly, we
   should make it extensible.]

4.3. Using legacy hosts as rendezvous points

   The behavior of ESTABLISH_RENDEZVOUS is unchanged from older versions
   of this protocol, except that relays should now ignore unexpected
   bytes at the end.

   Old versions of Tor required that RENDEZVOUS cell payloads be exactly
   168 bytes long. All shorter rendezvous payloads should be padded to
   this length with random bytes, to make them difficult to distinguish from
   older protocols at the rendezvous point.

   Relays older than 0.2.9.1 should not be used for rendezvous points by next
   generation onion services because they enforce too-strict length checks to
   rendezvous cells. Hence the "HSRend" protocol from proposal#264 should be
   used to select relays for rendezvous points.

5. Encrypting data between client and host

   A successfully completed handshake, as embedded in the
   INTRODUCE/RENDEZVOUS cells, gives the client and hidden service host
   a shared set of keys Kf, Kb, Df, Db, which they use for sending
   end-to-end traffic encryption and authentication as in the regular
   Tor relay encryption protocol, applying encryption with these keys
   before other encryption, and decrypting with these keys before other
   decryption. The client encrypts with Kf and decrypts with Kb; the
   service host does the opposite.

6. Encoding onion addresses [ONIONADDRESS]

   The onion address of a hidden service includes its identity public key, a
   version field and a basic checksum. All this information is then base32
   encoded as shown below:

     onion_address = base32(PUBKEY | CHECKSUM | VERSION) + ".onion"
     CHECKSUM = H(".onion checksum" | PUBKEY | VERSION)[:2]

     where:
       - PUBKEY is the 32 bytes ed25519 master pubkey of the hidden service.
       - VERSION is an one byte version field (default value '\x03')
       - ".onion checksum" is a constant string
       - CHECKSUM is truncated to two bytes before inserting it in onion_address

  Here are a few example addresses:

       pg6mmjiyjmcrsslvykfwnntlaru7p5svn6y2ymmju6nubxndf4pscryd.onion
       sp3k262uwy4r2k3ycr5awluarykdpag6a7y33jxop4cs2lu5uz5sseqd.onion
       xa4r2iadxm55fbnqgwwi5mymqdcofiu3w6rpbtqn7b2dyn7mgwj64jyd.onion

   For more information about this encoding, please see our discussion thread
   at [ONIONADDRESS-REFS].

7. Open Questions:

   Scaling hidden services is hard. There are on-going discussions that
   you might be able to help with. See [SCALING-REFS].

   How can we improve the HSDir unpredictability design proposed in
   [SHAREDRANDOM]? See [SHAREDRANDOM-REFS] for discussion.

   How can hidden service addresses become memorable while retaining
   their self-authenticating and decentralized nature? See
   [HUMANE-HSADDRESSES-REFS] for some proposals; many more are possible.

   Hidden Services are pretty slow. Both because of the lengthy setup
   procedure and because the final circuit has 6 hops. How can we make
   the Hidden Service protocol faster? See [PERFORMANCE-REFS] for some
   suggestions.

References:

[KEYBLIND-REFS]:
        https://trac.torproject.org/projects/tor/ticket/8106
        https://lists.torproject.org/pipermail/tor-dev/2012-September/004026.html

[KEYBLIND-PROOF]:
        https://lists.torproject.org/pipermail/tor-dev/2013-December/005943.html

[SHAREDRANDOM-REFS]:
        https://gitweb.torproject.org/torspec.git/tree/proposals/250-commit-reveal-consensus.txt
        https://trac.torproject.org/projects/tor/ticket/8244

[SCALING-REFS]:
        https://lists.torproject.org/pipermail/tor-dev/2013-October/005556.html

[HUMANE-HSADDRESSES-REFS]:
        https://gitweb.torproject.org/torspec.git/blob/HEAD:/proposals/ideas/xxx-onion-nyms.txt
        http://archives.seul.org/or/dev/Dec-2011/msg00034.html

[PERFORMANCE-REFS]:
        "Improving Efficiency and Simplicity of Tor circuit
        establishment and hidden services" by Overlier, L., and
        P. Syverson

        [TODO: Need more here! Do we have any? :( ]

[ATTACK-REFS]:
        "Trawling for Tor Hidden Services: Detection, Measurement,
        Deanonymization" by Alex Biryukov, Ivan Pustogarov,
        Ralf-Philipp Weinmann

        "Locating Hidden Servers" by Lasse Øverlier and Paul
        Syverson

[ED25519-REFS]:
        "High-speed high-security signatures" by Daniel
        J. Bernstein, Niels Duif, Tanja Lange, Peter Schwabe, and
        Bo-Yin Yang. http://cr.yp.to/papers.html#ed25519

[ED25519-B-REF]:
        https://tools.ietf.org/html/draft-josefsson-eddsa-ed25519-03#section-5:

[PRNG-REFS]:
        http://projectbullrun.org/dual-ec/ext-rand.html
        https://lists.torproject.org/pipermail/tor-dev/2015-November/009954.html

[SRV-TP-REFS]:
        https://lists.torproject.org/pipermail/tor-dev/2016-April/010759.html

[VANITY-REFS]:
        https://github.com/Yawning/horse25519

[ONIONADDRESS-REFS]:
        https://lists.torproject.org/pipermail/tor-dev/2017-January/011816.html

[TORSION-REFS]:
        https://lists.torproject.org/pipermail/tor-dev/2017-April/012164.html
        https://getmonero.org/2017/05/17/disclosure-of-a-major-bug-in-cryptonote-based-currencies.html

Appendix A. Signature scheme with key blinding [KEYBLIND]

A.1. Key derivation overview

  As described in [IMD:DIST] and [SUBCRED] above, we require a "key
  blinding" system that works (roughly) as follows:

        There is a master keypair (sk, pk).

        Given the keypair and a nonce n, there is a derivation function
        that gives a new blinded keypair (sk_n, pk_n).  This keypair can
        be used for signing.

        Given only the public key and the nonce, there is a function
        that gives pk_n.

        Without knowing pk, it is not possible to derive pk_n; without
        knowing sk, it is not possible to derive sk_n.

        It's possible to check that a signature was made with sk_n while
        knowing only pk_n.

        Someone who sees a large number of blinded public keys and
        signatures made using those public keys can't tell which
        signatures and which blinded keys were derived from the same
        master keypair.

        You can't forge signatures.

        [TODO: Insert a more rigorous definition and better references.]

A.2. Tor's key derivation scheme

  We propose the following scheme for key blinding, based on Ed25519.

  (This is an ECC group, so remember that scalar multiplication is the
  trapdoor function, and it's defined in terms of iterated point
  addition. See the Ed25519 paper [Reference ED25519-REFS] for a fairly
  clear writeup.)

  Let B be the ed25519 basepoint as found in section 5 of [ED25519-B-REF]:
      B = (15112221349535400772501151409588531511454012693041857206046113283949847762202,
           46316835694926478169428394003475163141307993866256225615783033603165251855960)

  Assume B has prime order l, so lB=0. Let a master keypair be written as
  (a,A), where a is the private key and A is the public key (A=aB).

  To derive the key for a nonce N and an optional secret s, compute the
  blinding factor like this:

           h = H(BLIND_STRING | A | s | B | N)
           BLIND_STRING = "Derive temporary signing key"
           N = "key-blind" | INT_8(period-number) | INT_8(period_length)

  then clamp the blinding factor 'h' according to the ed25519 spec:

           h[0] &= 248;
           h[31] &= 127;
           h[31] |= 64;

  and do the key derivation as follows:

      private key for the period:   a' = h a
      public key for the period:    A' = h A = (ha)B

  Generating a signature of M: given a deterministic random-looking r
  (see EdDSA paper), take R=rB, S=r+hash(R,A',M)ah mod l. Send signature
  (R,S) and public key A'.

  Verifying the signature: Check whether SB = R+hash(R,A',M)A'.

  (If the signature is valid,
       SB = (r + hash(R,A',M)ah)B
          = rB + (hash(R,A',M)ah)B
          = R + hash(R,A',M)A' )

  See [KEYBLIND-REFS] for an extensive discussion on this scheme and
  possible alternatives. Also, see [KEYBLIND-PROOF] for a security
  proof of this scheme.

Appendix B. Selecting nodes [PICKNODES]

  Picking introduction points
  Picking rendezvous points
  Building paths
  Reusing circuits

  (TODO: This needs a writeup)

Appendix C. Recommendations for searching for vanity .onions [VANITY]

  EDITORIAL NOTE: The author thinks that it's silly to brute-force the
  keyspace for a key that, when base-32 encoded, spells out the name of
  your website. It also feels a bit dangerous to me. If you train your
  users to connect to

      llamanymityx4fi3l6x2gyzmtmgxjyqyorj9qsb5r543izcwymle.onion

  I worry that you're making it easier for somebody to trick them into
  connecting to

      llamanymityb4sqi0ta0tsw6uovyhwlezkcrmczeuzdvfauuemle.onion

  Nevertheless, people are probably going to try to do this, so here's a
  decent algorithm to use.

  To search for a public key with some criterion X:

        Generate a random (sk,pk) pair.

        While pk does not satisfy X:

            Add the number 8 to sk
            Add the scalar 8*B to pk

        Return sk, pk.

  We add 8 and 8*B, rather than 1 and B, so that sk is always a valid
  Curve25519 private key, with the lowest 3 bits equal to 0.

  This algorithm is safe [source: djb, personal communication] [TODO:
  Make sure I understood correctly!] so long as only the final (sk,pk)
  pair is used, and all previous values are discarded.

  To parallelize this algorithm, start with an independent (sk,pk) pair
  generated for each independent thread, and let each search proceed
  independently.

  See [VANITY-REFS] for a reference implementation of this vanity .onion
  search scheme.

Appendix D. Numeric values reserved in this document

  [TODO: collect all the lists of commands and values mentioned above]

Appendix E. Reserved numbers

  We reserve these certificate type values for Ed25519 certificates:

      [08] short-term descriptor signing key, signed with blinded
           public key. (Section 2.4)
      [09] intro point authentication key, cross-certifying the descriptor
           signing key. (Section 2.5)
      [0B] ed25519 key derived from the curve25519 intro point encryption key,
           cross-certifying the descriptor signing key. (Section 2.5)

      Note: The value "0A" is skipped because it's reserved for the onion key
            cross-certifying ntor identity key from proposal 228.

Appendix F. Hidden service directory format [HIDSERVDIR-FORMAT]

  This appendix section specifies the contents of the HiddenServiceDir directory:

  - "hostname"                                       [FILE]

   This file contains the onion address of the onion service.

  - "private_key_ed25519"                            [FILE]

   This file contains the private master ed25519 key of the onion service.
   [TODO: Offline keys]

  - "client_authorized_pubkeys"                      [FILE]

   If client authorization is _enabled_, this is a newline-separated file of
   "<client name> <pubkeys> entries for authorized clients. You can think of it
   as the ~/.ssh/authorized_keys of onion services. See [CLIENT-AUTH-MGMT] for
   more details.

  - "./client_authorized_privkeys/"                  [DIRECTORY]
    "./client_authorized_privkeys/alice.privkey"     [FILE]
    "./client_authorized_privkeys/bob.privkey"       [FILE]
    "./client_authorized_privkeys/charlie.privkey"   [FILE]

   If client authorization is _enabled_ _AND_ if the hidden service is
   responsible for generating and distributing private keys for its clients,
   then this directory contains files with client's private keys. See
   [CLIENT-AUTH-MGMT] for more details.

Appendix E. Managing authorized client data [CLIENT-AUTH-MGMT]

  Hidden services and clients can configure their authorized client data either
  using the torrc, or using the control port. This section presents a suggested
  scheme for configuring client authorization. Please see appendix
  [HIDSERVDIR-FORMAT] for more information about relevant hidden service files.

  E.1. Configuring client authorization using torrc

  E.1.1. Hidden Service side

     A hidden service that wants to perform client authorization, adds a new
     option HiddenServiceAuthorizeClient to its torrc file:

        HiddenServiceAuthorizeClient auth-type client-name,client-name,...

     The only recognized auth-type value is "basic" which describes the scheme in
     section [CLIENT-AUTH]. The rest of the line is a comma-separated list of
     human-readable authorized client names.

     Let's consider that one of the listed client names is "alice". In this
     case, Tor checks the "client_authorized_pubkeys" file for any entries
     with client_name being "alice". If an "alice" entry is found, we use the
     relevant pubkeys to authenticate Alice.

     If no "alice" entry is found in the "client_authorized_pubkeys" file, Tor
     is tasked with generating public/private keys for Alice. To do so, Tor
     generates x25519 and ed25519 keypairs for Alice, then makes a
     "client_authorized_privkeys/alice.privkey" file and writes the private
     keys inside; it also adds an entry for alice to the
     "client_authorized_pubkeys" file.

     In this last case, the hidden service operator has the responsibility to
     pass the .key file to Alice in a secure out-of-band way. After the file
     is passed to Alice, it can be shredded from the filesystem, as only the
     public keys are required for the hidden service to function.

  E.1.2. Client side

     A client who wants to register client authorization data for a hidden service
     needs to add the following line to their torrc:

           HidServAuth onion-address x25519-private-key ed25519-private-key

     The keys above are either generated by Alice using a key generation utility,
     or they are extracted from a .key file provided by the hidden service.

     In the former case, the client is also tasked with transfering the public
     keys to the hidden service in a secure out-of-band way.

  E.2. Configuring client authorization using the control port

  E.2.1. Service side

     A hidden service also has the option to configure authorized clients
     using the control port. The idea is that hidden service operators can use
     controller utilities that manage their access control instead of using
     the filesystem to register client keys.

     Specifically, we require a new control port command ADD_ONION_CLIENT_AUTH
     which is able to register x25519/ed25519 public keys tied to a specific
     authorized client.
      [XXX figure out control port command format]

     Hidden services who use the control port interface for client auth need
     to perform their own key management.

  E.2.2. Client side

     There should also be a control port interface for clients to register
     authorization data for hidden services without having to use the
     torrc. It should allow both generation of client authorization private
     keys, and also to import client authorization data provided by a hidden
     service

     This way, Tor Browser can present "Generate client auth keys" and "Import
     client auth keys" dialogs to users when they try to visit a hidden service
     that is protected by client authorization.

     Specifically, we require two new control port commands:
                   IMPORT_ONION_CLIENT_AUTH_DATA
                   GENERATE_ONION_CLIENT_AUTH_DATA
     which import and generate client authorization data respectively.

     [XXX how does key management work here?]
     [XXX what happens when people use both the control port interface and the
          filesystem interface?]

```
