
                     Tor Rendezvous Specification - Version 3

This document specifies how the hidden service version 3 protocol works.  This
text used to be proposal 224-rend-spec-ng.txt.


Table of contents:

    0. Hidden services: overview and preliminaries.
        0.1. Improvements over previous versions.
        0.2. Notation and vocabulary
        0.3. Cryptographic building blocks
        0.4. Protocol building blocks [BUILDING-BLOCKS]
        0.5. Assigned relay cell types
        0.6. Acknowledgments
    1. Protocol overview
        1.1. View from 10,000 feet
        1.2. In more detail: naming hidden services [NAMING]
        1.3. In more detail: Access control [IMD:AC]
        1.4. In more detail: Distributing hidden service descriptors. [IMD:DIST]
        1.5. In more detail: Scaling to multiple hosts
        1.6. In more detail: Backward compatibility with older hidden service
        1.7. In more detail: Keeping crypto keys offline
        1.8. In more detail: Encryption Keys And Replay Resistance
        1.9. In more detail: A menagerie of keys
            1.9.1. In even more detail: Client authorization [CLIENT-AUTH]
    2. Generating and publishing hidden service descriptors [HSDIR]
        2.1. Deriving blinded keys and subcredentials [SUBCRED]
        2.2. Locating, uploading, and downloading hidden service descriptors
            2.2.1. Dividing time into periods [TIME-PERIODS]
            2.2.2. When to publish a hidden service descriptor [WHEN-HSDESC]
            2.2.3. Where to publish a hidden service descriptor [WHERE-HSDESC]
            2.2.4. Using time periods and SRVs to fetch/upload HS descriptors
            2.2.5. Expiring hidden service descriptors [EXPIRE-DESC]
            2.2.6. URLs for anonymous uploading and downloading
        2.3. Publishing shared random values [PUB-SHAREDRANDOM]
            2.3.1. Client behavior in the absence of shared random values
            2.3.2. Hidden services and changing shared random values
        2.4. Hidden service descriptors: outer wrapper [DESC-OUTER]
        2.5. Hidden service descriptors: encryption format [HS-DESC-ENC]
            2.5.1. First layer of encryption [HS-DESC-FIRST-LAYER]
                2.5.1.1. First layer encryption logic
                2.5.1.2. First layer plaintext format
                2.5.1.3. Client behavior
                2.5.1.4. Obfuscating the number of authorized clients
            2.5.2. Second layer of encryption [HS-DESC-SECOND-LAYER]
                2.5.2.1. Second layer encryption keys
                2.5.2.2. Second layer plaintext format
            2.5.3. Deriving hidden service descriptor encryption keys [HS-DESC-ENCRYPTION-KEYS]
    3. The introduction protocol [INTRO-PROTOCOL]
        3.1. Registering an introduction point [REG_INTRO_POINT]
            3.1.1. Extensible ESTABLISH_INTRO protocol. [EST_INTRO]
               3.1.1.1. Denial-of-Server Defense Extension. [EST_INTRO_DOS_EXT]
            3.1.2. Registering an introduction point on a legacy Tor node [LEGACY_EST_INTRO]
            3.1.3. Acknowledging establishment of introduction point [INTRO_ESTABLISHED]
        3.2. Sending an INTRODUCE1 cell to the introduction point. [SEND_INTRO1]
            3.2.1. INTRODUCE1 cell format [FMT_INTRO1]
            3.2.2. INTRODUCE_ACK cell format. [INTRO_ACK]
        3.3. Processing an INTRODUCE2 cell at the hidden service. [PROCESS_INTRO2]
            3.3.1. Introduction handshake encryption requirements [INTRO-HANDSHAKE-REQS]
            3.3.2. Example encryption handshake: ntor with extra data [NTOR-WITH-EXTRA-DATA]
        3.4. Authentication during the introduction phase. [INTRO-AUTH]
            3.4.1. Ed25519-based authentication.
    4. The rendezvous protocol
        4.1. Establishing a rendezvous point [EST_REND_POINT]
        4.2. Joining to a rendezvous point [JOIN_REND]
            4.2.1. Key expansion
        4.3. Using legacy hosts as rendezvous points
    5. Encrypting data between client and host
    6. Encoding onion addresses [ONIONADDRESS]
    7. Open Questions:

-1. Draft notes

   This document describes a proposed design and specification for
   hidden services in Tor version 0.2.5.x or later. It's a replacement
   for the current rend-spec.txt, rewritten for clarity and for improved
   design.

   Look for the string "TODO" below: it describes gaps or uncertainties
   in the design.

   Change history:

       2013-11-29: Proposal first numbered. Some TODO and XXX items remain.

       2014-01-04: Clarify some unclear sections.

       2014-01-21: Fix a typo.

       2014-02-20: Move more things to the revised certificate format in the
           new updated proposal 220.

       2015-05-26: Fix two typos.


0. Hidden services: overview and preliminaries.

   Hidden services aim to provide responder anonymity for bidirectional
   stream-based communication on the Tor network. Unlike regular Tor
   connections, where the connection initiator receives anonymity but
   the responder does not, hidden services attempt to provide
   bidirectional anonymity.

   Participants:

      Operator -- A person running a hidden service

      Host, "Server" -- The Tor software run by the operator to provide
         a hidden service.

      User -- A person contacting a hidden service.

      Client -- The Tor software running on the User's computer

      Hidden Service Directory (HSDir) -- A Tor node that hosts signed
        statements from hidden service hosts so that users can make
        contact with them.

      Introduction Point -- A Tor node that accepts connection requests
        for hidden services and anonymously relays those requests to the
        hidden service.

      Rendezvous Point -- A Tor node to which clients and servers
        connect and which relays traffic between them.

0.1. Improvements over previous versions.

   Here is a list of improvements of this proposal over the legacy hidden
   services:

   a) Better crypto (replaced SHA1/DH/RSA1024 with SHA3/ed25519/curve25519)
   b) Improved directory protocol leaking less to directory servers.
   c) Improved directory protocol with smaller surface for targeted attacks.
   d) Better onion address security against impersonation.
   e) More extensible introduction/rendezvous protocol.
   f) Offline keys for onion services
   g) Advanced client authorization

0.2. Notation and vocabulary

   Unless specified otherwise, all multi-octet integers are big-endian.

   We write sequences of bytes in two ways:

     1. A sequence of two-digit hexadecimal values in square brackets,
        as in [AB AD 1D EA].

     2. A string of characters enclosed in quotes, as in "Hello". The
        characters in these strings are encoded in their ascii
        representations; strings are NOT nul-terminated unless
        explicitly described as NUL terminated.

   We use the words "byte" and "octet" interchangeably.

   We use the vertical bar | to denote concatenation.

   We use INT_N(val) to denote the network (big-endian) encoding of the
   unsigned integer "val" in N bytes. For example, INT_4(1337) is [00 00
   05 39]. Values are truncated like so: val % (2 ^ (N * 8)). For example,
   INT_4(42) is 42 % 4294967296 (32 bit).

0.3. Cryptographic building blocks

   This specification uses the following cryptographic building blocks:

      * A pseudorandom number generator backed by a strong entropy source.
        The output of the PRNG should always be hashed before being posted on
        the network to avoid leaking raw PRNG bytes to the network
        (see [PRNG-REFS]).

      * A stream cipher STREAM(iv, k) where iv is a nonce of length
        S_IV_LEN bytes and k is a key of length S_KEY_LEN bytes.

      * A public key signature system SIGN_KEYGEN()->seckey, pubkey;
        SIGN_SIGN(seckey,msg)->sig; and SIGN_CHECK(pubkey, sig, msg) ->
        { "OK", "BAD" }; where secret keys are of length SIGN_SECKEY_LEN
        bytes, public keys are of length SIGN_PUBKEY_LEN bytes, and
        signatures are of length SIGN_SIG_LEN bytes.

        This signature system must also support key blinding operations
        as discussed in appendix [KEYBLIND] and in section [SUBCRED]:
        SIGN_BLIND_SECKEY(seckey, blind)->seckey2 and
        SIGN_BLIND_PUBKEY(pubkey, blind)->pubkey2 .

      * A public key agreement system "PK", providing
        PK_KEYGEN()->seckey, pubkey; PK_VALID(pubkey) -> {"OK", "BAD"};
        and PK_HANDSHAKE(seckey, pubkey)->output; where secret keys are
        of length PK_SECKEY_LEN bytes, public keys are of length
        PK_PUBKEY_LEN bytes, and the handshake produces outputs of
        length PK_OUTPUT_LEN bytes.

      * A cryptographic hash function H(d), which should be preimage and
        collision resistant. It produces hashes of length HASH_LEN
        bytes.

      * A cryptographic message authentication code MAC(key,msg) that
        produces outputs of length MAC_LEN bytes.

      * A key derivation function KDF(message, n) that outputs n bytes.

   As a first pass, I suggest:

      * Instantiate STREAM with AES256-CTR.

      * Instantiate SIGN with Ed25519 and the blinding protocol in
        [KEYBLIND].

      * Instantiate PK with Curve25519.

      * Instantiate H with SHA3-256.

      * Instantiate KDF with SHAKE-256.

      * Instantiate MAC(key=k, message=m) with H(k_len | k | m),
        where k_len is htonll(len(k)).

	When we need a particular MAC key length below, we choose
	MAC_KEY_LEN=32 (256 bits).

   For legacy purposes, we specify compatibility with older versions of
   the Tor introduction point and rendezvous point protocols. These used
   RSA1024, DH1024, AES128, and SHA1, as discussed in
   rend-spec.txt.

   As in [proposal 220], all signatures are generated not over strings
   themselves, but over those strings prefixed with a distinguishing
   value.

0.4. Protocol building blocks [BUILDING-BLOCKS]

   In sections below, we need to transmit the locations and identities
   of Tor nodes. We do so in the link identification format used by
   EXTEND2 cells in the Tor protocol.

         NSPEC      (Number of link specifiers)   [1 byte]
         NSPEC times:
           LSTYPE (Link specifier type)           [1 byte]
           LSLEN  (Link specifier length)         [1 byte]
           LSPEC  (Link specifier)                [LSLEN bytes]

   Link specifier types are as described in tor-spec.txt. Every set of
   link specifiers SHOULD include at minimum specifiers of type [00]
   (TLS-over-TCP, IPv4), [02] (legacy node identity) and [03] (ed25519
   identity key).  Sets of link specifiers without these three types
   SHOULD be rejected.

   As of 0.4.1.1-alpha, Tor includes both IPv4 and IPv6 link specifiers
   in v3 onion service protocol link specifier lists. All available
   addresses SHOULD be included as link specifiers, regardless of the
   address that Tor actually used to connect/extend to the remote relay.

   We also incorporate Tor's circuit extension handshakes, as used in
   the CREATE2 and CREATED2 cells described in tor-spec.txt. In these
   handshakes, a client who knows a public key for a server sends a
   message and receives a message from that server. Once the exchange is
   done, the two parties have a shared set of forward-secure key
   material, and the client knows that nobody else shares that key
   material unless they control the secret key corresponding to the
   server's public key.

0.5. Assigned relay cell types

   These relay cell types are reserved for use in the hidden service
   protocol.

      32 -- RELAY_COMMAND_ESTABLISH_INTRO

            Sent from hidden service host to introduction point;
            establishes introduction point. Discussed in
            [REG_INTRO_POINT].

      33 -- RELAY_COMMAND_ESTABLISH_RENDEZVOUS

            Sent from client to rendezvous point; creates rendezvous
            point. Discussed in [EST_REND_POINT].

      34 -- RELAY_COMMAND_INTRODUCE1

            Sent from client to introduction point; requests
            introduction. Discussed in [SEND_INTRO1]

      35 -- RELAY_COMMAND_INTRODUCE2

            Sent from introduction point to hidden service host; requests
            introduction. Same format as INTRODUCE1. Discussed in
            [FMT_INTRO1] and [PROCESS_INTRO2]

      36 -- RELAY_COMMAND_RENDEZVOUS1

            Sent from hidden service host to rendezvous point;
            attempts to join host's circuit to
            client's circuit. Discussed in [JOIN_REND]

      37 -- RELAY_COMMAND_RENDEZVOUS2

            Sent from rendezvous point to client;
            reports join of host's circuit to
            client's circuit. Discussed in [JOIN_REND]

      38 -- RELAY_COMMAND_INTRO_ESTABLISHED

            Sent from introduction point to hidden service host;
            reports status of attempt to establish introduction
            point. Discussed in [INTRO_ESTABLISHED]

      39 -- RELAY_COMMAND_RENDEZVOUS_ESTABLISHED

            Sent from rendezvous point to client; acknowledges
            receipt of ESTABLISH_RENDEZVOUS cell. Discussed in
            [EST_REND_POINT]

      40 -- RELAY_COMMAND_INTRODUCE_ACK

            Sent from introduction point to client; acknowledges
            receipt of INTRODUCE1 cell and reports success/failure.
            Discussed in [INTRO_ACK]

0.6. Acknowledgments

   This design includes ideas from many people, including

     Christopher Baines,
     Daniel J. Bernstein,
     Matthew Finkel,
     Ian Goldberg,
     George Kadianakis,
     Aniket Kate,
     Tanja Lange,
     Robert Ransom,
     Roger Dingledine,
     Aaron Johnson,
     Tim Wilson-Brown ("teor"),
     special (John Brooks),
     s7r

   It's based on Tor's original hidden service design by Roger
   Dingledine, Nick Mathewson, and Paul Syverson, and on improvements to
   that design over the years by people including

     Tobias Kamm,
     Thomas Lauterbach,
     Karsten Loesing,
     Alessandro Preite Martinez,
     Robert Ransom,
     Ferdinand Rieger,
     Christoph Weingarten,
     Christian Wilms,

   We wouldn't be able to do any of this work without good attack
   designs from researchers including

     Alex Biryukov,
     Lasse Øverlier,
     Ivan Pustogarov,
     Paul Syverson,
     Ralf-Philipp Weinmann,

   See [ATTACK-REFS] for their papers.

   Several of these ideas have come from conversations with

      Christian Grothoff,
      Brian Warner,
      Zooko Wilcox-O'Hearn,

   And if this document makes any sense at all, it's thanks to
   editing help from

      Matthew Finkel,
      George Kadianakis,
      Peter Palfrader,
      Tim Wilson-Brown ("teor"),


   [XXX  Acknowledge the huge bunch of people working on 8106.]
   [XXX  Acknowledge the huge bunch of people working on 8244.]


   Please forgive me if I've missed you; please forgive me if I've
   misunderstood your best ideas here too.


1. Protocol overview

   In this section, we outline the hidden service protocol. This section
   omits some details in the name of simplicity; those are given more
   fully below, when we specify the protocol in more detail.

1.1. View from 10,000 feet

   A hidden service host prepares to offer a hidden service by choosing
   several Tor nodes to serve as its introduction points. It builds
   circuits to those nodes, and tells them to forward introduction
   requests to it using those circuits.

   Once introduction points have been picked, the host builds a set of
   documents called "hidden service descriptors" (or just "descriptors"
   for short) and uploads them to a set of HSDir nodes. These documents
   list the hidden service's current introduction points and describe
   how to make contact with the hidden service.

   When a client wants to connect to a hidden service, it first chooses
   a Tor node at random to be its "rendezvous point" and builds a
   circuit to that rendezvous point. If the client does not have an
   up-to-date descriptor for the service, it contacts an appropriate
   HSDir and requests such a descriptor.

   The client then builds an anonymous circuit to one of the hidden
   service's introduction points listed in its descriptor, and gives the
   introduction point an introduction request to pass to the hidden
   service. This introduction request includes the target rendezvous
   point and the first part of a cryptographic handshake.

   Upon receiving the introduction request, the hidden service host
   makes an anonymous circuit to the rendezvous point and completes the
   cryptographic handshake. The rendezvous point connects the two
   circuits, and the cryptographic handshake gives the two parties a
   shared key and proves to the client that it is indeed talking to the
   hidden service.

   Once the two circuits are joined, the client can send Tor RELAY cells
   to the server. RELAY_BEGIN cells open streams to an external process
   or processes configured by the server; RELAY_DATA cells are used to
   communicate data on those streams, and so forth.

1.2. In more detail: naming hidden services [NAMING]

   A hidden service's name is its long term master identity key.  This is
   encoded as a hostname by encoding the entire key in Base 32, including a
   version byte and a checksum, and then appending the string ".onion" at the
   end. The result is a 56-character domain name.

   (This is a change from older versions of the hidden service protocol,
   where we used an 80-bit truncated SHA1 hash of a 1024 bit RSA key.)

   The names in this format are distinct from earlier names because of
   their length. An older name might look like:

        unlikelynamefora.onion
        yyhws9optuwiwsns.onion

   And a new name following this specification might look like:

        l5satjgud6gucryazcyvyvhuxhr74u6ygigiuyixe3a6ysis67ororad.onion

   Please see section [ONIONADDRESS] for the encoding specification.

1.3. In more detail: Access control [IMD:AC]

   Access control for a hidden service is imposed at multiple points through
   the process above. Furthermore, there is also the option to impose
   additional client authorization access control using pre-shared secrets
   exchanged out-of-band between the hidden service and its clients.

   The first stage of access control happens when downloading HS descriptors.
   Specifically, in order to download a descriptor, clients must know which
   blinded signing key was used to sign it. (See the next section for more info
   on key blinding.)

   To learn the introduction points, clients must decrypt the body of the
   hidden service descriptor. To do so, clients must know the _unblinded_
   public key of the service, which makes the descriptor unusable by entities
   without that knowledge (e.g. HSDirs that don't know the onion address).

   Also, if optional client authorization is enabled, hidden service
   descriptors are superencrypted using each authorized user's identity x25519
   key, to further ensure that unauthorized entities cannot decrypt it.

   In order to make the introduction point send a rendezvous request to the
   service, the client needs to use the per-introduction-point authentication
   key found in the hidden service descriptor.

   The final level of access control happens at the server itself, which may
   decide to respond or not respond to the client's request depending on the
   contents of the request. The protocol is extensible at this point: at a
   minimum, the server requires that the client demonstrate knowledge of the
   contents of the encrypted portion of the hidden service descriptor. If
   optional client authorization is enabled, the service may additionally
   require the client to prove knowledge of a pre-shared private key.

1.4. In more detail: Distributing hidden service descriptors. [IMD:DIST]

   Periodically, hidden service descriptors become stored at different
   locations to prevent a single directory or small set of directories
   from becoming a good DoS target for removing a hidden service.

   For each period, the Tor directory authorities agree upon a
   collaboratively generated random value. (See section 2.3 for a
   description of how to incorporate this value into the voting
   practice; generating the value is described in other proposals,
   including [SHAREDRANDOM-REFS].) That value, combined with hidden service
   directories' public identity keys, determines each HSDir's position
   in the hash ring for descriptors made in that period.

   Each hidden service's descriptors are placed into the ring in
   positions based on the key that was used to sign them. Note that
   hidden service descriptors are not signed with the services' public
   keys directly. Instead, we use a key-blinding system [KEYBLIND] to
   create a new key-of-the-day for each hidden service. Any client that
   knows the hidden service's public identity key can derive these blinded
   signing keys for a given period. It should be impossible to derive
   the blinded signing key lacking that knowledge.

   This is achieved using two nonces:

    * A "credential", derived from the public identity key KP_hs_id.
      N_hs_cred.

    * A "subcredential", derived from the credential N_hs_cred
      and information which various with the current time period.
      N_hs_subcred.

   The body of each descriptor is also encrypted with a key derived from
   the public signing key.

   To avoid a "thundering herd" problem where every service generates
   and uploads a new descriptor at the start of each period, each
   descriptor comes online at a time during the period that depends on
   its blinded signing key. The keys for the last period remain valid
   until the new keys come online.

1.5. In more detail: Scaling to multiple hosts

   This design is compatible with our current approaches for scaling hidden
   services. Specifically, hidden service operators can use onionbalance to
   achieve high availability between multiple nodes on the HSDir
   layer. Furthermore, operators can use proposal 255 to load balance their
   hidden services on the introduction layer. See [SCALING-REFS] for further
   discussions on this topic and alternative designs.

1.6. In more detail: Backward compatibility with older hidden service
      protocols

   This design is incompatible with the clients, server, and hsdir node
   protocols from older versions of the hidden service protocol as
   described in rend-spec.txt. On the other hand, it is designed to
   enable the use of older Tor nodes as rendezvous points and
   introduction points.

1.7. In more detail: Keeping crypto keys offline

   In this design, a hidden service's secret identity key may be
   stored offline.  It's used only to generate blinded signing keys,
   which are used to sign descriptor signing keys.

   In order to operate a hidden service, the operator can generate in
   advance a number of blinded signing keys and descriptor signing
   keys (and their credentials; see [DESC-OUTER] and [HS-DESC-ENC]
   below), and their corresponding descriptor encryption keys, and
   export those to the hidden service hosts.

   As a result, in the scenario where the Hidden Service gets
   compromised, the adversary can only impersonate it for a limited
   period of time (depending on how many signing keys were generated
   in advance).

   It's important to not send the private part of the blinded signing
   key to the Hidden Service since an attacker can derive from it the
   secret master identity key. The secret blinded signing key should
   only be used to create credentials for the descriptor signing keys.

   (NOTE: although the protocol allows them, offline keys are not
   implemented as of 0.3.2.1-alpha.)

1.8. In more detail: Encryption Keys And Replay Resistance

   To avoid replays of an introduction request by an introduction point,
   a hidden service host must never accept the same request
   twice. Earlier versions of the hidden service design used an
   authenticated timestamp here, but including a view of the current
   time can create a problematic fingerprint. (See proposal 222 for more
   discussion.)

1.9. In more detail: A menagerie of keys

   [In the text below, an "encryption keypair" is roughly "a keypair you
   can do Diffie-Hellman with" and a "signing keypair" is roughly "a
   keypair you can do ECDSA with."]

   Public/private keypairs defined in this document:

      Master (hidden service) identity key -- A master signing keypair
        used as the identity for a hidden service.  This key is long
        term and not used on its own to sign anything; it is only used
        to generate blinded signing keys as described in [KEYBLIND]
        and [SUBCRED]. The public key is encoded in the ".onion"
        address according to [NAMING].
        KP_hs_id, KS_hs_id.

      Blinded signing key -- A keypair derived from the identity key,
        used to sign descriptor signing keys. It changes periodically for
        each service. Clients who know a 'credential' consisting of the
        service's public identity key and an optional secret can derive
        the public blinded identity key for a service.  This key is used
        as an index in the DHT-like structure of the directory system
        (see [SUBCRED]).
        KP_hs_blind_id, KS_hs_blind_id.

      Descriptor signing key -- A key used to sign hidden service
        descriptors.  This is signed by blinded signing keys. Unlike
        blinded signing keys and master identity keys, the secret part
        of this key must be stored online by hidden service hosts. The
        public part of this key is included in the unencrypted section
        of HS descriptors (see [DESC-OUTER]).
        KP_hs_desc_sign, KS_hs_desc_sign.

      Introduction point authentication key -- A short-term signing
        keypair used to identify a hidden service's session at a given
        introduction point. The service makes a fresh keypair for each
        introduction point; these are used to sign the request that a
        hidden service host makes when establishing an introduction
        point, so that clients who know the public component of this key
        can get their introduction requests sent to the right
        service. No keypair is ever used with more than one introduction
        point. (previously called a "service key" in rend-spec.txt)
        KP_hs_ipt_sid, KS_hs_ipt_sid
        ("hidden service introduction point session id").

      Introduction point encryption key -- A short-term encryption
        keypair used when establishing connections via an introduction
        point. Plays a role analogous to Tor nodes' onion keys. The service
        makes a fresh keypair for each introduction point.
        KP_hss_ntor, KS_hss_ntor.

      Ephemeral descriptor encryption key -- A short-lived encryption
        keypair made by the service, and used to encrypt the inner layer
        of hidden service descriptors when client authentication is in
        use.
        KP_hss_desc_enc, KS_hss_desc_enc

   Nonces defined in this document:

      N_hs_desc_enc -- a nonce used to derive keys to decrypt the inner
        encryption layer of hidden service descriptors.  This is
        sometimes also called a "descriptor cookie".

   Public/private keypairs defined elsewhere:

      Onion key -- Short-term encryption keypair (KS_ntor, KP_ntor).

      (Node) identity key (KP_relayid).

   Symmetric key-like things defined elsewhere:

      KH from circuit handshake -- An unpredictable value derived as
      part of the Tor circuit extension handshake, used to tie a request
      to a particular circuit.

1.9.1. In even more detail: Client authorization keys [CLIENT-AUTH]

   When client authorization is enabled, each authorized client of a hidden
   service has two more asymmetric keypairs which are shared with the hidden
   service. An entity without those keys is not able to use the hidden
   service. Throughout this document, we assume that these pre-shared keys are
   exchanged between the hidden service and its clients in a secure out-of-band
   fashion.

   Specifically, each authorized client possesses:

   - An x25519 keypair used to compute decryption keys that allow the client to
     decrypt the hidden service descriptor. See [HS-DESC-ENC].  This is
     the client's counterpart to KP_hss_desc_enc.
     KP_hsc_desc_enc, KS_hsd_desc_enc.

   - An ed25519 keypair which allows the client to compute signatures which
     prove to the hidden service that the client is authorized. These
     signatures are inserted into the INTRODUCE1 cell, and without them the
     introduction to the hidden service cannot be completed. See [INTRO-AUTH].
     KP_hsc_intro_auth, KS_hsc_intro_auth.

   The right way to exchange these keys is to have the client generate keys and
   send the corresponding public keys to the hidden service out-of-band. An
   easier but less secure way of doing this exchange would be to have the
   hidden service generate the keypairs and pass the corresponding private keys
   to its clients. See section [CLIENT-AUTH-MGMT] for more details on how these
   keys should be managed.

   [TODO: Also specify stealth client authorization.]

   (NOTE: client authorization is implemented as of 0.3.5.1-alpha.)

2. Generating and publishing hidden service descriptors [HSDIR]

   Hidden service descriptors follow the same metaformat as other Tor
   directory objects. They are published anonymously to Tor servers with the
   HSDir flag, HSDir=2 protocol version and tor version >= 0.3.0.8 (because a
   bug was fixed in this version).

2.1. Deriving blinded keys and subcredentials [SUBCRED]

   In each time period (see [TIME-PERIODS] for a definition of time
   periods), a hidden service host uses a different blinded private key
   to sign its directory information, and clients use a different
   blinded public key as the index for fetching that information.

   For a candidate for a key derivation method, see Appendix [KEYBLIND].

   Additionally, clients and hosts derive a subcredential for each
   period. Knowledge of the subcredential is needed to decrypt hidden
   service descriptors for each period and to authenticate with the
   hidden service host in the introduction process. Unlike the
   credential, it changes each period. Knowing the subcredential, even
   in combination with the blinded private key, does not enable the
   hidden service host to derive the main credential--therefore, it is
   safe to put the subcredential on the hidden service host while
   leaving the hidden service's private key offline.

   The subcredential for a period is derived as:

       N_hs_subcred = H("subcredential" | N_hs_cred | blinded-public-key).

   In the above formula, credential corresponds to:

       N_hs_cred = H("credential" | public-identity-key)

   where public-identity-key is the public identity master key of the hidden
   service.

2.2. Locating, uploading, and downloading hidden service descriptors
       [HASHRING]

   To avoid attacks where a hidden service's descriptor is easily
   targeted for censorship, we store them at different directories over
   time, and use shared random values to prevent those directories from
   being predictable far in advance.

   Which Tor servers hosts a hidden service depends on:

         * the current time period,
         * the daily subcredential,
         * the hidden service directories' public keys,
         * a shared random value that changes in each time period,
           shared_random_value.
         * a set of network-wide networkstatus consensus parameters.
           (Consensus parameters are integer values voted on by authorities
           and published in the consensus documents, described in
           dir-spec.txt, section 3.3.)

   Below we explain in more detail.

2.2.1. Dividing time into periods [TIME-PERIODS]

   To prevent a single set of hidden service directory from becoming a
   target by adversaries looking to permanently censor a hidden service,
   hidden service descriptors are uploaded to different locations that
   change over time.

   The length of a "time period" is controlled by the consensus
   parameter 'hsdir-interval', and is a number of minutes between 30 and
   14400 (10 days). The default time period length is 1440 (one day).

   Time periods start at the Unix epoch (Jan 1, 1970), and are computed by
   taking the number of minutes since the epoch and dividing by the time
   period. However, we want our time periods to start at a regular offset
   from the SRV voting schedule, so  we subtract a "rotation time offset"
   of 12 voting periods from the number of minutes since the epoch, before
   dividing by the time period (effectively making "our" epoch start at Jan
   1, 1970 12:00UTC when the voting period is 1 hour.)

   Example: If the current time is 2016-04-13 11:15:01 UTC, making the seconds
   since the epoch 1460546101, and the number of minutes since the epoch
   24342435.  We then subtract the "rotation time offset" of 12*60 minutes from
   the minutes since the epoch, to get 24341715. If the current time period
   length is 1440 minutes, by doing the division we see that we are currently
   in time period number 16903.

   Specifically, time period #16903 began 16903*1440*60 + (12*60*60) seconds
   after the epoch, at 2016-04-12 12:00 UTC, and ended at 16904*1440*60 +
   (12*60*60) seconds after the epoch, at 2016-04-13 12:00 UTC.

2.2.2. When to publish a hidden service descriptor [WHEN-HSDESC]

   Hidden services periodically publish their descriptor to the responsible
   HSDirs. The set of responsible HSDirs is determined as specified in
   [WHERE-HSDESC].

   Specifically, every time a hidden service publishes its descriptor, it also
   sets up a timer for a random time between 60 minutes and 120 minutes in the
   future. When the timer triggers, the hidden service needs to publish its
   descriptor again to the responsible HSDirs for that time period.
   [TODO: Control republish period using a consensus parameter?]

2.2.2.1. Overlapping descriptors

   Hidden services need to upload multiple descriptors so that they can be
   reachable to clients with older or newer consensuses than them. Services
   need to upload their descriptors to the HSDirs _before_ the beginning of
   each upcoming time period, so that they are readily available for clients to
   fetch them. Furthermore, services should keep uploading their old descriptor
   even after the end of a time period, so that they can be reachable by
   clients that still have consensuses from the previous time period.

   Hence, services maintain two active descriptors at every point. Clients on
   the other hand, don't have a notion of overlapping descriptors, and instead
   always download the descriptor for the current time period and shared random
   value. It's the job of the service to ensure that descriptors will be
   available for all clients. See section [FETCHUPLOADDESC] for how this is
   achieved.

   [TODO: What to do when we run multiple hidden services in a single host?]

2.2.3. Where to publish a hidden service descriptor [WHERE-HSDESC]

   This section specifies how the HSDir hash ring is formed at any given
   time. Whenever a time value is needed (e.g. to get the current time period
   number), we assume that clients and services use the valid-after time from
   their latest live consensus.

   The following consensus parameters control where a hidden service
   descriptor is stored;

        hsdir_n_replicas = an integer in range [1,16] with default value 2.
        hsdir_spread_fetch = an integer in range [1,128] with default value 3.
        hsdir_spread_store = an integer in range [1,128] with default value 4.
           (Until 0.3.2.8-rc, the default was 3.)

   To determine where a given hidden service descriptor will be stored
   in a given period, after the blinded public key for that period is
   derived, the uploading or downloading party calculates:

        for replicanum in 1...hsdir_n_replicas:
            hs_service_index(replicanum) = H("store-at-idx" |
                                     blinded_public_key |
                                     INT_8(replicanum) |
                                     INT_8(period_length) |
                                     INT_8(period_num) )

   where blinded_public_key is specified in section [KEYBLIND], period_length
   is the length of the time period in minutes, and period_num is calculated
   using the current consensus "valid-after" as specified in section
   [TIME-PERIODS].

   Then, for each node listed in the current consensus with the HSDir flag,
   we compute a directory index for that node as:

           hs_relay_index(node) = H("node-idx" | node_identity |
                                 shared_random_value |
                                 INT_8(period_num) |
                                 INT_8(period_length) )

   where shared_random_value is the shared value generated by the authorities
   in section [PUB-SHAREDRANDOM], and node_identity is the ed25519 identity
   key of the node.

   Finally, for replicanum in 1...hsdir_n_replicas, the hidden service
   host uploads descriptors to the first hsdir_spread_store nodes whose
   indices immediately follow hs_service_index(replicanum). If any of those
   nodes have already been selected for a lower-numbered replica of the
   service, any nodes already chosen are disregarded (i.e. skipped over)
   when choosing a replica's hsdir_spread_store nodes.

   When choosing an HSDir to download from, clients choose randomly from
   among the first hsdir_spread_fetch nodes after the indices.  (Note
   that, in order to make the system better tolerate disappearing
   HSDirs, hsdir_spread_fetch may be less than hsdir_spread_store.)
   Again, nodes from lower-numbered replicas are disregarded when
   choosing the spread for a replica.

2.2.4. Using time periods and SRVs to fetch/upload HS descriptors [FETCHUPLOADDESC]

   Hidden services and clients need to make correct use of time periods (TP)
   and shared random values (SRVs) to successfully fetch and upload
   descriptors. Furthermore, to avoid problems with skewed clocks, both clients
   and services use the 'valid-after' time of a live consensus as a way to take
   decisions with regards to uploading and fetching descriptors. By using the
   consensus times as the ground truth here, we minimize the desynchronization
   of clients and services due to system clock. Whenever time-based decisions
   are taken in this section, assume that they are consensus times and not
   system times.

   As [PUB-SHAREDRANDOM] specifies, consensuses contain two shared random
   values (the current one and the previous one). Hidden services and clients
   are asked to match these shared random values with descriptor time periods
   and use the right SRV when fetching/uploading descriptors. This section
   attempts to precisely specify how this works.

   Let's start with an illustration of the system:

      +------------------------------------------------------------------+
      |                                                                  |
      | 00:00      12:00       00:00       12:00       00:00       12:00 |
      | SRV#1      TP#1        SRV#2       TP#2        SRV#3       TP#3  |
      |                                                                  |
      |  $==========|-----------$===========|-----------$===========|    |
      |                                                                  |
      |                                                                  |
      +------------------------------------------------------------------+

                                      Legend: [TP#1 = Time Period #1]
                                              [SRV#1 = Shared Random Value #1]
                                              ["$" = descriptor rotation moment]

2.2.4.1. Client behavior for fetching descriptors [CLIENTFETCH]

   And here is how clients use TPs and SRVs to fetch descriptors:

   Clients always aim to synchronize their TP with SRV, so they always want to
   use TP#N with SRV#N: To achieve this wrt time periods, clients always use
   the current time period when fetching descriptors. Now wrt SRVs, if a client
   is in the time segment between a new time period and a new SRV (i.e. the
   segments drawn with "-") it uses the current SRV, else if the client is in a
   time segment between a new SRV and a new time period (i.e. the segments
   drawn with "="), it uses the previous SRV.

   Example:

   +------------------------------------------------------------------+
   |                                                                  |
   | 00:00      12:00       00:00       12:00       00:00       12:00 |
   | SRV#1      TP#1        SRV#2       TP#2        SRV#3       TP#3  |
   |                                                                  |
   |  $==========|-----------$===========|-----------$===========|    |
   |              ^           ^                                       |
   |              C1          C2                                      |
   +------------------------------------------------------------------+

   If a client (C1) is at 13:00 right after TP#1, then it will use TP#1 and
   SRV#1 for fetching descriptors. Also, if a client (C2) is at 01:00 right
   after SRV#2, it will still use TP#1 and SRV#1.

2.2.4.2. Service behavior for uploading descriptors [SERVICEUPLOAD]

   As discussed above, services maintain two active descriptors at any time. We
   call these the "first" and "second" service descriptors. Services rotate
   their descriptor every time they receive a consensus with a valid_after time
   past the next SRV calculation time. They rotate their descriptors by
   discarding their first descriptor, pushing the second descriptor to the
   first, and rebuilding their second descriptor with the latest data.

   Services like clients also employ a different logic for picking SRV and TP
   values based on their position in the graph above. Here is the logic:

2.2.4.2.1. First descriptor upload logic [FIRSTDESCUPLOAD]

   Here is the service logic for uploading its first descriptor:

   When a service is in the time segment between a new time period a new SRV
   (i.e. the segments drawn with "-"), it uses the previous time period and
   previous SRV for uploading its first descriptor: that's meant to cover
   for clients that have a consensus that is still in the previous time period.

   Example: Consider in the above illustration that the service is at 13:00
   right after TP#1. It will upload its first descriptor using TP#0 and SRV#0.
   So if a client still has a 11:00 consensus it will be able to access it
   based on the client logic above.

   Now if a service is in the time segment between a new SRV and a new time
   period (i.e. the segments drawn with "=") it uses the current time period
   and the previous SRV for its first descriptor: that's meant to cover clients
   with an up-to-date consensus in the same time period as the service.

   Example:

   +------------------------------------------------------------------+
   |                                                                  |
   | 00:00      12:00       00:00       12:00       00:00       12:00 |
   | SRV#1      TP#1        SRV#2       TP#2        SRV#3       TP#3  |
   |                                                                  |
   |  $==========|-----------$===========|-----------$===========|    |
   |                          ^                                       |
   |                          S                                       |
   +------------------------------------------------------------------+

   Consider that the service is at 01:00 right after SRV#2: it will upload its
   first descriptor using TP#1 and SRV#1.

2.2.4.2.2. Second descriptor upload logic [SECONDDESCUPLOAD]

   Here is the service logic for uploading its second descriptor:

   When a service is in the time segment between a new time period a new SRV
   (i.e. the segments drawn with "-"), it uses the current time period and
   current SRV for uploading its second descriptor: that's meant to cover for
   clients that have an up-to-date consensus on the same TP as the service.

   Example: Consider in the above illustration that the service is at 13:00
   right after TP#1: it will upload its second descriptor using TP#1 and SRV#1.

   Now if a service is in the time segment between a new SRV and a new time
   period (i.e. the segments drawn with "=") it uses the next time period and
   the current SRV for its second descriptor: that's meant to cover clients
   with a newer consensus than the service (in the next time period).

   Example:

   +------------------------------------------------------------------+
   |                                                                  |
   | 00:00      12:00       00:00       12:00       00:00       12:00 |
   | SRV#1      TP#1        SRV#2       TP#2        SRV#3       TP#3  |
   |                                                                  |
   |  $==========|-----------$===========|-----------$===========|    |
   |                          ^                                       |
   |                          S                                       |
   +------------------------------------------------------------------+

   Consider that the service is at 01:00 right after SRV#2: it will upload its
   second descriptor using TP#2 and SRV#2.

2.2.4.3. Directory behavior for handling descriptor uploads [DIRUPLOAD]

   Upon receiving a hidden service descriptor publish request, directories MUST
   check the following:

     * The outer wrapper of the descriptor can be parsed according to
       [DESC-OUTER]
     * The version-number of the descriptor is "3"
     * If the directory has already cached a descriptor for this hidden service,
       the revision-counter of the uploaded descriptor must be greater than the
       revision-counter of the cached one
     * The descriptor signature is valid

   If any of these basic validity checks fails, the directory MUST reject the
   descriptor upload.

   NOTE: Even if the descriptor passes the checks above, its first and second
   layers could still be invalid: directories cannot validate the encrypted
   layers of the descriptor, as they do not have access to the public key of the
   service (required for decrypting the first layer of encryption), or the
   necessary client credentials (for decrypting the second layer).

2.2.5. Expiring hidden service descriptors [EXPIRE-DESC]

   Hidden services set their descriptor's "descriptor-lifetime" field to 180
   minutes (3 hours). Hidden services ensure that their descriptor will remain
   valid in the HSDir caches, by republishing their descriptors periodically as
   specified in [WHEN-HSDESC].

   Hidden services MUST also keep their introduction circuits alive for as long
   as descriptors including those intro points are valid (even if that's after
   the time period has changed).

2.2.6. URLs for anonymous uploading and downloading

   Hidden service descriptors conforming to this specification are uploaded
   with an HTTP POST request to the URL /tor/hs/<version>/publish relative to
   the hidden service directory's root, and downloaded with an HTTP GET
   request for the URL /tor/hs/<version>/<z> where <z> is a base64 encoding of
   the hidden service's blinded public key and <version> is the protocol
   version which is "3" in this case.

   These requests must be made anonymously, on circuits not used for
   anything else.

2.2.7. Client-side validation of onion addresses

   When a Tor client receives a prop224 onion address from the user, it
   MUST first validate the onion address before attempting to connect or
   fetch its descriptor. If the validation fails, the client MUST
   refuse to connect.

   As part of the address validation, Tor clients should check that the
   underlying ed25519 key does not have a torsion component. If Tor accepted
   ed25519 keys with torsion components, attackers could create multiple
   equivalent onion addresses for a single ed25519 key, which would map to the
   same service. We want to avoid that because it could lead to phishing
   attacks and surprising behaviors (e.g. imagine a browser plugin that blocks
   onion addresses, but could be bypassed using an equivalent onion address
   with a torsion component).

   The right way for clients to detect such fraudulent addresses (which should
   only occur malevolently and never naturally) is to extract the ed25519
   public key from the onion address and multiply it by the ed25519 group order
   and ensure that the result is the ed25519 identity element. For more
   details, please see [TORSION-REFS].

2.3. Publishing shared random values [PUB-SHAREDRANDOM]

   Our design for limiting the predictability of HSDir upload locations
   relies on a shared random value (SRV) that isn't predictable in advance or
   too influenceable by an attacker. The authorities must run a protocol
   to generate such a value at least once per hsdir period. Here we
   describe how they publish these values; the procedure they use to
   generate them can change independently of the rest of this
   specification. For more information see [SHAREDRANDOM-REFS].

   According to proposal 250, we add two new lines in consensuses:

     "shared-rand-previous-value" SP NUM_REVEALS SP VALUE NL
     "shared-rand-current-value" SP NUM_REVEALS SP VALUE NL

2.3.1. Client behavior in the absence of shared random values

   If the previous or current shared random value cannot be found in a
   consensus, then Tor clients and services need to generate their own random
   value for use when choosing HSDirs.

   To do so, Tor clients and services use:

     SRV = H("shared-random-disaster" | INT_8(period_length) | INT_8(period_num))

   where period_length is the length of a time period in minutes,
   rounded down; period_num is calculated as specified in
   [TIME-PERIODS] for the wanted shared random value that could not be
   found originally.

2.3.2. Hidden services and changing shared random values

   It's theoretically possible that the consensus shared random values will
   change or disappear in the middle of a time period because of directory
   authorities dropping offline or misbehaving.

   To avoid client reachability issues in this rare event, hidden services
   should use the new shared random values to find the new responsible HSDirs
   and upload their descriptors there.

   XXX How long should they upload descriptors there for?

2.4. Hidden service descriptors: outer wrapper [DESC-OUTER]

   The format for a hidden service descriptor is as follows, using the
   meta-format from dir-spec.txt.

     "hs-descriptor" SP version-number NL

       [At start, exactly once.]

       The version-number is a 32 bit unsigned integer indicating the version
       of the descriptor. Current version is "3".

     "descriptor-lifetime" SP LifetimeMinutes NL

       [Exactly once]

       The lifetime of a descriptor in minutes. An HSDir SHOULD expire the
       hidden service descriptor at least LifetimeMinutes after it was
       uploaded.

       The LifetimeMinutes field can take values between 30 and 720 (12
       hours).

    "descriptor-signing-key-cert" NL certificate NL

       [Exactly once.]

       The 'certificate' field contains a certificate in the format from
       proposal 220, wrapped with "-----BEGIN ED25519 CERT-----".  The
       certificate cross-certifies the short-term descriptor signing key with
       the blinded public key.  The certificate type must be [08], and the
       blinded public key must be present as the signing-key extension.

     "revision-counter" SP Integer NL

       [Exactly once.]

       The revision number of the descriptor. If an HSDir receives a
       second descriptor for a key that it already has a descriptor for,
       it should retain and serve the descriptor with the higher
       revision-counter.

       (Checking for monotonically increasing revision-counter values
       prevents an attacker from replacing a newer descriptor signed by
       a given key with a copy of an older version.)

       Implementations MUST be able to parse 64-bit values for these
       counters.

     "superencrypted" NL encrypted-string

       [Exactly once.]

       An encrypted blob, whose format is discussed in [HS-DESC-ENC] below. The
       blob is base64 encoded and enclosed in -----BEGIN MESSAGE---- and
       ----END MESSAGE---- wrappers. (The resulting document does not end with
       a newline character.)

     "signature" SP signature NL

       [exactly once, at end.]

       A signature of all previous fields, using the signing key in the
       descriptor-signing-key-cert line, prefixed by the string "Tor onion
       service descriptor sig v3". We use a separate key for signing, so that
       the hidden service host does not need to have its private blinded key
       online.

   HSDirs accept hidden service descriptors of up to 50k bytes (a consensus
   parameter should also be introduced to control this value).

2.5. Hidden service descriptors: encryption format [HS-DESC-ENC]

   Hidden service descriptors are protected by two layers of encryption.
   Clients need to decrypt both layers to connect to the hidden service.

   The first layer of encryption provides confidentiality against entities who
   don't know the public key of the hidden service (e.g. HSDirs), while the
   second layer of encryption is only useful when client authorization is enabled
   and protects against entities that do not possess valid client credentials.

2.5.1. First layer of encryption [HS-DESC-FIRST-LAYER]

   The first layer of HS descriptor encryption is designed to protect
   descriptor confidentiality against entities who don't know the public
   identity key of the hidden service.

2.5.1.1. First layer encryption logic

   The encryption keys and format for the first layer of encryption are
   generated as specified in [HS-DESC-ENCRYPTION-KEYS] with customization
   parameters:

     SECRET_DATA = blinded-public-key
     STRING_CONSTANT = "hsdir-superencrypted-data"

   The encryption scheme in [HS-DESC-ENCRYPTION-KEYS] uses the service
   credential which is derived from the public identity key (see [SUBCRED]) to
   ensure that only entities who know the public identity key can decrypt the
   first descriptor layer.

   The ciphertext is placed on the "superencrypted" field of the descriptor.

   Before encryption the plaintext is padded with NUL bytes to the nearest
   multiple of 10k bytes.

2.5.1.2. First layer plaintext format

   After clients decrypt the first layer of encryption, they need to parse the
   plaintext to get to the second layer ciphertext which is contained in the
   "encrypted" field.

   If client auth is enabled, the hidden service generates a fresh
   descriptor_cookie key (`N_hs_desc_enc`, 32 random bytes) and encrypts
   it using each authorized client's identity x25519 key. Authorized
   clients can use the descriptor cookie (`N_hs_desc_enc`) to decrypt
   the second (inner) layer of encryption. Our encryption scheme
   requires the hidden service to also generate an ephemeral x25519
   keypair for each new descriptor.

   If client auth is disabled, fake data is placed in each of the fields below
   to obfuscate whether client authorization is enabled.

   Here are all the supported fields:

     "desc-auth-type" SP type NL

      [Exactly once]

      This field contains the type of authorization used to protect the
      descriptor. The only recognized type is "x25519" and specifies the
      encryption scheme described in this section.

      If client authorization is disabled, the value here should be "x25519".

     "desc-auth-ephemeral-key" SP KP_hs_desc_ephem NL

      [Exactly once]

      This field contains `KP_hss_desc_enc`, an ephemeral x25519 public
      key generated by the hidden service and encoded in base64. The key
      is used by the encryption scheme below.

      If client authorization is disabled, the value here should be a fresh
      x25519 pubkey that will remain unused.

     "auth-client" SP client-id SP iv SP encrypted-cookie

      [At least once]

      When client authorization is enabled, the hidden service inserts an
      "auth-client" line for each of its authorized clients. If client
      authorization is disabled, the fields here can be populated with random
      data of the right size (that's 8 bytes for 'client-id', 16 bytes for 'iv'
      and 16 bytes for 'encrypted-cookie' all encoded with base64).

      When client authorization is enabled, each "auth-client" line
      contains the descriptor cookie `N_hs_desc_enc` encrypted to each
      individual client. We assume that each authorized client possesses
      a pre-shared x25519 keypair (`KP_hsc_desc_enc`) which is used to
      decrypt the descriptor cookie.

      We now describe the descriptor cookie encryption scheme. Here is what
      the hidden service computes:

          SECRET_SEED = x25519(KS_hs_desc_ephem, KP_hsc_desc_enc)
          KEYS = KDF(N_hs_subcred | SECRET_SEED, 40)
          CLIENT-ID = fist 8 bytes of KEYS
          COOKIE-KEY = last 32 bytes of KEYS

      Here is a description of the fields in the "auth-client" line:

      - The "client-id" field is CLIENT-ID from above encoded in base64.

      - The "iv" field is 16 random bytes encoded in base64.

      - The "encrypted-cookie" field contains the descriptor cookie ciphertext
        as follows and is encoded in base64:
           encrypted-cookie = STREAM(iv, COOKIE-KEY) XOR N_hs_desc_enc.

      See section [FIRST-LAYER-CLIENT-BEHAVIOR] for the client-side logic of
      how to decrypt the descriptor cookie.

    "encrypted" NL encrypted-string

     [Exactly once]

      An encrypted blob containing the second layer ciphertext, whose format is
      discussed in [HS-DESC-SECOND-LAYER] below. The blob is base64 encoded
      and enclosed in -----BEGIN MESSAGE---- and ----END MESSAGE---- wrappers.

    Compatibility note: The C Tor implementation does not include a final
    newline when generating this first-layer-plaintext section; other
    implementations MUST accept this section even if it is missing its final
    newline.  Other implementations MAY generate this section without a final
    newline themselves, to avoid being distinguishable from C tor.

2.5.1.3. Client behavior [FIRST-LAYER-CLIENT-BEHAVIOR]

    The goal of clients at this stage is to decrypt the "encrypted" field as
    described in [HS-DESC-SECOND-LAYER].

    If client authorization is enabled, authorized clients need to extract the
    descriptor cookie to proceed with decryption of the second layer as
    follows:

    An authorized client parsing the first layer of an encrypted descriptor,
    extracts the ephemeral key from "desc-auth-ephemeral-key" and calculates
    CLIENT-ID and COOKIE-KEY as described in the section above using their
    x25519 private key. The client then uses CLIENT-ID to find the right
    "auth-client" field which contains the ciphertext of the descriptor
    cookie. The client then uses COOKIE-KEY and the iv to decrypt the
    descriptor_cookie, which is used to decrypt the second layer of descriptor
    encryption as described in [HS-DESC-SECOND-LAYER].

2.5.1.4. Hiding client authorization data

    Hidden services should avoid leaking whether client authorization is
    enabled or how many authorized clients there are.

    Hence even when client authorization is disabled, the hidden service adds
    fake "desc-auth-type", "desc-auth-ephemeral-key" and "auth-client" lines to
    the descriptor, as described in [HS-DESC-FIRST-LAYER].

    The hidden service also avoids leaking the number of authorized clients by
    adding fake "auth-client" entries to its descriptor. Specifically,
    descriptors always contain a number of authorized clients that is a
    multiple of 16 by adding fake "auth-client" entries if needed.
    [XXX consider randomization of the value 16]

    Clients MUST accept descriptors with any number of "auth-client" lines as
    long as the total descriptor size is within the max limit of 50k (also
    controlled with a consensus parameter).

2.5.2. Second layer of encryption [HS-DESC-SECOND-LAYER]

   The second layer of descriptor encryption is designed to protect descriptor
   confidentiality against unauthorized clients. If client authorization is
   enabled, it's encrypted using the descriptor_cookie, and contains needed
   information for connecting to the hidden service, like the list of its
   introduction points.

   If client authorization is disabled, then the second layer of HS encryption
   does not offer any additional security, but is still used.

2.5.2.1. Second layer encryption keys

   The encryption keys and format for the second layer of encryption are
   generated as specified in [HS-DESC-ENCRYPTION-KEYS] with customization
   parameters as follows:

     SECRET_DATA = blinded-public-key | descriptor_cookie
     STRING_CONSTANT = "hsdir-encrypted-data"

   If client authorization is disabled the 'descriptor_cookie' field is left blank.

   The ciphertext is placed on the "encrypted" field of the descriptor.

2.5.2.2. Second layer plaintext format

   After decrypting the second layer ciphertext, clients can finally learn the
   list of intro points etc. The plaintext has the following format:

     "create2-formats" SP formats NL

      [Exactly once]

      A space-separated list of integers denoting CREATE2 cell HTYPEs
      (handshake types) that the server recognizes. Must include at least
      ntor as described in tor-spec.txt. See tor-spec section 5.1 for a list
      of recognized handshake types.

     "intro-auth-required" SP types NL

      [At most once]

      A space-separated list of introduction-layer authentication types; see
      section [INTRO-AUTH] for more info. A client that does not support at
      least one of these authentication types will not be able to contact the
      host. Recognized types are: 'ed25519'.

     "single-onion-service"

      [None or at most once]

      If present, this line indicates that the service is a Single Onion
      Service (see prop260 for more details about that type of service). This
      field has been introduced in 0.3.0 meaning 0.2.9 service don't include
      this.

     Followed by zero or more introduction points as follows (see section
     [NUM_INTRO_POINT] below for accepted values):

        "introduction-point" SP link-specifiers NL

          [Exactly once per introduction point at start of introduction
            point section]

          The link-specifiers is a base64 encoding of a link specifier
          block in the format described in [BUILDING-BLOCKS] above.

          As of 0.4.1.1-alpha, services include both IPv4 and IPv6 link
          specifiers in descriptors. All available addresses SHOULD be
          included in the descriptor, regardless of the address that the
          onion service actually used to connect/extend to the intro
          point.

          The client SHOULD NOT reject any LSTYPE fields which it doesn't
          recognize; instead, it should use them verbatim in its EXTEND
          request to the introduction point.

          The client SHOULD perform the basic validity checks on the link
          specifiers in the descriptor, described in `tor-spec.txt`
          section 5.1.2. These checks SHOULD NOT leak
          detailed information about the client's version, configuration,
          or consensus. (See 3.3 for service link specifier handling.)

          When connecting to the introduction point, the client SHOULD send
          this list of link specifiers verbatim, in the same order as given
          here.

          The client MAY reject the list of link specifiers if it is
          inconsistent with relay information from the directory, but SHOULD
          NOT modify it.

        "onion-key" SP "ntor" SP key NL

          [Exactly once per introduction point]

          The key is a base64 encoded curve25519 public key which is the onion
          key of the introduction point Tor node used for the ntor handshake
          when a client extends to it.

        "onion-key" SP KeyType SP key.. NL

          [Any number of times]

          Implementations should accept other types of onion keys using this
          syntax (where "KeyType" is some string other than "ntor");
          unrecognized key types should be ignored.

        "auth-key" NL certificate NL

          [Exactly once per introduction point]

          The certificate is a proposal 220 certificate wrapped in
          "-----BEGIN ED25519 CERT-----".  It contains the introduction
          point authentication key (`KP_hs_ipt_sid`), signed by
          the descriptor signing key (`KP_hs_desc_sign`).  The
          certificate type must be [09], and the signing key extension
          is mandatory.

          NOTE: This certificate was originally intended to be
          constructed the other way around: the signing and signed keys
          are meant to be reversed.  However, C tor implemented it
          backwards, and other implementations now need to do the same
          in order to conform.  (Since this section is inside the
          descriptor, which is _already_ signed by `KP_hs_desc_sign`,
          the verification aspect of this certificate serves no point in
          its current form.)

        "enc-key" SP "ntor" SP key NL

          [Exactly once per introduction point]

          The key is a base64 encoded curve25519 public key used to encrypt
          the introduction request to service. (`KP_hss_ntor`)

        "enc-key" SP KeyType SP key.. NL

          [Any number of times]

          Implementations should accept other types of onion keys using this
          syntax (where "KeyType" is some string other than "ntor");
          unrecognized key types should be ignored.

        "enc-key-cert" NL certificate NL

          [Exactly once per introduction point]

          Cross-certification of the encryption key using the descriptor
          signing key.

          For "ntor" keys, certificate is a proposal 220 certificate
          wrapped in "-----BEGIN ED25519 CERT-----" armor.  The subject
          key is the the ed25519 equivalent of a curve25519 public
          encryption key (`KP_hss_ntor`), with the ed25519 key
          derived using the process in proposal 228 appendix A.  The
          signing key is the descriptor signing key (`KP_hs_desc_sign`).
          The certificate type must be [0B], and the signing-key
          extension is mandatory.

          NOTE: As with "auth-key", this certificate was intended to be
          constructed the other way around.  However, for compatibility
          with C tor, implementations need to construct it this way.  It
          serves even less point than "auth-key", however, since the
          encryption key `KP_hss_ntor` is already available from
          the `enc-key` entry.

        "legacy-key" NL key NL

          [None or at most once per introduction point]
          [This field is obsolete and should never be generated; it
           is included for historical reasons only.]

          The key is an ASN.1 encoded RSA public key in PEM format used for a
          legacy introduction point as described in [LEGACY_EST_INTRO].

          This field is only present if the introduction point only supports
          legacy protocol (v2) that is <= 0.2.9 or the protocol version value
          "HSIntro 3".

        "legacy-key-cert" NL certificate NL

          [None or at most once per introduction point]
          [This field is obsolete and should never be generated; it
           is included for historical reasons only.]

          MUST be present if "legacy-key" is present.

          The certificate is a proposal 220 RSA->Ed cross-certificate wrapped
          in "-----BEGIN CROSSCERT-----" armor, cross-certifying the RSA
          public key found in "legacy-key" using the descriptor signing key.

   To remain compatible with future revisions to the descriptor format,
   clients should ignore unrecognized lines in the descriptor.
   Other encryption and authentication key formats are allowed; clients
   should ignore ones they do not recognize.

   Clients who manage to extract the introduction points of the hidden service
   can proceed with the introduction protocol as specified in [INTRO-PROTOCOL].

   Compatibility note: At least some versions of OnionBalance do not include
   a final newline when generating this inner plaintext section; other
   implementations MUST accept this section even if it is missing its final
   newline.

2.5.3. Deriving hidden service descriptor encryption keys [HS-DESC-ENCRYPTION-KEYS]

   In this section we present the generic encryption format for hidden service
   descriptors. We use the same encryption format in both encryption layers,
   hence we introduce two customization parameters SECRET_DATA and
   STRING_CONSTANT which vary between the layers.

   The SECRET_DATA parameter specifies the secret data that are used during
   encryption key generation, while STRING_CONSTANT is merely a string constant
   that is used as part of the KDF.

   Here is the key generation logic:

       SALT = 16 bytes from H(random), changes each time we rebuild the
              descriptor even if the content of the descriptor hasn't changed.
              (So that we don't leak whether the intro point list etc. changed)

       secret_input = SECRET_DATA | N_hs_subcred | INT_8(revision_counter)

       keys = KDF(secret_input | salt | STRING_CONSTANT, S_KEY_LEN + S_IV_LEN + MAC_KEY_LEN)

       SECRET_KEY = first S_KEY_LEN bytes of keys
       SECRET_IV  = next S_IV_LEN bytes of keys
       MAC_KEY    = last MAC_KEY_LEN bytes of keys

   The encrypted data has the format:

       SALT       hashed random bytes from above  [16 bytes]
       ENCRYPTED  The ciphertext                  [variable]
       MAC        D_MAC of both above fields      [32 bytes]

   The final encryption format is ENCRYPTED = STREAM(SECRET_IV,SECRET_KEY) XOR Plaintext .

   Where D_MAC = H(mac_key_len | MAC_KEY | salt_len | SALT | ENCRYPTED)
   and
    mac_key_len = htonll(len(MAC_KEY))
   and
    salt_len = htonll(len(SALT)).

2.5.4. Number of introduction points [NUM_INTRO_POINT]

   This section defines how many introduction points an hidden service
   descriptor can have at minimum, by default and the maximum:

      Minimum: 0 - Default: 3 - Maximum: 20

   A value of 0 would means that the service is still alive but doesn't want
   to be reached by any client at the moment. Note that the descriptor size
   increases considerably as more introduction points are added.

   The reason for a maximum value of 20 is to give enough scalability to tools
   like OnionBalance to be able to load balance up to 120 servers (20 x 6
   HSDirs) but also in order for the descriptor size to not overwhelmed hidden
   service directories with user defined values that could be gigantic.

3. The introduction protocol [INTRO-PROTOCOL]

   The introduction protocol proceeds in three steps.

   First, a hidden service host builds an anonymous circuit to a Tor
   node and registers that circuit as an introduction point.

   Single Onion Services attempt to build a non-anonymous single-hop circuit,
   but use an anonymous 3-hop circuit if:

     * the intro point is on an address that is configured as unreachable via
       a direct connection, or
     * the initial attempt to connect to the intro point over a single-hop
       circuit fails, and they are retrying the intro point connection.

        [After 'First' and before 'Second', the hidden service publishes its
        introduction points and associated keys, and the client fetches
        them as described in section [HSDIR] above.]

   Second, a client builds an anonymous circuit to the introduction
   point, and sends an introduction request.

   Third, the introduction point relays the introduction request along
   the introduction circuit to the hidden service host, and acknowledges
   the introduction request to the client.

3.1. Registering an introduction point [REG_INTRO_POINT]

3.1.1. Extensible ESTABLISH_INTRO protocol. [EST_INTRO]

   When a hidden service is establishing a new introduction point, it
   sends an ESTABLISH_INTRO cell with the following contents:

     AUTH_KEY_TYPE    [1 byte]
     AUTH_KEY_LEN     [2 bytes]
     AUTH_KEY         [AUTH_KEY_LEN bytes]
     N_EXTENSIONS     [1 byte]
     N_EXTENSIONS times:
        EXT_FIELD_TYPE [1 byte]
        EXT_FIELD_LEN  [1 byte]
        EXT_FIELD      [EXT_FIELD_LEN bytes]
     HANDSHAKE_AUTH   [MAC_LEN bytes]
     SIG_LEN          [2 bytes]
     SIG              [SIG_LEN bytes]

   The AUTH_KEY_TYPE field indicates the type of the introduction point
   authentication key and the type of the MAC to use in
   HANDSHAKE_AUTH. Recognized types are:

       [00, 01] -- Reserved for legacy introduction cells; see
                   [LEGACY_EST_INTRO below]
       [02] -- Ed25519; SHA3-256.

   The AUTH_KEY_LEN field determines the length of the AUTH_KEY
   field. The AUTH_KEY field contains the public introduction point
   authentication key, KP_hs_ipt_sid.

   The EXT_FIELD_TYPE, EXT_FIELD_LEN, EXT_FIELD entries are reserved for
   extensions to the introduction protocol. Extensions with
   unrecognized EXT_FIELD_TYPE values must be ignored.
   (`EXT_FIELD_LEN` may be zero, in which case EXT_FIELD is absent.)

   Unless otherwise specified in the documentation for an extension type:
      * Each extension type SHOULD be sent only once in a message.
      * Parties MUST ignore any occurrences all occurrences of an extension
        with a given type after the first such occurrence.
      * Extensions SHOULD be sent in numerically ascending order by type.
   (The above extension sorting and multiplicity rules are only defaults;
   they may be overridden in the descriptions of individual extensions.)

   The HANDSHAKE_AUTH field contains the MAC of all earlier fields in
   the cell using as its key the shared per-circuit material ("KH")
   generated during the circuit extension protocol; see tor-spec.txt
   section 5.2, "Setting circuit keys". It prevents replays of
   ESTABLISH_INTRO cells.

   SIG_LEN is the length of the signature.

   SIG is a signature, using AUTH_KEY, of all contents of the cell, up
   to but not including SIG_LEN and SIG. These contents are prefixed
   with the string "Tor establish-intro cell v1".

   Upon receiving an ESTABLISH_INTRO cell, a Tor node first decodes the
   key and the signature, and checks the signature. The node must reject
   the ESTABLISH_INTRO cell and destroy the circuit in these cases:

        * If the key type is unrecognized
        * If the key is ill-formatted
        * If the signature is incorrect
        * If the HANDSHAKE_AUTH value is incorrect

        * If the circuit is already a rendezvous circuit.
        * If the circuit is already an introduction circuit.
          [TODO: some scalability designs fail there.]
        * If the key is already in use by another circuit.

   Otherwise, the node must associate the key with the circuit, for use
   later in INTRODUCE1 cells.

3.1.1.1. Denial-of-Service Defense Extension. [EST_INTRO_DOS_EXT]

   This extension can be used to send Denial-of-Service (DoS) parameters to
   the introduction point in order for it to apply them for the introduction
   circuit.

   If used, it needs to be encoded within the N_EXTENSIONS field of the
   ESTABLISH_INTRO cell defined in the previous section. The content is
   defined as follow:

      EXT_FIELD_TYPE:

         [01] -- Denial-of-Service Parameters.

         If this flag is set, the extension should be used by the introduction
         point to learn what values the denial of service subsystem should be
         using.

      EXT_FIELD content format is:

        N_PARAMS       [1 byte]
        N_PARAMS times:
           PARAM_TYPE  [1 byte]
           PARAM_VALUE [8 byte]

        The PARAM_TYPE possible values are:

         [01] -- DOS_INTRODUCE2_RATE_PER_SEC
                 The rate per second of INTRODUCE2 cell relayed to the
                 service.

         [02] -- DOS_INTRODUCE2_BURST_PER_SEC
                 The burst per second of INTRODUCE2 cell relayed to the
                 service.

        The PARAM_VALUE size is 8 bytes in order to accommodate 64bit values.
        It MUST match the specified limit for the following PARAM_TYPE:

         [01] -- Min: 0, Max: 2147483647
         [02] -- Min: 0, Max: 2147483647

        A value of 0 means the defense is disabled. If the rate per second is
        set to 0 (param 0x01) then the burst value should be ignored. And
        vice-versa, if the burst value is 0 (param 0x02), then the rate value
        should be ignored. In other words, setting one single parameter to 0
        disables the defense.

        The burst can NOT be smaller than the rate. If so, the parameters
        should be ignored by the introduction point.

        Any valid value does have precedence over the network wide consensus
        parameter.

   Using this extension extends the payload of the ESTABLISH_INTRO cell by 19
   bytes bringing it from 134 bytes to 155 bytes.

   This extension can only be used with relays supporting the protocol version
   "HSIntro=5".

   Introduced in tor-0.4.2.1-alpha.

3.1.2. Registering an introduction point on a legacy Tor node
       [LEGACY_EST_INTRO]

   [This section is obsolete and refers to a workaround for now-obsolete Tor
    relay versions. It is included for historical reasons.]

   Tor nodes should also support an older version of the ESTABLISH_INTRO
   cell, first documented in rend-spec.txt. New hidden service hosts
   must use this format when establishing introduction points at older
   Tor nodes that do not support the format above in [EST_INTRO].

   In this older protocol, an ESTABLISH_INTRO cell contains:

        KEY_LEN        [2 bytes]
        KEY            [KEY_LEN bytes]
        HANDSHAKE_AUTH [20 bytes]
        SIG            [variable, up to end of relay payload]

   The KEY_LEN variable determines the length of the KEY field.

   The KEY field is the ASN1-encoded legacy RSA public key that was also
   included in the hidden service descriptor.

   The HANDSHAKE_AUTH field contains the SHA1 digest of (KH | "INTRODUCE").

   The SIG field contains an RSA signature, using PKCS1 padding, of all
   earlier fields.

   Older versions of Tor always use a 1024-bit RSA key for these introduction
   authentication keys.

3.1.3. Acknowledging establishment of introduction point [INTRO_ESTABLISHED]

   After setting up an introduction circuit, the introduction point reports its
   status back to the hidden service host with an INTRO_ESTABLISHED cell.

   The INTRO_ESTABLISHED cell has the following contents:

     N_EXTENSIONS [1 byte]
     N_EXTENSIONS times:
       EXT_FIELD_TYPE [1 byte]
       EXT_FIELD_LEN  [1 byte]
       EXT_FIELD      [EXT_FIELD_LEN bytes]

   Older versions of Tor send back an empty INTRO_ESTABLISHED cell instead.
   Services must accept an empty INTRO_ESTABLISHED cell from a legacy relay.
   [The above paragraph is obsolete and refers to a workaround for
   now-obsolete Tor relay versions. It is included for historical reasons.]

   The same rules for multiplicity, ordering, and handling unknown types
   apply to the extension fields here as described [EST_INTRO] above.


3.2. Sending an INTRODUCE1 cell to the introduction point. [SEND_INTRO1]

   In order to participate in the introduction protocol, a client must
   know the following:

     * An introduction point for a service.
     * The introduction authentication key for that introduction point.
     * The introduction encryption key for that introduction point.

   The client sends an INTRODUCE1 cell to the introduction point,
   containing an identifier for the service, an identifier for the
   encryption key that the client intends to use, and an opaque blob to
   be relayed to the hidden service host.

   In reply, the introduction point sends an INTRODUCE_ACK cell back to
   the client, either informing it that its request has been delivered,
   or that its request will not succeed.

   [TODO: specify what tor should do when receiving a malformed cell. Drop it?
          Kill circuit? This goes for all possible cells.]

3.2.1. INTRODUCE1 cell format [FMT_INTRO1]

   When a client is connecting to an introduction point, INTRODUCE1 cells
   should be of the form:

     LEGACY_KEY_ID   [20 bytes]
     AUTH_KEY_TYPE   [1 byte]
     AUTH_KEY_LEN    [2 bytes]
     AUTH_KEY        [AUTH_KEY_LEN bytes]
     N_EXTENSIONS    [1 byte]
     N_EXTENSIONS times:
       EXT_FIELD_TYPE [1 byte]
       EXT_FIELD_LEN  [1 byte]
       EXT_FIELD      [EXT_FIELD_LEN bytes]
     ENCRYPTED        [Up to end of relay payload]

   AUTH_KEY_TYPE is defined as in [EST_INTRO]. Currently, the only value of
   AUTH_KEY_TYPE for this cell is an Ed25519 public key [02].

   The LEGACY_KEY_ID field is used to distinguish between legacy and new style
   INTRODUCE1 cells. In new style INTRODUCE1 cells, LEGACY_KEY_ID is 20 zero
   bytes. Upon receiving an INTRODUCE1 cell, the introduction point checks the
   LEGACY_KEY_ID field. If LEGACY_KEY_ID is non-zero, the INTRODUCE1 cell
   should be handled as a legacy INTRODUCE1 cell by the intro point.

   Upon receiving a INTRODUCE1 cell, the introduction point checks
   whether AUTH_KEY matches the introduction point authentication key for an
   active introduction circuit.  If so, the introduction point sends an
   INTRODUCE2 cell with exactly the same contents to the service, and sends an
   INTRODUCE_ACK response to the client.

   (Note that the introduction point does not "clean up" the
   INTRODUCE1 cells that it retransmits. Specifically, it does not
   change the order or multiplicity of the extensions sent by the
   client.)

   The same rules for multiplicity, ordering, and handling unknown types
   apply to the extension fields here as described [EST_INTRO] above.


3.2.2. INTRODUCE_ACK cell format. [INTRO_ACK]

   An INTRODUCE_ACK cell has the following fields:

     STATUS       [2 bytes]
     N_EXTENSIONS [1 bytes]
     N_EXTENSIONS times:
       EXT_FIELD_TYPE [1 byte]
       EXT_FIELD_LEN  [1 byte]
       EXT_FIELD      [EXT_FIELD_LEN bytes]

   Recognized status values are:

     [00 00] -- Success: cell relayed to hidden service host.
     [00 01] -- Failure: service ID not recognized
     [00 02] -- Bad message format
     [00 03] -- Can't relay cell to service

   The same rules for multiplicity, ordering, and handling unknown types
   apply to the extension fields here as described [EST_INTRO] above.


3.3. Processing an INTRODUCE2 cell at the hidden service. [PROCESS_INTRO2]

   Upon receiving an INTRODUCE2 cell, the hidden service host checks whether
   the AUTH_KEY or LEGACY_KEY_ID field matches the keys for this
   introduction circuit.

   The service host then checks whether it has received a cell with these
   contents or rendezvous cookie before. If it has, it silently drops it as a
   replay. (It must maintain a replay cache for as long as it accepts cells
   with the same encryption key. Note that the encryption format below should
   be non-malleable.)

   If the cell is not a replay, it decrypts the ENCRYPTED field,
   establishes a shared key with the client, and authenticates the whole
   contents of the cell as having been unmodified since they left the
   client. There may be multiple ways of decrypting the ENCRYPTED field,
   depending on the chosen type of the encryption key. Requirements for
   an introduction handshake protocol are described in
   [INTRO-HANDSHAKE-REQS]. We specify one below in section
   [NTOR-WITH-EXTRA-DATA].

   The decrypted plaintext must have the form:

      RENDEZVOUS_COOKIE                          [20 bytes]
      N_EXTENSIONS                               [1 byte]
      N_EXTENSIONS times:
          EXT_FIELD_TYPE                         [1 byte]
          EXT_FIELD_LEN                          [1 byte]
          EXT_FIELD                              [EXT_FIELD_LEN bytes]
      ONION_KEY_TYPE                             [1 bytes]
      ONION_KEY_LEN                              [2 bytes]
      ONION_KEY                                  [ONION_KEY_LEN bytes]
      NSPEC      (Number of link specifiers)     [1 byte]
      NSPEC times:
          LSTYPE (Link specifier type)           [1 byte]
          LSLEN  (Link specifier length)         [1 byte]
          LSPEC  (Link specifier)                [LSLEN bytes]
      PAD        (optional padding)              [up to end of plaintext]

   Upon processing this plaintext, the hidden service makes sure that
   any required authentication is present in the extension fields, and
   then extends a rendezvous circuit to the node described in the LSPEC
   fields, using the ONION_KEY to complete the extension. As mentioned
   in [BUILDING-BLOCKS], the "TLS-over-TCP, IPv4" and "Legacy node
   identity" specifiers must be present.

   As of 0.4.1.1-alpha, clients include both IPv4 and IPv6 link specifiers
   in INTRODUCE1 cells. All available addresses SHOULD be included in the
   cell, regardless of the address that the client actually used to extend
   to the rendezvous point.

   The hidden service should handle invalid or unrecognised link specifiers
   the same way as clients do in section 2.5.2.2. In particular, services
   SHOULD perform basic validity checks on link specifiers, and SHOULD NOT
   reject unrecognised link specifiers, to avoid information leaks.
   The list of link specifiers received here SHOULD either be rejected, or
   sent verbatim when extending to the rendezvous point, in the same order
   received.

   The service MAY reject the list of link specifiers if it is
   inconsistent with relay information from the directory, but SHOULD
   NOT modify it.

   The ONION_KEY_TYPE field is:

      [01] NTOR:          ONION_KEY is 32 bytes long.

   The ONION_KEY field describes the onion key that must be used when
   extending to the rendezvous point. It must be of a type listed as
   supported in the hidden service descriptor.

   The PAD field should be filled with zeros; its size should be chosen
   so that the INTRODUCE2 message occupies a fixed maximum size, in
   order to hide the length of the encrypted data.  (This maximum size is
   490, since we assume that a future Tor implementations will implement
   proposal 340 and thus lower the number of bytes that can be contained
   in a single relay message.)  Note also that current versions of Tor
   only pad the INTRODUCE2 message up to 246 bytes.

   Upon receiving a well-formed INTRODUCE2 cell, the hidden service host
   will have:

     * The information needed to connect to the client's chosen
       rendezvous point.
     * The second half of a handshake to authenticate and establish a
       shared key with the hidden service client.
     * A set of shared keys to use for end-to-end encryption.

   The same rules for multiplicity, ordering, and handling unknown types
   apply to the extension fields here as described [EST_INTRO] above.


3.3.1. Introduction handshake encryption requirements [INTRO-HANDSHAKE-REQS]

   When decoding the encrypted information in an INTRODUCE2 cell, a
   hidden service host must be able to:

     * Decrypt additional information included in the INTRODUCE2 cell,
       to include the rendezvous token and the information needed to
       extend to the rendezvous point.

     * Establish a set of shared keys for use with the client.

     * Authenticate that the cell has not been modified since the client
       generated it.

   Note that the old TAP-derived protocol of the previous hidden service
   design achieved the first two requirements, but not the third.

3.3.2. Example encryption handshake: ntor with extra data
       [NTOR-WITH-EXTRA-DATA]

   [TODO: relocate this]

   This is a variant of the ntor handshake (see tor-spec.txt, section
   5.1.4; see proposal 216; and see "Anonymity and one-way
   authentication in key-exchange protocols" by Goldberg, Stebila, and
   Ustaoglu).

   It behaves the same as the ntor handshake, except that, in addition
   to negotiating forward secure keys, it also provides a means for
   encrypting non-forward-secure data to the server (in this case, to
   the hidden service host) as part of the handshake.

   Notation here is as in section 5.1.4 of tor-spec.txt, which defines
   the ntor handshake.

   The PROTOID for this variant is "tor-hs-ntor-curve25519-sha3-256-1".
   We also use the following tweak values:

      t_hsenc    = PROTOID | ":hs_key_extract"
      t_hsverify = PROTOID | ":hs_verify"
      t_hsmac    = PROTOID | ":hs_mac"
      m_hsexpand = PROTOID | ":hs_key_expand"

   To make an INTRODUCE1 cell, the client must know a public encryption
   key B for the hidden service on this introduction circuit. The client
   generates a single-use keypair:

             x,X = KEYGEN()

   and computes:

             intro_secret_hs_input = EXP(B,x) | AUTH_KEY | X | B | PROTOID
             info = m_hsexpand | N_hs_subcred
             hs_keys = KDF(intro_secret_hs_input | t_hsenc | info, S_KEY_LEN+MAC_LEN)
             ENC_KEY = hs_keys[0:S_KEY_LEN]
             MAC_KEY = hs_keys[S_KEY_LEN:S_KEY_LEN+MAC_KEY_LEN]

   and sends, as the ENCRYPTED part of the INTRODUCE1 cell:

          CLIENT_PK                [PK_PUBKEY_LEN bytes]
          ENCRYPTED_DATA           [Padded to length of plaintext]
          MAC                      [MAC_LEN bytes]


   Substituting those fields into the INTRODUCE1 cell body format
   described in [FMT_INTRO1] above, we have

            LEGACY_KEY_ID               [20 bytes]
            AUTH_KEY_TYPE               [1 byte]
            AUTH_KEY_LEN                [2 bytes]
            AUTH_KEY                    [AUTH_KEY_LEN bytes]
            N_EXTENSIONS                [1 bytes]
            N_EXTENSIONS times:
               EXT_FIELD_TYPE           [1 byte]
               EXT_FIELD_LEN            [1 byte]
               EXT_FIELD                [EXT_FIELD_LEN bytes]
            ENCRYPTED:
               CLIENT_PK                [PK_PUBKEY_LEN bytes]
               ENCRYPTED_DATA           [Padded to length of plaintext]
               MAC                      [MAC_LEN bytes]


   (This format is as documented in [FMT_INTRO1] above, except that here
   we describe how to build the ENCRYPTED portion.)

   Here, the encryption key plays the role of B in the regular ntor
   handshake, and the AUTH_KEY field plays the role of the node ID.
   The CLIENT_PK field is the public key X. The ENCRYPTED_DATA field is
   the message plaintext, encrypted with the symmetric key ENC_KEY. The
   MAC field is a MAC of all of the cell from the AUTH_KEY through the
   end of ENCRYPTED_DATA, using the MAC_KEY value as its key.

   To process this format, the hidden service checks PK_VALID(CLIENT_PK)
   as necessary, and then computes ENC_KEY and MAC_KEY as the client did
   above, except using EXP(CLIENT_PK,b) in the calculation of
   intro_secret_hs_input. The service host then checks whether the MAC is
   correct. If it is invalid, it drops the cell. Otherwise, it computes
   the plaintext by decrypting ENCRYPTED_DATA.

   The hidden service host now completes the service side of the
   extended ntor handshake, as described in tor-spec.txt section 5.1.4,
   with the modified PROTOID as given above. To be explicit, the hidden
   service host generates a keypair of y,Y = KEYGEN(), and uses its
   introduction point encryption key 'b' to compute:

      intro_secret_hs_input = EXP(X,b) | AUTH_KEY | X | B | PROTOID
      info = m_hsexpand | N_hs_subcred
      hs_keys = KDF(intro_secret_hs_input | t_hsenc | info, S_KEY_LEN+MAC_LEN)
      HS_DEC_KEY = hs_keys[0:S_KEY_LEN]
      HS_MAC_KEY = hs_keys[S_KEY_LEN:S_KEY_LEN+MAC_KEY_LEN]

      (The above are used to check the MAC and then decrypt the
      encrypted data.)

      rend_secret_hs_input = EXP(X,y) | EXP(X,b) | AUTH_KEY | B | X | Y | PROTOID
      NTOR_KEY_SEED = MAC(rend_secret_hs_input, t_hsenc)
      verify = MAC(rend_secret_hs_input, t_hsverify)
      auth_input = verify | AUTH_KEY | B | Y | X | PROTOID | "Server"
      AUTH_INPUT_MAC = MAC(auth_input, t_hsmac)

      (The above are used to finish the ntor handshake.)

   The server's handshake reply is:

       SERVER_PK   Y                         [PK_PUBKEY_LEN bytes]
       AUTH        AUTH_INPUT_MAC            [MAC_LEN bytes]

   These fields will be sent to the client in a RENDEZVOUS1 cell using the
   HANDSHAKE_INFO element (see [JOIN_REND]).

   The hidden service host now also knows the keys generated by the
   handshake, which it will use to encrypt and authenticate data
   end-to-end between the client and the server. These keys are as
   computed in tor-spec.txt section 5.1.4, except that instead of using
   AES-128 and SHA1 for this hop, we use AES-256 and SHA3-256.

3.4. Authentication during the introduction phase. [INTRO-AUTH]

   Hidden services may restrict access only to authorized users.
   One mechanism to do so is the credential mechanism, where only users who
   know the credential for a hidden service may connect at all.

   There is one defined authentication type: `ed25519`.


3.4.1. Ed25519-based authentication `ed25519`.

   (NOTE: This section is not implemented by Tor.  It is likely
   that we would want to change its design substantially before
   deploying any implementation.  At the very least, we would
   want to bind these extensions to a single onion service, to
   prevent replays. We might also want to look for ways to limit
   the number of keys a user needs to have.)

   To authenticate with an Ed25519 private key, the user must include an
   extension field in the encrypted part of the INTRODUCE1 cell with an
   EXT_FIELD_TYPE type of [02] and the contents:

        Nonce     [16 bytes]
        Pubkey    [32 bytes]
        Signature [64 bytes]

   Nonce is a random value. Pubkey is the public key that will be used
   to authenticate. [TODO: should this be an identifier for the public
   key instead?]  Signature is the signature, using Ed25519, of:

        "hidserv-userauth-ed25519"
        Nonce       (same as above)
        Pubkey      (same as above)
        AUTH_KEY    (As in the INTRODUCE1 cell)

   The hidden service host checks this by seeing whether it recognizes
   and would accept a signature from the provided public key. If it
   would, then it checks whether the signature is correct. If it is,
   then the correct user has authenticated.

   Replay prevention on the whole cell is sufficient to prevent replays
   on the authentication.

   Users SHOULD NOT use the same public key with multiple hidden
   services.

4. The rendezvous protocol

   Before connecting to a hidden service, the client first builds a
   circuit to an arbitrarily chosen Tor node (known as the rendezvous
   point), and sends an ESTABLISH_RENDEZVOUS cell. The hidden service
   later connects to the same node and sends a RENDEZVOUS cell. Once
   this has occurred, the relay forwards the contents of the RENDEZVOUS
   cell to the client, and joins the two circuits together.

   Single Onion Services attempt to build a non-anonymous single-hop circuit,
   but use an anonymous 3-hop circuit if:

     * the rend point is on an address that is configured as unreachable via
       a direct connection, or
     * the initial attempt to connect to the rend point over a single-hop
       circuit fails, and they are retrying the rend point connection.

4.1. Establishing a rendezvous point [EST_REND_POINT]

   The client sends the rendezvous point a RELAY_COMMAND_ESTABLISH_RENDEZVOUS
   cell containing a 20-byte value.

            RENDEZVOUS_COOKIE         [20 bytes]

   Rendezvous points MUST ignore any extra bytes in an
   ESTABLISH_RENDEZVOUS cell. (Older versions of Tor did not.)

   The rendezvous cookie is an arbitrary 20-byte value, chosen randomly
   by the client. The client SHOULD choose a new rendezvous cookie for
   each new connection attempt. If the rendezvous cookie is already in
   use on an existing circuit, the rendezvous point should reject it and
   destroy the circuit.

   Upon receiving an ESTABLISH_RENDEZVOUS cell, the rendezvous point associates
   the cookie with the circuit on which it was sent. It replies to the client
   with an empty RENDEZVOUS_ESTABLISHED cell to indicate success. Clients MUST
   ignore any extra bytes in a RENDEZVOUS_ESTABLISHED cell.

   The client MUST NOT use the circuit which sent the cell for any
   purpose other than rendezvous with the given location-hidden service.

   The client should establish a rendezvous point BEFORE trying to
   connect to a hidden service.

4.2. Joining to a rendezvous point [JOIN_REND]

   To complete a rendezvous, the hidden service host builds a circuit to
   the rendezvous point and sends a RENDEZVOUS1 cell containing:

       RENDEZVOUS_COOKIE          [20 bytes]
       HANDSHAKE_INFO             [variable; depends on handshake type
                                   used.]

   where RENDEZVOUS_COOKIE is the cookie suggested by the client during the
   introduction (see [PROCESS_INTRO2]) and HANDSHAKE_INFO is defined in
   [NTOR-WITH-EXTRA-DATA].

   If the cookie matches the rendezvous cookie set on any
   not-yet-connected circuit on the rendezvous point, the rendezvous
   point connects the two circuits, and sends a RENDEZVOUS2 cell to the
   client containing the HANDSHAKE_INFO field of the RENDEZVOUS1 cell.

   Upon receiving the RENDEZVOUS2 cell, the client verifies that HANDSHAKE_INFO
   correctly completes a handshake. To do so, the client parses SERVER_PK from
   HANDSHAKE_INFO and reverses the final operations of section
   [NTOR-WITH-EXTRA-DATA] as shown here:

      rend_secret_hs_input = EXP(Y,x) | EXP(B,x) | AUTH_KEY | B | X | Y | PROTOID
      NTOR_KEY_SEED = MAC(ntor_secret_input, t_hsenc)
      verify = MAC(ntor_secret_input, t_hsverify)
      auth_input = verify | AUTH_KEY | B | Y | X | PROTOID | "Server"
      AUTH_INPUT_MAC = MAC(auth_input, t_hsmac)

   Finally the client verifies that the received AUTH field of HANDSHAKE_INFO
   is equal to the computed AUTH_INPUT_MAC.

   Now both parties use the handshake output to derive shared keys for use on
   the circuit as specified in the section below:

4.2.1. Key expansion

   The hidden service and its client need to derive crypto keys from the
   NTOR_KEY_SEED part of the handshake output. To do so, they use the KDF
   construction as follows:

       K = KDF(NTOR_KEY_SEED | m_hsexpand,    HASH_LEN * 2 + S_KEY_LEN * 2)

   The first HASH_LEN bytes of K form the forward digest Df; the next HASH_LEN
   bytes form the backward digest Db; the next S_KEY_LEN bytes form Kf, and the
   final S_KEY_LEN bytes form Kb.  Excess bytes from K are discarded.

   Subsequently, the rendezvous point passes relay cells, unchanged, from each
   of the two circuits to the other.  When Alice's OP sends RELAY cells along
   the circuit, it authenticates with Df, and encrypts them with the Kf, then
   with all of the keys for the ORs in Alice's side of the circuit; and when
   Alice's OP receives RELAY cells from the circuit, it decrypts them with the
   keys for the ORs in Alice's side of the circuit, then decrypts them with Kb,
   and checks integrity with Db.  Bob's OP does the same, with Kf and Kb
   interchanged.

   [TODO: Should we encrypt HANDSHAKE_INFO as we did INTRODUCE2
   contents? It's not necessary, but it could be wise. Similarly, we
   should make it extensible.]

4.3. Using legacy hosts as rendezvous points

   [This section is obsolete and refers to a workaround for now-obsolete Tor
   relay versions. It is included for historical reasons.]

   The behavior of ESTABLISH_RENDEZVOUS is unchanged from older versions
   of this protocol, except that relays should now ignore unexpected
   bytes at the end.

   Old versions of Tor required that RENDEZVOUS cell payloads be exactly
   168 bytes long. All shorter rendezvous payloads should be padded to
   this length with random bytes, to make them difficult to distinguish from
   older protocols at the rendezvous point.

   Relays older than 0.2.9.1 should not be used for rendezvous points by next
   generation onion services because they enforce too-strict length checks to
   rendezvous cells. Hence the "HSRend" protocol from proposal#264 should be
   used to select relays for rendezvous points.

5. Encrypting data between client and host

   A successfully completed handshake, as embedded in the
   INTRODUCE/RENDEZVOUS cells, gives the client and hidden service host
   a shared set of keys Kf, Kb, Df, Db, which they use for sending
   end-to-end traffic encryption and authentication as in the regular
   Tor relay encryption protocol, applying encryption with these keys
   before other encryption, and decrypting with these keys before other
   decryption. The client encrypts with Kf and decrypts with Kb; the
   service host does the opposite.

6. Encoding onion addresses [ONIONADDRESS]

   The onion address of a hidden service includes its identity public key, a
   version field and a basic checksum. All this information is then base32
   encoded as shown below:

     onion_address = base32(PUBKEY | CHECKSUM | VERSION) + ".onion"
     CHECKSUM = H(".onion checksum" | PUBKEY | VERSION)[:2]

     where:
       - PUBKEY is the 32 bytes ed25519 master pubkey of the hidden service.
       - VERSION is a one byte version field (default value '\x03')
       - ".onion checksum" is a constant string
       - CHECKSUM is truncated to two bytes before inserting it in onion_address

  Here are a few example addresses:

       pg6mmjiyjmcrsslvykfwnntlaru7p5svn6y2ymmju6nubxndf4pscryd.onion
       sp3k262uwy4r2k3ycr5awluarykdpag6a7y33jxop4cs2lu5uz5sseqd.onion
       xa4r2iadxm55fbnqgwwi5mymqdcofiu3w6rpbtqn7b2dyn7mgwj64jyd.onion

   For more information about this encoding, please see our discussion thread
   at [ONIONADDRESS-REFS].

7. Open Questions:

   Scaling hidden services is hard. There are on-going discussions that
   you might be able to help with. See [SCALING-REFS].

   How can we improve the HSDir unpredictability design proposed in
   [SHAREDRANDOM]? See [SHAREDRANDOM-REFS] for discussion.

   How can hidden service addresses become memorable while retaining
   their self-authenticating and decentralized nature? See
   [HUMANE-HSADDRESSES-REFS] for some proposals; many more are possible.

   Hidden Services are pretty slow. Both because of the lengthy setup
   procedure and because the final circuit has 6 hops. How can we make
   the Hidden Service protocol faster? See [PERFORMANCE-REFS] for some
   suggestions.

References:

[KEYBLIND-REFS]:
        https://trac.torproject.org/projects/tor/ticket/8106
        https://lists.torproject.org/pipermail/tor-dev/2012-September/004026.html

[KEYBLIND-PROOF]:
        https://lists.torproject.org/pipermail/tor-dev/2013-December/005943.html

[SHAREDRANDOM-REFS]:
        https://gitweb.torproject.org/torspec.git/tree/proposals/250-commit-reveal-consensus.txt
        https://trac.torproject.org/projects/tor/ticket/8244

[SCALING-REFS]:
        https://lists.torproject.org/pipermail/tor-dev/2013-October/005556.html

[HUMANE-HSADDRESSES-REFS]:
        https://gitweb.torproject.org/torspec.git/blob/HEAD:/proposals/ideas/xxx-onion-nyms.txt
        http://archives.seul.org/or/dev/Dec-2011/msg00034.html

[PERFORMANCE-REFS]:
        "Improving Efficiency and Simplicity of Tor circuit
        establishment and hidden services" by Overlier, L., and
        P. Syverson

        [TODO: Need more here! Do we have any? :( ]

[ATTACK-REFS]:
        "Trawling for Tor Hidden Services: Detection, Measurement,
        Deanonymization" by Alex Biryukov, Ivan Pustogarov,
        Ralf-Philipp Weinmann

        "Locating Hidden Servers" by Lasse Øverlier and Paul
        Syverson

[ED25519-REFS]:
        "High-speed high-security signatures" by Daniel
        J. Bernstein, Niels Duif, Tanja Lange, Peter Schwabe, and
        Bo-Yin Yang. http://cr.yp.to/papers.html#ed25519

[ED25519-B-REF]:
        https://tools.ietf.org/html/draft-josefsson-eddsa-ed25519-03#section-5:

[PRNG-REFS]:
        http://projectbullrun.org/dual-ec/ext-rand.html
        https://lists.torproject.org/pipermail/tor-dev/2015-November/009954.html

[SRV-TP-REFS]:
        https://lists.torproject.org/pipermail/tor-dev/2016-April/010759.html

[VANITY-REFS]:
        https://github.com/Yawning/horse25519

[ONIONADDRESS-REFS]:
        https://lists.torproject.org/pipermail/tor-dev/2017-January/011816.html

[TORSION-REFS]:
        https://lists.torproject.org/pipermail/tor-dev/2017-April/012164.html
        https://getmonero.org/2017/05/17/disclosure-of-a-major-bug-in-cryptonote-based-currencies.html

Appendix A. Signature scheme with key blinding [KEYBLIND]

A.1. Key derivation overview

  As described in [IMD:DIST] and [SUBCRED] above, we require a "key
  blinding" system that works (roughly) as follows:

        There is a master keypair (sk, pk).

        Given the keypair and a nonce n, there is a derivation function
        that gives a new blinded keypair (sk_n, pk_n).  This keypair can
        be used for signing.

        Given only the public key and the nonce, there is a function
        that gives pk_n.

        Without knowing pk, it is not possible to derive pk_n; without
        knowing sk, it is not possible to derive sk_n.

        It's possible to check that a signature was made with sk_n while
        knowing only pk_n.

        Someone who sees a large number of blinded public keys and
        signatures made using those public keys can't tell which
        signatures and which blinded keys were derived from the same
        master keypair.

        You can't forge signatures.

        [TODO: Insert a more rigorous definition and better references.]

A.2. Tor's key derivation scheme

  We propose the following scheme for key blinding, based on Ed25519.

  (This is an ECC group, so remember that scalar multiplication is the
  trapdoor function, and it's defined in terms of iterated point
  addition. See the Ed25519 paper [Reference ED25519-REFS] for a fairly
  clear writeup.)

  Let B be the ed25519 basepoint as found in section 5 of [ED25519-B-REF]:

      B = (15112221349535400772501151409588531511454012693041857206046113283949847762202,
           46316835694926478169428394003475163141307993866256225615783033603165251855960)

  Assume B has prime order l, so lB=0. Let a master keypair be written as
  (a,A), where a is the private key and A is the public key (A=aB).

  To derive the key for a nonce N and an optional secret s, compute the
  blinding factor like this:

           h = H(BLIND_STRING | A | s | B | N)
           BLIND_STRING = "Derive temporary signing key" | INT_1(0)
           N = "key-blind" | INT_8(period-number) | INT_8(period_length)
           B = "(1511[...]2202, 4631[...]5960)"

  then clamp the blinding factor 'h' according to the ed25519 spec:

           h[0] &= 248;
           h[31] &= 63;
           h[31] |= 64;

  and do the key derivation as follows:

      private key for the period:

           a' = h a mod l
           RH' = SHA-512(RH_BLIND_STRING | RH)[:32]
           RH_BLIND_STRING = "Derive temporary signing key hash input"

      public key for the period:

           A' = h A = (ha)B

  Generating a signature of M: given a deterministic random-looking r
  (see EdDSA paper), take R=rB, S=r+hash(R,A',M)ah mod l. Send signature
  (R,S) and public key A'.

  Verifying the signature: Check whether SB = R+hash(R,A',M)A'.

  (If the signature is valid,
       SB = (r + hash(R,A',M)ah)B
          = rB + (hash(R,A',M)ah)B
          = R + hash(R,A',M)A' )

  This boils down to regular Ed25519 with key pair (a', A').

  See [KEYBLIND-REFS] for an extensive discussion on this scheme and
  possible alternatives. Also, see [KEYBLIND-PROOF] for a security
  proof of this scheme.

Appendix B. Selecting nodes [PICKNODES]

  Picking introduction points
  Picking rendezvous points
  Building paths
  Reusing circuits

  (TODO: This needs a writeup)

Appendix C. Recommendations for searching for vanity .onions [VANITY]

  EDITORIAL NOTE: The author thinks that it's silly to brute-force the
  keyspace for a key that, when base-32 encoded, spells out the name of
  your website. It also feels a bit dangerous to me. If you train your
  users to connect to

      llamanymityx4fi3l6x2gyzmtmgxjyqyorj9qsb5r543izcwymle.onion

  I worry that you're making it easier for somebody to trick them into
  connecting to

      llamanymityb4sqi0ta0tsw6uovyhwlezkcrmczeuzdvfauuemle.onion

  Nevertheless, people are probably going to try to do this, so here's a
  decent algorithm to use.

  To search for a public key with some criterion X:

        Generate a random (sk,pk) pair.

        While pk does not satisfy X:

            Add the number 8 to sk
            Add the point 8*B to pk

        Return sk, pk.

  We add 8 and 8*B, rather than 1 and B, so that sk is always a valid
  Curve25519 private key, with the lowest 3 bits equal to 0.

  This algorithm is safe [source: djb, personal communication] [TODO:
  Make sure I understood correctly!] so long as only the final (sk,pk)
  pair is used, and all previous values are discarded.

  To parallelize this algorithm, start with an independent (sk,pk) pair
  generated for each independent thread, and let each search proceed
  independently.

  See [VANITY-REFS] for a reference implementation of this vanity .onion
  search scheme.

Appendix D. Numeric values reserved in this document

  [TODO: collect all the lists of commands and values mentioned above]

Appendix E. Reserved numbers

  We reserve these certificate type values for Ed25519 certificates:

      [08] short-term descriptor signing key, signed with blinded
           public key. (Section 2.4)
      [09] intro point authentication key, cross-certifying the descriptor
           signing key. (Section 2.5)
      [0B] ed25519 key derived from the curve25519 intro point encryption key,
           cross-certifying the descriptor signing key. (Section 2.5)

      Note: The value "0A" is skipped because it's reserved for the onion key
            cross-certifying ntor identity key from proposal 228.

Appendix F. Hidden service directory format [HIDSERVDIR-FORMAT]

  This appendix section specifies the contents of the HiddenServiceDir directory:

  - "hostname"                                       [FILE]

   This file contains the onion address of the onion service.

  - "private_key_ed25519"                            [FILE]

   This file contains the private master ed25519 key of the onion service.
   [TODO: Offline keys]

  - "./authorized_clients/"                  [DIRECTORY]
    "./authorized_clients/alice.auth"        [FILE]
    "./authorized_clients/bob.auth"          [FILE]
    "./authorized_clients/charlie.auth"      [FILE]

   If client authorization is enabled, this directory MUST contain a ".auth"
   file for each authorized client. Each such file contains the public key of
   the respective client. The files are transmitted to the service operator by
   the client.

   See section [CLIENT-AUTH-MGMT] for more details and the format of the client file.

   (NOTE: client authorization is implemented as of 0.3.5.1-alpha.)

Appendix G. Managing authorized client data [CLIENT-AUTH-MGMT]

  Hidden services and clients can configure their authorized client data either
  using the torrc, or using the control port. This section presents a suggested
  scheme for configuring client authorization. Please see appendix
  [HIDSERVDIR-FORMAT] for more information about relevant hidden service files.

  (NOTE: client authorization is implemented as of 0.3.5.1-alpha.)

  G.1. Configuring client authorization using torrc

  G.1.1. Hidden Service side configuration

     A hidden service that wants to enable client authorization, needs to
     populate the "authorized_clients/" directory of its HiddenServiceDir
     directory with the ".auth" files of its authorized clients.

     When Tor starts up with a configured onion service, Tor checks its
     <HiddenServiceDir>/authorized_clients/ directory for ".auth" files, and if
     any recognized and parseable such files are found, then client
     authorization becomes activated for that service.

  G.1.2. Service-side bookkeeping

     This section contains more details on how onion services should be keeping
     track of their client ".auth" files.

     For the "descriptor" authentication type, the ".auth" file MUST contain
     the x25519 public key of that client. Here is a suggested file format:

        <auth-type>:<key-type>:<base32-encoded-public-key>

     Here is an an example:

        descriptor:x25519:OM7TGIVRYMY6PFX6GAC6ATRTA5U6WW6U7A4ZNHQDI6OVL52XVV2Q

     Tor SHOULD ignore lines it does not recognize.
     Tor SHOULD ignore files that don't use the ".auth" suffix.

  G.1.3. Client side configuration

     A client who wants to register client authorization data for onion
     services needs to add the following line to their torrc to indicate the
     directory which hosts ".auth_private" files containing client-side
     credentials for onion services:

         ClientOnionAuthDir <DIR>

     The <DIR> contains a file with the suffix ".auth_private" for each onion
     service the client is authorized with. Tor should scan the directory for
     ".auth_private" files to find which onion services require client
     authorization from this client.

     For the "descriptor" auth-type, a ".auth_private" file contains the
     private x25519 key:

        <onion-address>:descriptor:x25519:<base32-encoded-privkey>

     The keypair used for client authorization is created by a third party tool
     for which the public key needs to be transferred to the service operator
     in a secure out-of-band way. The third party tool SHOULD add appropriate
     headers to the private key file to ensure that users won't accidentally
     give out their private key.

  G.2. Configuring client authorization using the control port

  G.2.1. Service side

     A hidden service also has the option to configure authorized clients
     using the control port. The idea is that hidden service operators can use
     controller utilities that manage their access control instead of using
     the filesystem to register client keys.

     Specifically, we require a new control port command ADD_ONION_CLIENT_AUTH
     which is able to register x25519/ed25519 public keys tied to a specific
     authorized client.
      [XXX figure out control port command format]

     Hidden services who use the control port interface for client auth need
     to perform their own key management.

  G.2.2. Client side

     There should also be a control port interface for clients to register
     authorization data for hidden services without having to use the
     torrc. It should allow both generation of client authorization private
     keys, and also to import client authorization data provided by a hidden
     service

     This way, Tor Browser can present "Generate client auth keys" and "Import
     client auth keys" dialogs to users when they try to visit a hidden service
     that is protected by client authorization.

     Specifically, we require two new control port commands:
                   IMPORT_ONION_CLIENT_AUTH_DATA
                   GENERATE_ONION_CLIENT_AUTH_DATA
     which import and generate client authorization data respectively.

     [XXX how does key management work here?]
     [XXX what happens when people use both the control port interface and the
          filesystem interface?]

Appendix F. Two methods for managing revision counters.

  Implementations MAY generate revision counters in any way they please,
  so long as they are monotonically increasing over the lifetime of each
  blinded public key.  But to avoid fingerprinting, implementors SHOULD
  choose a strategy also used by other Tor implementations. Here we
  describe two, and additionally list some strategies that implementors
  should NOT use.

  F.1. Increment-on-generation

    This is the simplest strategy, and the one used by Tor through at
    least version 0.3.4.0-alpha.

    Whenever using a new blinded key, the service records the
    highest revision counter it has used with that key.  When generating
    a descriptor, the service uses the smallest non-negative number
    higher than any number it has already used.

    In other words, the revision counters under this system start fresh
    with each blinded key as 0, 1, 2, 3, and so on.

  F.2. Encrypted time in period

    This scheme is what we recommend for situations when multiple
    service instances need to coordinate their revision counters,
    without an actual coordination mechanism.

    Let T be the number of seconds that have elapsed since the descriptor
    became valid, plus 1.  (T must be at least 1.) Implementations can use the
    number of seconds since the start time of the shared random protocol run
    that corresponds to this descriptor.

    Let S be a secret that all the service providers share.  For
    example, it could be the private signing key corresponding to the
    current blinded key.

    Let K be an AES-256 key, generated as
        K = H("rev-counter-generation" | S)

    Use K, and AES in counter mode with IV=0, to generate a stream of T
    * 2 bytes.  Consider these bytes as a sequence of T 16-bit
    little-endian words.  Add these words.

    Let the sum of these words be the revision counter.


    Cryptowiki attributes roughly this scheme to G. Bebek in:

         G. Bebek. Anti-tamper database research: Inference control
         techniques. Technical Report EECS 433 Final Report, Case
         Western Reserve University, November 2002.

    Although we believe it is suitable for use in this application, it
    is not a perfect order-preserving encryption algorithm (and all
    order-preserving encryption has weaknesses).  Please think twice
    before using it for anything else.

    (This scheme can be optimized pretty easily by caching the encryption of
    X*1, X*2, X*3, etc for some well chosen X.)

    For a slow reference implementation, see src/test/ope_ref.py in the
    Tor source repository. [XXXX for now, see the same file in Nick's
    "ope_hax" branch -- it isn't merged yet.]

    This scheme is not currently implemented in Tor.

  F.X. Some revision-counter strategies to avoid

    Though it might be tempting, implementations SHOULD NOT use the
    current time or the current time within the period directly as their
    revision counter -- doing so leaks their view of the current time,
    which can be used to link the onion service to other services run on
    the same host.

    Similarly, implementations SHOULD NOT let the revision counter
    increase forever without resetting it -- doing so links the service
    across changes in the blinded public key.

Appendix G. Text vectors

  G.1. Test vectors for hs-ntor / NTOR-WITH-EXTRA-DATA

    Here is a set of test values for the hs-ntor handshake, called
    [NTOR-WITH-EXTRA-DATA] in this document.  They were generated by
    instrumenting Tor's code to dump the values for an INTRODUCE/RENDEZVOUS
    handshake, and then by running that code on a Chutney network.

    We assume an onion service with:

      KP_hs_ipd_sid = 34E171E4358E501BFF21ED907E96AC6B
                      FEF697C779D040BBAF49ACC30FC5D21F
      KP_hss_ntor   = 8E5127A40E83AABF6493E41F142B6EE3
                      604B85A3961CD7E38D247239AFF71979
      KS_hss_ntor   = A0ED5DBF94EEB2EDB3B514E4CF6ABFF6
                      022051CC5F103391F1970A3FCD15296A
      N_hs_subcred  = 0085D26A9DEBA252263BF0231AEAC59B
                      17CA11BAD8A218238AD6487CBAD68B57

    The client wants to make in INTRODUCE request.  It generates
    the following header (everything before the ENCRYPTED portion)
    of its INTRODUCE1 cell:

      H = 000000000000000000000000000000000000000002002034E171E4358E501BFF
          21ED907E96AC6BFEF697C779D040BBAF49ACC30FC5D21F00

    It generates the following plaintext body to encrypt.  (This
    is the "decrypted plaintext body" from [PROCESS_INTRO2].

      P = 6BD364C12638DD5C3BE23D76ACA05B04E6CE932C0101000100200DE6130E4FCA
          C4EDDA24E21220CC3EADAE403EF6B7D11C8273AC71908DE565450300067F0000
          0113890214F823C4F8CC085C792E0AEE0283FE00AD7520B37D0320728D5DF39B
          7B7077A0118A900FF4456C382F0041300ACF9C58E51C392795EF870000000000
          0000000000000000000000000000000000000000000000000000000000000000
          000000000000000000000000000000000000000000000000000000000000

      (Note! This should in fact be padded to be longer; when these
      test vectors were generated, the target INTRODUCE1 length in C
      Tor was needlessly short.)

    The client now begins the hs-ntor handshake.  It generates
    a curve25519 keypair:

      x = 60B4D6BF5234DCF87A4E9D7487BDF3F4
          A69B6729835E825CA29089CFDDA1E341
      X = BF04348B46D09AED726F1D66C618FDEA
          1DE58E8CB8B89738D7356A0C59111D5D

    Then it calculates:

      ENC_KEY = 9B8917BA3D05F3130DACCE5300C3DC27
                F6D012912F1C733036F822D0ED238706
      MAC_KEY = FC4058DA59D4DF61E7B40985D122F502
                FD59336BC21C30CAF5E7F0D4A2C38FD5

    With these, it encrypts the plaintext body P with ENC_KEY, getting
    an encrypted value C.  It computes MAC(MAC_KEY, H | X | C),
    getting a MAC value M.  It then assembles the final INTRODUCE1
    body as H | X | C | M:

      000000000000000000000000000000000000000002002034E171E4358E501BFF
      21ED907E96AC6BFEF697C779D040BBAF49ACC30FC5D21F00BF04348B46D09AED
      726F1D66C618FDEA1DE58E8CB8B89738D7356A0C59111D5DADBECCCB38E37830
      4DCC179D3D9E437B452AF5702CED2CCFEC085BC02C4C175FA446525C1B9D5530
      563C362FDFFB802DAB8CD9EBC7A5EE17DA62E37DEEB0EB187FBB48C63298B0E8
      3F391B7566F42ADC97C46BA7588278273A44CE96BC68FFDAE31EF5F0913B9A9C
      7E0F173DBC0BDDCD4ACB4C4600980A7DDD9EAEC6E7F3FA3FC37CD95E5B8BFB3E
      35717012B78B4930569F895CB349A07538E42309C993223AEA77EF8AEA64F25D
      DEE97DA623F1AEC0A47F150002150455845C385E5606E41A9A199E7111D54EF2
      D1A51B7554D8B3692D85AC587FB9E69DF990EFB776D8

   Later the service receives that body in an INTRODUCE2 cell.  It
   processes it according to the hs-ntor handshake, and recovers
   the client's plaintext P.  To continue the hs-ntor handshake,
   the service chooses a curve25519 keypair:

      y = 68CB5188CA0CD7924250404FAB54EE13
          92D3D2B9C049A2E446513875952F8F55
      Y = 8FBE0DB4D4A9C7FF46701E3E0EE7FD05
          CD28BE4F302460ADDEEC9E93354EE700

   From this and the client's input, it computes:

      AUTH_INPUT_MAC = 4A92E8437B8424D5E5EC279245D5C72B
                       25A0327ACF6DAF902079FCB643D8B208
      NTOR_KEY_SEED  = 4D0C72FE8AFF35559D95ECC18EB5A368
                       83402B28CDFD48C8A530A5A3D7D578DB

   The service sends back Y | AUTH_INPUT_MAC in its RENDEZVOUS1 cell
   body.  From these, the client finishes the handshake, validates
   AUTH_INPUT_MAC, and computes the same NTOR_KEY_SEED.

   Now that both parties have the same NTOR_KEY_SEED, they can derive
   the shared key material they will use for their circuit.
