  o Minor features (IPv6, relay):
    - Allow clients and relays to send dual-stack and IPv6-only EXTEND2 cells.
      Parse dual-stack and IPv6-only EXTEND2 cells on relays.
      Closes ticket 33901.
